<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<library>
<description>EE-440 library</description>
<packages>
<package name="DIL16">
</package>
<package name="TSSOP14">
</package>
<package name="DIX-10X2-.05">
</package>
<package name="DC-POWERJACK">
</package>
<package name="SFM2X10">
</package>
<package name="TO220(V)">
<description>&lt;b&gt;TO-220&lt;/b&gt;&lt;p&gt;
grid 2,54mm, vertikal</description>
</package>
<package name="TO92">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
<package name="TO220H">
<description>&lt;b&gt;TO-220&lt;/b&gt;</description>
</package>
<package name="TO39">
<description>&lt;b&gt;Metal Can Package&lt;/b&gt;</description>
</package>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
<package name="PLCC-44">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square, package type L</description>
</package>
<package name="MQFP44-2">
<description>&lt;b&gt;Plastic Metric Quad Flat Pack&lt;/b&gt;&lt;p&gt;
package type PQ</description>
</package>
<package name="TQFP44">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;&lt;p&gt;
package type TQ</description>
</package>
<package name="DIL40">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
<package name="JP2W">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="2X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="SO-08M">
<description>&lt;B&gt;Small Outline Medium Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
207-mil body, package type SM</description>
</package>
<package name="TSSOP8">
<description>&lt;b&gt;Thin Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type ST</description>
</package>
<package name="SO-08">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SN</description>
</package>
<package name="PBSWITCH">
</package>
<package name="DT6">
<description>&lt;b&gt;ITT SWITCH&lt;/b&gt;</description>
</package>
<package name="DTE6">
<description>&lt;b&gt;ITT SWITCH&lt;/b&gt;</description>
</package>
<package name="DTE6K">
<description>&lt;b&gt;ITT SWITCH&lt;/b&gt;</description>
</package>
<package name="DO41Z10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SOCKED-20">
<description>&lt;b&gt;Dual In Line Socked&lt;/b&gt;</description>
</package>
<package name="2X12">
</package>
<package name="SQFP-S-6X6-48">
<description>&lt;b&gt;QFP48&lt;/b&gt;&lt;p&gt;
shrink quad flat pack, square</description>
</package>
<package name="SQFP-S-7X7-48">
<description>&lt;b&gt;QFP48&lt;/b&gt;&lt;p&gt;
shrink quad flat pack, square</description>
</package>
<package name="F09HP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="SM-MMS-110-01">
</package>
<package name="XBEE-MOD">
</package>
<package name="TSSOP16">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 16&lt;/b&gt;&lt;p&gt;
http://www.maxim-ic.com .. MAX3223-MAX3243.pdf</description>
</package>
<package name="SO16L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; .300 SIOC&lt;p&gt;
Source: http://www.maxim-ic.com/cgi-bin/packages?pkg=16%2FSOIC%2E300&amp;Type=Max</description>
</package>
<package name="SOIC-.3-28">
</package>
<package name="DIL28-3">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.3 inch</description>
</package>
<package name="SOT23-5L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="2X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="DIL24-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
<package name="LEDDISP">
</package>
<package name="DIL24-3">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.3 inch</description>
</package>
<package name="SO24W">
<description>&lt;b&gt;Wide Small Outline package&lt;/b&gt; 300 mil</description>
</package>
<package name="MODULAR-6">
<description>&lt;b&gt;Modular Jack&lt;/b&gt;&lt;p&gt;without Panel Stops</description>
</package>
<package name="TO18">
<description>&lt;b&gt;TO 18&lt;/b&gt;</description>
</package>
<package name="TO92-CBE">
<description>&lt;b&gt;TO-92&lt;/b&gt; Pads In Line</description>
</package>
<package name="1X02N">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03N">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04N">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X05N">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X10N">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06N">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X09N">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="SIL8">
<description>&lt;b&gt;Single In Line&lt;/b&gt;</description>
</package>
<package name="SIL10">
<description>&lt;b&gt;Single In Line&lt;/b&gt;</description>
</package>
<package name="1X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="LEDDISPLRGPKG">
</package>
<package name="E-320">
</package>
<package name="SOIC-ADAPT">
<description>&lt;B&gt;Small Outline Wide Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
300-mil body, package type SO</description>
</package>
<package name="1X14">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="TO220BV">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
<package name="4POL254">
<description>&lt;b&gt;PHOENIX CONNECTOR&lt;/b&gt;</description>
</package>
<package name="SAPDELUG">
</package>
<package name="MW-MICROFIT-6">
</package>
<package name="SO08">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AA</description>
</package>
<package name="MW-MICROFIT-8">
</package>
<package name="LINX-LC-S-RX">
</package>
<package name="LINX-LC-S-TX">
</package>
<package name="MOLEX-34045-RA-8">
</package>
<package name="SO16">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AC</description>
</package>
<package name="ACS755">
</package>
<package name="QFN40">
</package>
<package name="RABNC">
</package>
<package name="MOLEX-34045-RA-10">
</package>
<package name="MOLEX-34045-RA-4">
</package>
<package name="MOLEX-34045-10">
</package>
<package name="MOLEX-34045-8">
</package>
<package name="MOLEX-34045-4">
</package>
<package name="ACS755-RH">
</package>
<package name="HAIS200">
</package>
<package name="BIGLUG">
</package>
<package name="9VBATHOLDER">
<description>Keystone 9v battery holder</description>
</package>
<package name="3TERMINALSTRIP">
</package>
<package name="FUSESOCKET">
</package>
<package name="12MMBATSM">
</package>
<package name="SPDT-SMT">
</package>
<package name="LQFP32">
<description>&lt;b&gt;LQFP-32 package&lt;/b&gt;&lt;p&gt;
7x7 mm case, 0.8 mm lead pitch</description>
</package>
<package name="CSTCR-RESONATOR">
</package>
<package name="SOT89">
<description>&lt;b&gt;Small Outline Transistor; 3 leads&lt;/b&gt; Reflow soldering&lt;p&gt;
INFINEON, www.infineon.com/cmc_upload/0/000/010/257/eh_db_5b.pdf</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="DIL8">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
<package name="32QN1">
</package>
<package name="TQFP-80-12X12MM">
</package>
<package name="CSTCE-10M0G">
</package>
<package name="TQFP80-12X12">
<description>&lt;b&gt;TQFP80&lt;/b&gt; 12x12x1 mm Body&lt;p&gt;
Source: http://www.microchip.com/ .. 39663c.pdf</description>
</package>
<package name="TQFP64-10X10">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;&lt;p&gt;
package type TQ</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor 223&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 318E-04&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM137M-D.PDF</description>
</package>
<package name="SOP28">
<description>&lt;b&gt;SMALL OUTLINE PACKAGE&lt;/b&gt;</description>
</package>
<package name="SSOP28">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt; SSOP-28&lt;p&gt;
http://www.ftdichip.com/Documents/DataSheets/DS_FT232R_v104.pdf</description>
</package>
<package name="QFN32">
<description>&lt;b&gt;QFN 32&lt;/b&gt;&lt;p&gt;
Source: http://www.ftdichip.com/Documents/DataSheets/DS_FT232R_v104.pdf</description>
</package>
<package name="TQFP64-10X10RMS">
</package>
<package name="2X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X12">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA07-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="USB-B-H">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-MB-S">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-S">
<description>&lt;b&gt;USB Series A Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-MB-H">
<description>&lt;b&gt;USB Series Mini-B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-HU">
<description>&lt;b&gt;USB Series A Hole Mounted Up-Right&lt;/b&gt;</description>
</package>
<package name="USB-B-SMT">
<description>USB Series B Surface Mounted</description>
</package>
<package name="USB-BV2">
</package>
<package name="2X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="DPAK">
</package>
<package name="TQFP64-10X10RMSSTOP">
</package>
<package name="CSTCE-20M0V">
</package>
<package name="MLF32">
<description>&lt;b&gt;32M1-A&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="XTAL4025">
</package>
<package name="32QN1R1">
</package>
<package name="SMT-POT-TC73">
</package>
<package name="PT-10">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="PT-10S">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="PT-SPIN">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="B25P">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 25</description>
</package>
<package name="B25U">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 25</description>
</package>
<package name="B25V">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 25</description>
</package>
<package name="B25X">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 25</description>
</package>
<package name="B64W">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 64</description>
</package>
<package name="B64Y">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 64</description>
</package>
<package name="SP19L">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="CA6H">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
<package name="CA6V">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
<package name="CA9H">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
<package name="CA9V">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
<package name="CA14V">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
<package name="CA14H">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
<package name="CT6">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Copal</description>
</package>
<package name="ECP10P">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="ECP10S">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="LI10">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Piher</description>
</package>
<package name="LI15">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Piher</description>
</package>
<package name="RJ6">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Copal</description>
</package>
<package name="RJ6S">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Copal</description>
</package>
<package name="RJ9W">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Copal</description>
</package>
<package name="RS3">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Copal</description>
</package>
<package name="S63P">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Spectrol</description>
</package>
<package name="S63S">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Spectrol</description>
</package>
<package name="S63X">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Spectrol</description>
</package>
<package name="S64W">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Spectrol</description>
</package>
<package name="S64Y">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Spectrol</description>
</package>
<package name="S75H">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="S75P">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="ST10">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Piher</description>
</package>
<package name="ST15">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Piher</description>
</package>
<package name="SP19LKN">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="TSSOP-3-28-L">
</package>
<package name="MSOP8">
<description>&lt;b&gt;Micro Small Outline Package&lt;/b&gt;</description>
</package>
<package name="2X09">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="JOY-252">
</package>
<package name="JOY-252-SW">
</package>
<package name="JOY-253">
</package>
<package name="JOY-253-SW">
</package>
<package name="HDR-2MM-2X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2MM"</description>
</package>
<package name="2TERMINALSTRIP">
</package>
<package name="TERMBLOCK-5.08-4">
</package>
<package name="TERMBLOCK-10.0-4">
</package>
<package name="LCD-MULTI">
</package>
<package name="R0805RMS">
</package>
<package name="2X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="D2PACK">
<description>&lt;b&gt;D2PACK&lt;/b&gt;&lt;p&gt;
INTERNATIONAL RECTIFIER, irg4bc15ud-s.pdf</description>
</package>
<package name="D2PAK(TO-263)">
</package>
<package name="DO13M">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 6.35 mm metall, horizontal, grid 20.32 mm</description>
</package>
<package name="DO15-12">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 3.5 mm, horizontal, grid 12.7 mm</description>
</package>
<package name="SMB">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
<package name="SMC">
<description>&lt;b&gt;DIODE&lt;/b&gt;</description>
</package>
<package name="SMA">
</package>
<package name="BALUN-0805">
</package>
<package name="MOLEX-MINIFIT-RA-1-5">
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="DF11-TH">
</package>
<package name="DF-11-SM-16">
</package>
<package name="SOT363_PHILIPS">
<description>&lt;b&gt;Small Outline Transistor; 6 leads&lt;/b&gt;&lt;p&gt;
Philips Semiconductors, SOT363.pdf</description>
</package>
<package name="DIL28-6">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
<package name="IDC-NL-ASSMAN-NL">
</package>
<package name="FFC-1MMTHRA">
</package>
<package name="AMP2X2-.1IN">
</package>
<package name="AMP2X3-.1IN">
</package>
<package name="AMP2X5-.1IN">
</package>
<package name="ICD-FL">
</package>
<package name="AMP2X4-.1IN">
</package>
<package name="POT-VADJ">
</package>
<package name="PB-TYCO">
</package>
<package name="QFN44ML8X8">
<description>&lt;b&gt;44-Lead Plastic Quad Flat No Lead Package (ML)&lt;/b&gt; 8x8 mm Body (QFN)&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf</description>
</package>
<package name="QFN44ML8X8-2">
</package>
<package name="1X16">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="SOD323-W">
<description>&lt;b&gt;SOD323 Wave soldering&lt;/b&gt; Philips SC01_Mounting_1996.pdf</description>
</package>
<package name="1X04L">
</package>
<package name="FFC-8-1MM">
</package>
<package name="1V60R">
<description>&lt;b&gt;NC ACCU&lt;/b&gt; Varta</description>
</package>
<package name="SW-SPDT-2MM">
</package>
<package name="A68-A31">
<description>&lt;b&gt;SLIDING SWITCH&lt;/b&gt;&lt;p&gt;
Siemens, distributor Buerklin, 11G766</description>
</package>
<package name="ZIG-DAUGHTER">
</package>
<package name="AMP2X3-.1IN-RA">
</package>
<package name="AMP2X4-.1IN-RA">
</package>
<package name="AMP2X5-.1IN-RA">
</package>
<package name="SCREW-TERM-3">
</package>
<package name="TYCO-5.08MM-3">
</package>
<package name="SOD123">
<description>&lt;b&gt;SOD123</description>
</package>
<package name="LGA5X3">
</package>
<package name="TSSOP20">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 20&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
<package name="TYCO-5.08MM-2">
</package>
<package name="SCREW-TERM-1X4">
<description>1x4 screw terminal</description>
</package>
<package name="PHOE-5MM-4">
</package>
<package name="TYCO-5.08MM-4">
</package>
<package name="PHOE-5MM-5">
</package>
<package name="TYCO-5.08MM-5">
</package>
<package name="TYCO-3.5MM-3">
</package>
<package name="TYCO-3.5MM-4">
</package>
<package name="TYCO-3.81MM-4">
</package>
<package name="TYCO-5.00MM-4">
</package>
<package name="TYCO-5.00MM-5">
</package>
<package name="IDC-10-RA">
</package>
<package name="IDC-10">
</package>
<package name="PROGRAMMER">
</package>
<package name="TYCO-3.5MM-5">
</package>
<package name="TYCO-3.81MM-5">
</package>
<package name="TYCO-3.81MM-3">
</package>
<package name="TYCO-3.81MM-2">
</package>
<package name="EG1218">
<description>&lt;b&gt;SLIDING SWITCH&lt;/b&gt;&lt;p&gt;
E-switch EG1218 
DIgikey: EG1903</description>
</package>
<package name="ZIG-DAUGHTER-SMALL">
</package>
<package name="ABM3B-XTAL">
</package>
<package name="BU-SMA-V">
<description>FEMALE &lt;b&gt;SMA CONNECTOR&lt;/b&gt;&lt;p&gt;
Radiall&lt;p&gt;
distributor RS 112-3794</description>
</package>
<package name="EG2301">
<description>DP3T slide
E switch 2301A
D: EG1944</description>
</package>
<package name="EG2201">
<description>DPDT slide
E-switch 2201
D:EG1905</description>
</package>
<package name="IDC-24">
</package>
<package name="EG2208">
</package>
<package name="EG2308">
<description>DP3T RA
EG2308
D:EG1945</description>
</package>
<package name="SPST-RA">
<description>RA SPST switch
D:EG1836</description>
</package>
<package name="QFN28-ML_6X6MM">
<description>&lt;b&gt;QFN28-ML_6X6MM&lt;/b&gt;&lt;p&gt;
Source: http://www.microchip.com .. 39637a.pdf</description>
</package>
<package name="QFN6X6-.55">
<description>QFN 6x6mm
.55 contact length</description>
</package>
<package name="SO28W">
<description>&lt;B&gt;28-Lead Plastic Small Outline (SO) &lt;/B&gt; Wide, 300 mil Body (SOIC)&lt;/B&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf</description>
</package>
<package name="EG2209">
<description>Slide DPDT
EG2209
D:EG1908/08</description>
</package>
<package name="TP">
</package>
<package name="LED10">
</package>
<package name="EG2201-2">
</package>
<package name="UMAX-10">
</package>
<package name="GBJ">
</package>
<package name="GBU4S">
<description>&lt;b&gt;GENERAL INSTRUMENT RECTIFIER&lt;/b&gt;</description>
</package>
<package name="OMRONSPDT">
</package>
<package name="RT2C/O">
<description>&lt;b&gt;Power PCB Relay DC and AC-coil&lt;/b&gt; SCHRACK&lt;p&gt;
2 pole 8 A&lt;br&gt;
Source: http://www.schrack.com/.. 5842.pdf</description>
</package>
<package name="RT-C/O12A3.5">
<description>&lt;b&gt;Power PCB Relay 1 pole 12 / 16 A, DC- or AC-coil&lt;/b&gt; SCHRACK&lt;p&gt;
12A, pinning 3.5 mm&lt;br&gt;
Source: http://www.schrack.com/.. 5819.pdf</description>
</package>
<package name="LCD-NEW-0216">
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="1206">
<description>&lt;b&gt;CHICAGO MINIATURE LAMP, INC.&lt;/b&gt;&lt;p&gt;
7022X Series SMT LEDs 1206 Package Size</description>
</package>
<package name="LD260">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, square, Siemens</description>
</package>
<package name="LED2X5">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
2 x 5 mm, rectangle</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="LSU260">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
1 mm, round, Siemens</description>
</package>
<package name="LZR181">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
1 LED, Siemens</description>
</package>
<package name="Q62902-B152">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="Q62902-B153">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="Q62902-B155">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="Q62902-B156">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="SFH480">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
infrared emitting diode, Infineon
TO-18, lead spacing 2.54 mm, cathode marking&lt;p&gt;
Inifineon</description>
</package>
<package name="SFH482">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
infrared emitting diode, Infineon
TO-18, lead spacing 2.54 mm, cathode marking&lt;p&gt;
Inifineon</description>
</package>
<package name="U57X32">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
rectangle, 5.7 x 3.2 mm</description>
</package>
<package name="IRL80A">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
IR transmitter Siemens</description>
</package>
<package name="P-LCC-2">
<description>&lt;b&gt;TOPLED® High-optical Power LED (HOP)&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... ls_t675.pdf</description>
</package>
<package name="OSRAM-MINI-TOP-LED">
<description>&lt;b&gt;BLUE LINETM Hyper Mini TOPLED® Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LB M676.pdf</description>
</package>
<package name="OSRAM-SIDELED">
<description>&lt;b&gt;Super SIDELED® High-Current LED&lt;/b&gt;&lt;p&gt;
LG A672, LP A672 &lt;br&gt;
Source: http://www.osram.convergy.de/ ... LG_LP_A672.pdf (2004.05.13)</description>
</package>
<package name="SMART-LED">
<description>&lt;b&gt;SmartLEDTM Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY L896.pdf</description>
</package>
<package name="P-LCC-2-TOPLED-RG">
<description>&lt;b&gt;Hyper TOPLED® RG Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY T776.pdf</description>
</package>
<package name="MICRO-SIDELED">
<description>&lt;b&gt;Hyper Micro SIDELED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY Y876.pdf</description>
</package>
<package name="P-LCC-4">
<description>&lt;b&gt;Power TOPLED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LA_LY E67B.pdf</description>
</package>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
<package name="MINI-TOPLED-SANTANA">
<description>&lt;b&gt;Mini TOPLED Santana®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG M470.pdf</description>
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
<package name="CHIPLED-0603-TTW">
<description>&lt;b&gt;CHIPLED-0603&lt;/b&gt;&lt;p&gt;
Recommended Solder Pad useable for SmartLEDTM and Chipled - Package 0603&lt;br&gt;
Package able to withstand TTW-soldering heat&lt;br&gt;
Package suitable for TTW-soldering&lt;br&gt;
Source: http://www.osram.convergy.de/ ... LO_LS_LY L89K.pdf</description>
</package>
<package name="SMARTLED-TTW">
<description>&lt;b&gt;SmartLED TTW&lt;/b&gt;&lt;p&gt;
Recommended Solder Pad useable for SmartLEDTM and Chipled - Package 0603&lt;br&gt;
Package able to withstand TTW-soldering heat&lt;br&gt;
Package suitable for TTW-soldering&lt;br&gt;
Source: http://www.osram.convergy.de/ ... LO_LS_LY L89K.pdf</description>
</package>
<package name="LUMILED+">
<description>&lt;b&gt;Lumileds Lighting. LUXEON®&lt;/b&gt; with cool pad&lt;p&gt;
Source: K2.pdf</description>
</package>
<package name="LUMILED">
<description>&lt;b&gt;Lumileds Lighting. LUXEON®&lt;/b&gt; without cool pad&lt;p&gt;
Source: K2.pdf</description>
</package>
<package name="QFN44ML8X8-2G">
</package>
<package name="ACPOWER">
</package>
<package name="1X01">
</package>
<package name="DIN-6">
</package>
<package name="POWER-16GAUGE">
</package>
<package name="PHONO-JACK-RA">
</package>
<package name="TQFP44C">
</package>
<package name="LED-RGB">
</package>
<package name="SD-5638">
</package>
<package name="LED-RGB2">
</package>
<package name="TSSOP28">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;, 5 lead</description>
</package>
<package name="CUR_SENS_TAMURA">
</package>
<package name="SSOP20">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
<package name="ANT-315-SCREW">
</package>
<package name="TYCO-5.00MM-6">
</package>
<package name="TYCO-5.00MM-3">
</package>
<package name="LED2-0606">
</package>
<package name="INV300X">
</package>
<package name="MOLEX-4301">
</package>
<package name="TYCO-5.00MM-2">
</package>
<package name="MOLEX-4302">
</package>
<package name="MOLEX-4303">
</package>
<package name="LUS-0805">
</package>
<package name="DIODE-SMA">
</package>
<package name="MOLEX-4304">
</package>
<package name="CUR-SEN-LEM">
</package>
<package name="8-SMD">
</package>
<package name="DC-IN-1.3MM">
</package>
<package name="TYCO-5.00MM-12R">
</package>
<package name="TYCO-5.00MM-12L">
</package>
<package name="IDC-10-RA-M">
</package>
<package name="IDC-10-RA-F">
</package>
<package name="SCREW-TERM-.325-2">
</package>
<package name="MOLEX-4202">
</package>
<package name="MOLEX-4200">
</package>
<package name="SOT-223">
</package>
<package name="MOLEX-4306">
</package>
<package name="WM-4204">
</package>
<package name="MOLEX-4201">
</package>
<package name="MOLEX-4204">
</package>
<package name="MOLEX-4300">
</package>
<package name="MOLEX-4203">
</package>
<package name="MOLEX-4206">
</package>
<package name="MPU-60X0">
</package>
<package name="LCC8">
</package>
<package name="LGA14">
<description>Land Grid Array (LGA-14)</description>
</package>
<package name="ADMP405">
</package>
<package name="MEDIATEK3329">
</package>
<package name="CON-CGRIDIII-5X2-RA">
</package>
<package name="CON-CGRIDIII-4X2-V">
<description>&lt;b&gt;C-Grid III&lt;/b&gt;&lt;p&gt;
vertical, dual row</description>
</package>
<package name="CON-CGRIDIII-5X2-V">
<description>&lt;b&gt;C-Grid III&lt;/b&gt;&lt;p&gt;
vertical, dual row</description>
</package>
<package name="CON-CGRIDIII-4X2-RA">
</package>
<package name="USC-MICRO-FCI">
</package>
<package name="MOLEX-47364-0001">
</package>
<package name="S108T01">
</package>
<package name="ACS714">
</package>
<package name="SSOP16">
</package>
<package name="PICKIT3">
</package>
</packages>
<symbols>
<symbol name="MAX3323">
<pin name="TXEN" direction="in"/>
<pin name="TIN" direction="in"/>
<pin name="ROUT" direction="out"/>
<pin name="C1+" direction="in"/>
<pin name="C1-" direction="in"/>
<pin name="V+" direction="in"/>
<pin name="RXEN" direction="in"/>
<pin name="TOUT" direction="out"/>
<pin name="RIN" direction="in"/>
<pin name="C2+" direction="in"/>
<pin name="C2-" direction="in"/>
<pin name="V-" direction="in"/>
<pin name="VL" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="SHDN" direction="in"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="DIL-10X2-.05">
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
<pin name="P$3" direction="pas"/>
<pin name="P$4" direction="pas"/>
<pin name="P$5" direction="pas"/>
<pin name="P$6" direction="pas"/>
<pin name="P$7" direction="pas"/>
<pin name="P$8" direction="pas"/>
<pin name="P$9" direction="pas"/>
<pin name="P$10" direction="pas"/>
<pin name="P$11" direction="pas"/>
<pin name="P$12" direction="pas"/>
<pin name="P$13" direction="pas"/>
<pin name="P$14" direction="pas"/>
<pin name="P$15" direction="pas"/>
<pin name="P$16" direction="pas"/>
<pin name="P$17" direction="pas"/>
<pin name="P$18" direction="pas"/>
<pin name="P$19" direction="pas"/>
<pin name="P$20" direction="pas"/>
</symbol>
<symbol name="MAX3378">
<pin name="VC1"/>
<pin name="VC2"/>
<pin name="VC3"/>
<pin name="VC4"/>
<pin name="GND" direction="pwr"/>
<pin name="/TRI" direction="in"/>
<pin name="VL4"/>
<pin name="VL3"/>
<pin name="VL2"/>
<pin name="VL1"/>
<pin name="VDD" direction="pwr"/>
<pin name="V3.3" direction="pwr"/>
</symbol>
<symbol name="DC-POWERJACK">
<pin name="+V" direction="sup"/>
<pin name="P$2" direction="pwr"/>
<pin name="P$3" direction="pwr"/>
</symbol>
<symbol name="LM2937-3.3">
<pin name="IN" direction="in"/>
<pin name="VOUT" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="78XX">
<pin name="VI" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V5.0" direction="sup"/>
</symbol>
<symbol name="18F4620">
<pin name="MCLR#" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4/T0CKI"/>
<pin name="RA5/AN4"/>
<pin name="RE0/AN5"/>
<pin name="RE1/AN6"/>
<pin name="RE2/AN7"/>
<pin name="RA7/OX1"/>
<pin name="RA6/OX2"/>
<pin name="RC0"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3/SCK"/>
<pin name="RD0"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RC4/MISO"/>
<pin name="RC5/MOSI"/>
<pin name="RC6/TX"/>
<pin name="RC7/RX"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3/PGM"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6/PGC"/>
<pin name="RB7/PGD"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
</symbol>
<symbol name="PIC17F874">
<pin name="MCLR#/THV" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4/T0CKI"/>
<pin name="RA5/AN4"/>
<pin name="RE0/RD#/AN5"/>
<pin name="RE1/WR#/AN6"/>
<pin name="RE2/CS#/AN7"/>
<pin name="OSC1/CLKIN" direction="in"/>
<pin name="OSC2/CLKOUT" direction="out"/>
<pin name="RC0/T1OSO"/>
<pin name="RC1/T1OSI"/>
<pin name="RC2/CCP1"/>
<pin name="RC3/SCK"/>
<pin name="RD0/PSP0"/>
<pin name="RD1/PSP1"/>
<pin name="RD2/PSP2"/>
<pin name="RD3/PSP3"/>
<pin name="SDI/RC4"/>
<pin name="SDO/RC5"/>
<pin name="TX/RC6"/>
<pin name="RX/RC7"/>
<pin name="PSP4/RD4"/>
<pin name="PSP5/RD5"/>
<pin name="PSP6/RD6"/>
<pin name="PSP7/RD7"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="INT/RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="PGM/RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="PGC/RB6"/>
<pin name="PGD/RB7"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
</symbol>
<symbol name="JP3E">
<pin name="1" direction="pas"/>
<pin name="VDD" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="PINH2X10">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
</symbol>
<symbol name="TC-1265">
<pin name="VI" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V3.3" direction="sup"/>
</symbol>
<symbol name="+3V3">
<pin name="+3V3" direction="sup"/>
</symbol>
<symbol name="TS2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="P1" direction="pas"/>
</symbol>
<symbol name="+05V">
<pin name="V5.0" direction="sup"/>
</symbol>
<symbol name="24AA32">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="25SERIAL">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="!CS" direction="in"/>
<pin name="SO"/>
<pin name="!HOLD" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="SI" direction="in"/>
<pin name="!WP" direction="in"/>
</symbol>
<symbol name="24FC515">
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="24FC512">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="WP" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
</symbol>
<symbol name="25LC640">
<pin name="CS/"/>
<pin name="SO"/>
<pin name="WP/"/>
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="HD/"/>
<pin name="SCLK"/>
<pin name="SI"/>
</symbol>
<symbol name="DS1337">
<pin name="X1"/>
<pin name="X2"/>
<pin name="INTA" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="INTB" direction="out"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="LM1086CT-5">
<pin name="VI" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V5.0" direction="sup"/>
</symbol>
<symbol name="LM2937-5.0">
<pin name="IN" direction="in"/>
<pin name="VOUT" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="TS2-1">
<pin name="S" direction="pas"/>
<pin name="P" direction="pas"/>
<pin name="P@1" direction="pas"/>
<pin name="S@1" direction="pas"/>
</symbol>
<symbol name="ZD">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="LED10">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
</symbol>
<symbol name="DIL20">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="PINH2X12">
<pin name="1" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
</symbol>
<symbol name="CC2420">
<pin name="VCO_GRD"/>
<pin name="AV_VCO"/>
<pin name="AV_PRE"/>
<pin name="AV_RF1"/>
<pin name="GND@1"/>
<pin name="RF_P"/>
<pin name="TXRX_SW"/>
<pin name="RF_N"/>
<pin name="GND@2"/>
<pin name="AV_SW"/>
<pin name="P$11" direction="nc"/>
<pin name="P$12" direction="nc"/>
<pin name="P$13" direction="nc"/>
<pin name="AV_RF2"/>
<pin name="AV_IF2"/>
<pin name="P$16" direction="nc"/>
<pin name="AV_ADC"/>
<pin name="DV_ADC"/>
<pin name="DGND_GRD"/>
<pin name="DGUARD"/>
<pin name="RESETN"/>
<pin name="DGND"/>
<pin name="DSUB_P"/>
<pin name="DSUB_C"/>
<pin name="DV3.3"/>
<pin name="DV1.8"/>
<pin name="SFD"/>
<pin name="CCA"/>
<pin name="FIFOP"/>
<pin name="FIFO"/>
<pin name="CSN"/>
<pin name="SCLK"/>
<pin name="SI"/>
<pin name="SO"/>
<pin name="DV_RAM"/>
<pin name="P$36" direction="nc"/>
<pin name="AV_X16"/>
<pin name="XOSCQ2"/>
<pin name="XOSC_Q1"/>
<pin name="P$40" direction="nc"/>
<pin name="VREG_EN"/>
<pin name="VREG_OUT"/>
<pin name="VREG_IN"/>
<pin name="AVDD_IF1"/>
<pin name="R_BIAS"/>
<pin name="ATEST2"/>
<pin name="ATEST1"/>
<pin name="AV_CHP"/>
</symbol>
<symbol name="TEST8">
<pin name="VDD" direction="pwr"/>
<pin name="SIG1"/>
<pin name="SIG2"/>
<pin name="SIG3"/>
<pin name="VSS" direction="pwr"/>
<pin name="SIG4"/>
<pin name="SIG5"/>
<pin name="SIG6"/>
</symbol>
<symbol name="F09G">
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="G1" direction="pas"/>
<pin name="G2" direction="pas"/>
</symbol>
<symbol name="ZIG-MOD">
<pin name="V3.3" direction="pwr"/>
<pin name="DOUT" direction="out"/>
<pin name="DIN" direction="in"/>
<pin name="D08" direction="out"/>
<pin name="RSET" direction="in"/>
<pin name="RSSI" direction="out"/>
<pin name="P$7" direction="nc"/>
<pin name="P$8" direction="nc"/>
<pin name="DTR/" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="D04"/>
<pin name="CTS/"/>
<pin name="ON" direction="out"/>
<pin name="VREF"/>
<pin name="DIO5"/>
<pin name="RTS/"/>
<pin name="DIO3"/>
<pin name="DIO2"/>
<pin name="DIO1"/>
<pin name="DIO0"/>
</symbol>
<symbol name="MAX311X">
<pin name="R2IN" direction="in"/>
<pin name="R20UT" direction="out"/>
<pin name="T2IN" direction="in"/>
<pin name="T1IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="T1OUT" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="X2"/>
<pin name="X1"/>
<pin name="CTS/" direction="in"/>
<pin name="RTS/" direction="out"/>
<pin name="RX" direction="in"/>
<pin name="TX" direction="out"/>
<pin name="DIN" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="SCLK" direction="in"/>
<pin name="CS/" direction="in"/>
<pin name="IRQ/" direction="out"/>
<pin name="SHDN/" direction="in"/>
<pin name="V+"/>
<pin name="C1+"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="V-"/>
<pin name="GND" direction="pwr"/>
<pin name="T2OUT" direction="out"/>
</symbol>
<symbol name="DC-DC-CONV">
<pin name="VIN" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VOUT" direction="pwr"/>
<pin name="C+" direction="in"/>
<pin name="C-" direction="in"/>
</symbol>
<symbol name="PINH2X5">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
</symbol>
<symbol name="LEDDSP">
<pin name="A"/>
<pin name="F"/>
<pin name="CC1"/>
<pin name="E"/>
<pin name="CC2"/>
<pin name="LDP"/>
<pin name="RDP"/>
<pin name="D"/>
<pin name="CC3"/>
<pin name="C"/>
<pin name="G"/>
<pin name="B"/>
<pin name="CC4"/>
</symbol>
<symbol name="MAX7221">
<pin name="DIN" direction="in"/>
<pin name="DIG0" direction="in"/>
<pin name="DIG4" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="DIG6" direction="in"/>
<pin name="DIG2" direction="in"/>
<pin name="DIG3" direction="in"/>
<pin name="DIG7" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="DIG5" direction="in"/>
<pin name="DIG1" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="SEGA" direction="out"/>
<pin name="SEGF" direction="out"/>
<pin name="SEGB" direction="out"/>
<pin name="SEGG" direction="out"/>
<pin name="ISET"/>
<pin name="VDD" direction="pwr"/>
<pin name="SEGC" direction="out"/>
<pin name="SEGE" direction="out"/>
<pin name="SEGDP" direction="out"/>
<pin name="SEGD" direction="out"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="JACK6">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="NPN">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="PINHD2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD4">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD5">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD10">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD9">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
</symbol>
<symbol name="RNV">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="R9">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="PINHD8">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X4">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
</symbol>
<symbol name="LEDDISPLRG">
<pin name="CC1"/>
<pin name="E"/>
<pin name="D"/>
<pin name="C"/>
<pin name="DP"/>
<pin name="B"/>
<pin name="A"/>
<pin name="CC2"/>
<pin name="F"/>
<pin name="G"/>
</symbol>
<symbol name="D-TS">
</symbol>
<symbol name="E320PBSWITCH">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="ADAPTER-28">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25"/>
<pin name="P$26"/>
<pin name="P$27"/>
<pin name="P$28"/>
</symbol>
<symbol name="PINHD14">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
</symbol>
<symbol name="HBRIDGE">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
</symbol>
<symbol name="BRIDGE-DRIVER3940">
<pin name="VDR"/>
<pin name="LSS"/>
<pin name="GLB"/>
<pin name="SB"/>
<pin name="GHB"/>
<pin name="CB"/>
<pin name="VIN" direction="pwr"/>
<pin name="VR13"/>
<pin name="CA"/>
<pin name="GHA"/>
<pin name="SA"/>
<pin name="GLA"/>
<pin name="VBB"/>
<pin name="CP2"/>
<pin name="VCP"/>
<pin name="CP1"/>
<pin name="GND" direction="pwr"/>
<pin name="FAULT"/>
<pin name="OVSET"/>
<pin name="VR5"/>
<pin name="MODE"/>
<pin name="SR"/>
<pin name="EN"/>
<pin name="PHASE"/>
<pin name="RESET"/>
<pin name="LONG"/>
<pin name="IDEAD"/>
<pin name="VDSTH"/>
</symbol>
<symbol name="MFNS">
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="P-MOSFET-N">
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="SKB">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="SKBV">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="4620V2">
<pin name="MCLR#/THV" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4/T0CKI"/>
<pin name="RA5/AN4"/>
<pin name="RE0/RD#/AN5"/>
<pin name="RE1/WR#/AN6"/>
<pin name="RE2/CS#/AN7"/>
<pin name="RA7/OX1/CLKI"/>
<pin name="RA6/OX2/CLKO"/>
<pin name="RC0/T1OSO"/>
<pin name="RC1/T1OSI"/>
<pin name="RC2/CCP1"/>
<pin name="RC3/SCK"/>
<pin name="RD0/PSP0"/>
<pin name="RD1/PSP1"/>
<pin name="RD2/PSP2"/>
<pin name="RD3/PSP3"/>
<pin name="SDI/RC4"/>
<pin name="SDO/RC5"/>
<pin name="TX/RC6"/>
<pin name="RX/RC7"/>
<pin name="PSP4/RD4"/>
<pin name="PSP5/RD5"/>
<pin name="PSP6/RD6"/>
<pin name="PSP7/RD7"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="INT/RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="PGM/RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="PGC/RB6"/>
<pin name="PGD/RB7"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="NC@1"/>
<pin name="NC@2"/>
<pin name="NC@3"/>
<pin name="NC@4"/>
</symbol>
<symbol name="LUG">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="MICROFIT-6">
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
<pin name="P$3" direction="pas"/>
<pin name="P$4" direction="pas"/>
<pin name="P$5" direction="pas"/>
<pin name="P$6" direction="pas"/>
</symbol>
<symbol name="ACS706">
<pin name="IN@1" direction="pas"/>
<pin name="IN@2" direction="pas"/>
<pin name="OUT@1" direction="pas"/>
<pin name="OUT@2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="VAL" direction="pas"/>
<pin name="VCC" direction="pas"/>
</symbol>
<symbol name="MICROFIT-8">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="LINX-LC-S-TX">
<pin name="GND@1" direction="pwr"/>
<pin name="DATA" direction="in"/>
<pin name="GND@2" direction="pwr"/>
<pin name="LADJ" direction="pwr"/>
<pin name="ANT"/>
<pin name="GND@3"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@4"/>
</symbol>
<symbol name="LINX-LC-S-RC">
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="PDN" direction="in"/>
<pin name="NC@4" direction="nc"/>
<pin name="DATA" direction="out"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="NC@7" direction="nc"/>
<pin name="NC@8" direction="nc"/>
<pin name="NC@9" direction="nc"/>
<pin name="NC@10" direction="nc"/>
<pin name="GND@2" direction="pwr"/>
<pin name="ANT"/>
</symbol>
<symbol name="MOLEX-43045-8">
<pin name="4" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="1" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
</symbol>
<symbol name="ADAPTER-SOIC-16">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
</symbol>
<symbol name="ACS755">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VO"/>
<pin name="IP+"/>
<pin name="IP-"/>
</symbol>
<symbol name="MRF24J40">
<pin name="VDD@1" direction="pwr"/>
<pin name="RFP"/>
<pin name="RFN"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GPIO0"/>
<pin name="GPIO1"/>
<pin name="GPIO5"/>
<pin name="GPIO4"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="RESET/" direction="in"/>
<pin name="GND@2" direction="pwr"/>
<pin name="WAKE" direction="in"/>
<pin name="INT" direction="out"/>
<pin name="SDO"/>
<pin name="SDI"/>
<pin name="SCK" direction="in"/>
<pin name="CS/" direction="in"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="NC@1" direction="nc"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="CLKOUT"/>
<pin name="LPOSC2"/>
<pin name="LPOSC1"/>
<pin name="RXIP"/>
<pin name="RXQP"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="OSC2"/>
<pin name="OSC1"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="NC@2" direction="nc"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="LCAP"/>
</symbol>
<symbol name="MOLEX-34045-10">
<pin name="5" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="1" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="MOLEX-43045-4">
<pin name="2" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="1" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
<symbol name="LINX-LR-S-TX">
<pin name="GND@1" direction="pwr"/>
<pin name="DATA" direction="in"/>
<pin name="GND@2" direction="pwr"/>
<pin name="LADJ" direction="pwr"/>
<pin name="ANT"/>
<pin name="GND@3"/>
<pin name="VCC" direction="pwr"/>
<pin name="PDN" direction="in"/>
</symbol>
<symbol name="LINK-LR-S-RC">
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="PDN" direction="in"/>
<pin name="RSSI" direction="pas"/>
<pin name="DATA" direction="out"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="NC@7" direction="nc"/>
<pin name="NC@8" direction="nc"/>
<pin name="NC@9" direction="nc"/>
<pin name="NC@10" direction="nc"/>
<pin name="GND@2" direction="pwr"/>
<pin name="ANT"/>
</symbol>
<symbol name="HAIS200">
<pin name="+5" direction="pwr"/>
<pin name="0V" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="VREF" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="9VOLTBAT">
<pin name="PLUS"/>
<pin name="MINUS"/>
</symbol>
<symbol name="LTC1255">
<pin name="DS1"/>
<pin name="G1"/>
<pin name="GND" direction="pwr"/>
<pin name="IN1"/>
<pin name="IN2"/>
<pin name="VS" direction="pwr"/>
<pin name="G2"/>
<pin name="DS2"/>
</symbol>
<symbol name="3TERMINALBLOCK">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="BIGLUG">
<pin name="LUG1"/>
</symbol>
<symbol name="FUSESOCKET">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="BUTTON-BAT-12MM">
<pin name="N1"/>
<pin name="+"/>
<pin name="N2"/>
</symbol>
<symbol name="N-CHANNEL-MOSFET">
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="SDPT-SLIDE">
<pin name="1"/>
<pin name="C"/>
<pin name="3"/>
</symbol>
<symbol name="FT232BL">
<pin name="3V3OUT" direction="out"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="RSTOUT#" direction="out" function="dot"/>
<pin name="RESET#" direction="in" function="dot"/>
<pin name="XTIN" direction="in"/>
<pin name="XTOUT" direction="out"/>
<pin name="EECS"/>
<pin name="EESK" direction="out"/>
<pin name="EEDATA"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="RTS#" direction="out" function="dot"/>
<pin name="CTS#" direction="in" function="dot"/>
<pin name="DTR#" direction="out" function="dot"/>
<pin name="DSR#" direction="in" function="dot"/>
<pin name="DCD#" direction="in" function="dot"/>
<pin name="RI#" direction="in" function="dot"/>
<pin name="TXDEN" direction="out"/>
<pin name="TXLED#" direction="oc" function="dot"/>
<pin name="RXLED#" direction="oc" function="dot"/>
<pin name="PWRCTL" direction="in"/>
<pin name="PWREN#" direction="out" function="dot"/>
<pin name="SLEEP#" direction="out" function="dot"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
</symbol>
<symbol name="CSTCR-RESONATOR">
<pin name="GND" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MCP1700">
<pin name="VI" direction="in"/>
<pin name="VO" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="FERRITEBEAD">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="93LC46">
<pin name="VCC" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="DO" direction="hiz"/>
<pin name="NU" direction="pas"/>
<pin name="ORG" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="CS" direction="in"/>
</symbol>
<symbol name="18F8722">
<pin name="H2"/>
<pin name="H3"/>
<pin name="E1"/>
<pin name="E0"/>
<pin name="G0"/>
<pin name="G1/TX2"/>
<pin name="G2/RX2"/>
<pin name="G3"/>
<pin name="G5/!MCLR"/>
<pin name="G4"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="F7"/>
<pin name="F6"/>
<pin name="F5"/>
<pin name="F4"/>
<pin name="F3"/>
<pin name="F2"/>
<pin name="H7"/>
<pin name="H6"/>
<pin name="H5"/>
<pin name="H4"/>
<pin name="F1"/>
<pin name="F0"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="C1"/>
<pin name="C0"/>
<pin name="C6/TX1"/>
<pin name="C7/RX1"/>
<pin name="J4"/>
<pin name="J5"/>
<pin name="J6"/>
<pin name="J7"/>
<pin name="C2"/>
<pin name="C3/SCLK1"/>
<pin name="C4/SDI1"/>
<pin name="C5/SDO1"/>
<pin name="B7/PGD"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="A7/OSCI"/>
<pin name="A6/OSCO"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="B6/PGC"/>
<pin name="B5/PGM"/>
<pin name="B4"/>
<pin name="B3/INT3"/>
<pin name="B2/INT2"/>
<pin name="B1/INT1"/>
<pin name="B0/INT0"/>
<pin name="J3"/>
<pin name="J2"/>
<pin name="J1"/>
<pin name="J0"/>
<pin name="D7"/>
<pin name="D6/SCLK2"/>
<pin name="D5/SDI2"/>
<pin name="D4/SDO2"/>
<pin name="D3"/>
<pin name="D2"/>
<pin name="D1"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="D0"/>
<pin name="E7"/>
<pin name="E6"/>
<pin name="E5"/>
<pin name="E4"/>
<pin name="E3"/>
<pin name="E2"/>
<pin name="H0"/>
<pin name="H1"/>
</symbol>
<symbol name="PIC18F87J10">
<pin name="RE1/AD9/!WR/P2C"/>
<pin name="RE0/AD8/!RD/P2D"/>
<pin name="RG0/ECCP3/P3A"/>
<pin name="RG1/TX2/CK2"/>
<pin name="RG2/RX2/DT2"/>
<pin name="RG3/CCP4/P3D"/>
<pin name="!MCLR" direction="in"/>
<pin name="RG4/CCP5/P1D"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDDCORE/VCAP" direction="pwr"/>
<pin name="RF7/!SS1"/>
<pin name="RF6/AN11"/>
<pin name="RF5/AN10/CVREF"/>
<pin name="RF4/AN9"/>
<pin name="RF3/AN8"/>
<pin name="RF2/AN7/C1OUT"/>
<pin name="RF1/AN6/C2OUT"/>
<pin name="ENVREG" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA2/AN2/VREF-"/>
<pin name="RA1/AN1"/>
<pin name="RA0/AN0"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RA5/AN4"/>
<pin name="RA4/T0CK"/>
<pin name="RC1/T1OSI/ECCP2/P2A"/>
<pin name="RC0/T1OSO/T13CKI"/>
<pin name="RC6/TX1/CK1"/>
<pin name="RC7/RX1/DT1"/>
<pin name="RC2/ECCP1/P1A"/>
<pin name="RC3/SCK1/SCL1"/>
<pin name="RC4/SDI1/SDA1"/>
<pin name="RC5/SDO1"/>
<pin name="RB7/KBI2/PGD"/>
<pin name="VDD" direction="pwr"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="OSC2/CLKO" direction="out"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB5/KBI1"/>
<pin name="RB4/KBI0"/>
<pin name="RB3/INT3/ACCP2/P2A"/>
<pin name="RB2/INT2"/>
<pin name="RB1/INT1"/>
<pin name="RB0/INT0/FLT0"/>
<pin name="RD7/AD7/PSP7/!SS2"/>
<pin name="RD6/AD6/PSP6/SCK2/SCL2"/>
<pin name="RD5/AD5/PSP5/SDI2/SDA2"/>
<pin name="RD4/AD4/PSP4/SDO2"/>
<pin name="RD3/AD3/PSP3"/>
<pin name="RD2/AD2/PSP2"/>
<pin name="RD1/AD1/PSP1"/>
<pin name="RD0/AD0/PSP0"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="RE7/AD15/ECCP2/P2A"/>
<pin name="RE6/AD14/P1B"/>
<pin name="RE5/AD13/P1C"/>
<pin name="RE4/AD12/P3B"/>
<pin name="RE3/AD11/P3C"/>
<pin name="RE2/!AD10CS/P2B"/>
<pin name="RH2/A18"/>
<pin name="RH3/A19"/>
<pin name="RH7/AN15/P1B"/>
<pin name="RH6/AN14/P1C"/>
<pin name="RH5/AN13/P3B"/>
<pin name="RH4/AN12/P3C"/>
<pin name="RJ4/BA0"/>
<pin name="RJ5/!CE"/>
<pin name="RJ6/!LB"/>
<pin name="RJ7/!UB"/>
<pin name="RJ3/!WRH"/>
<pin name="RJ2/!WRL"/>
<pin name="RJ1/!OE"/>
<pin name="RJ0/ALE"/>
<pin name="RH0/A16"/>
<pin name="RH1/A17"/>
</symbol>
<symbol name="PIC64PIN-SQ">
<pin name="E1"/>
<pin name="E0"/>
<pin name="G0"/>
<pin name="G1/TX2"/>
<pin name="G2/RX2"/>
<pin name="G3"/>
<pin name="G5/!MCLR"/>
<pin name="G4"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="F7"/>
<pin name="F6"/>
<pin name="F5"/>
<pin name="F4"/>
<pin name="F3"/>
<pin name="F2"/>
<pin name="F1"/>
<pin name="F0"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="C1"/>
<pin name="C0"/>
<pin name="C6/TX1"/>
<pin name="C7/RX1"/>
<pin name="C2"/>
<pin name="C3/SCLK1"/>
<pin name="C4/MISO1"/>
<pin name="C5/MOSI1"/>
<pin name="B7/PGD"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="A7/OSCI"/>
<pin name="A6/OSCO"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="B6/PGC"/>
<pin name="B5/PGM"/>
<pin name="B4"/>
<pin name="B3/INT3"/>
<pin name="B2/INT2"/>
<pin name="B1/INT1"/>
<pin name="B0/INT0"/>
<pin name="D7"/>
<pin name="D6/SCLK2"/>
<pin name="D5/MISO2"/>
<pin name="D4/MOSI2"/>
<pin name="D3"/>
<pin name="D2"/>
<pin name="D1"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="D0"/>
<pin name="E7"/>
<pin name="E6"/>
<pin name="E5"/>
<pin name="E4"/>
<pin name="E3"/>
<pin name="E2"/>
</symbol>
<symbol name="LM2937A-3.3">
<pin name="IN" direction="in"/>
<pin name="VOUT" direction="pas"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="FT232R">
<pin name="VCC" direction="pwr"/>
<pin name="3V3OUT" direction="out"/>
<pin name="USBDP"/>
<pin name="USBDM"/>
<pin name="OSCO"/>
<pin name="OSCI"/>
<pin name="GND" direction="pwr"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="RTS#" direction="out"/>
<pin name="CTS#" direction="in"/>
<pin name="DTR#"/>
<pin name="DSR#"/>
<pin name="DCD#"/>
<pin name="RI#"/>
<pin name="CBUS0"/>
<pin name="CBUS1"/>
<pin name="CBUS2"/>
<pin name="CBUS3"/>
<pin name="CBUS4"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="RESET#" direction="in"/>
<pin name="GND@A" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="PINH2X6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD12">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X8">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
</symbol>
<symbol name="DM2023">
<pin name="GND" direction="pwr"/>
<pin name="V0" direction="pwr"/>
<pin name="R/W" direction="in"/>
<pin name="DB0"/>
<pin name="DB2"/>
<pin name="DB4"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="DB5"/>
<pin name="DB3"/>
<pin name="DB1"/>
<pin name="EN" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="5.0V" direction="pwr"/>
</symbol>
<symbol name="MA07-2">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="13" direction="pas"/>
</symbol>
<symbol name="DOCSMAL-L">
</symbol>
<symbol name="PORTOUT">
</symbol>
<symbol name="PORT3">
</symbol>
<symbol name="PORTIN">
</symbol>
<symbol name="PORTBI">
</symbol>
<symbol name="USB">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
</symbol>
<symbol name="USB-SHIELDED">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="LETTER_L">
</symbol>
<symbol name="DOCFIELD">
</symbol>
<symbol name="GENERIC28SSOP">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
</symbol>
<symbol name="AT86RF230">
<pin name="AVSS@1" direction="pwr"/>
<pin name="AVSS@2" direction="pwr"/>
<pin name="AVSS@3" direction="pwr"/>
<pin name="RFP"/>
<pin name="RFN"/>
<pin name="AVSS@4" direction="pwr"/>
<pin name="TST" direction="in"/>
<pin name="RST/" direction="in"/>
<pin name="DVSS@1" direction="pwr"/>
<pin name="DVSS@2" direction="pwr"/>
<pin name="SLP" direction="in"/>
<pin name="DVSS@3" direction="pwr"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="DEVDD" direction="pwr"/>
<pin name="DVSS@4" direction="pwr"/>
<pin name="CLKM" direction="out"/>
<pin name="DVSS@5" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="MISO"/>
<pin name="DVSS@6" direction="pwr"/>
<pin name="MOSI" direction="out"/>
<pin name="SEL/" direction="in"/>
<pin name="IRQ" direction="out"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="AVSS@5" direction="pwr"/>
<pin name="EVDD" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS@6" direction="pwr"/>
<pin name="AVSS@7" direction="pwr"/>
<pin name="AVSS@8" direction="pwr"/>
</symbol>
<symbol name="XTAL4025">
<pin name="GND@2" direction="pwr"/>
<pin name="X1" direction="pas"/>
<pin name="GND@1" direction="pwr"/>
<pin name="X2" direction="pas"/>
</symbol>
<symbol name="AT86RF230R1">
<pin name="AVSS@1" direction="pwr"/>
<pin name="AVSS@2" direction="pwr"/>
<pin name="AVSS@3" direction="pwr"/>
<pin name="RFP"/>
<pin name="RFN"/>
<pin name="AVSS@4" direction="pwr"/>
<pin name="TST" direction="in"/>
<pin name="RST/" direction="in"/>
<pin name="DVSS@1" direction="pwr"/>
<pin name="DVSS@2" direction="pwr"/>
<pin name="SLP" direction="in"/>
<pin name="DVSS@3" direction="pwr"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="DEVDD" direction="pwr"/>
<pin name="DVSS@4" direction="pwr"/>
<pin name="CLKM" direction="out"/>
<pin name="DVSS@5" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="MISO"/>
<pin name="DVSS@6" direction="pwr"/>
<pin name="MOSI" direction="out"/>
<pin name="SEL/" direction="in"/>
<pin name="IRQ" direction="out"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="AVSS@5" direction="pwr"/>
<pin name="EVDD" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS@6" direction="pwr"/>
<pin name="AVSS@7" direction="pwr"/>
<pin name="AVSS@8" direction="pwr"/>
<pin name="AVSS@0"/>
</symbol>
<symbol name="POT_US-">
<pin name="A" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="BRIDGE-DRIVER3941">
<pin name="VDR"/>
<pin name="LSS"/>
<pin name="GLB"/>
<pin name="SB"/>
<pin name="GHB"/>
<pin name="CB"/>
<pin name="VREG@1" direction="pwr"/>
<pin name="VREG@2" direction="pwr"/>
<pin name="CA"/>
<pin name="GHA"/>
<pin name="SA"/>
<pin name="GLA"/>
<pin name="VBB@1" direction="pwr"/>
<pin name="VBB@2" direction="pwr"/>
<pin name="CP2"/>
<pin name="CP1"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="PHASE"/>
<pin name="V5"/>
<pin name="SR"/>
<pin name="PWML"/>
<pin name="PWMH"/>
<pin name="RESET"/>
<pin name="FF1"/>
<pin name="FF2"/>
<pin name="RDEAD"/>
<pin name="VDSTH"/>
<pin name="PAD" direction="pwr"/>
</symbol>
<symbol name="MCP1252/3">
<pin name="PGOOD" direction="oc"/>
<pin name="VOUT" direction="sup"/>
<pin name="VIN" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="C-" direction="pas"/>
<pin name="C+" direction="pas"/>
<pin name="SHDN#" direction="in"/>
<pin name="SELECT" direction="in"/>
</symbol>
<symbol name="CF-LCD-128">
<pin name="GND" direction="pwr"/>
<pin name="V0" direction="pwr"/>
<pin name="R/W" direction="in"/>
<pin name="DB0"/>
<pin name="DB2"/>
<pin name="DB4"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="DB5"/>
<pin name="DB3"/>
<pin name="DB1"/>
<pin name="EN" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="5.0V" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="RESET/" direction="in"/>
<pin name="CS/" direction="in"/>
</symbol>
<symbol name="PINH2X9">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
</symbol>
<symbol name="ZIG-DAUGHTER">
<pin name="SLP" direction="in"/>
<pin name="MISO" direction="out"/>
<pin name="!SEL" direction="in"/>
<pin name="NC"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="!RST" direction="in"/>
<pin name="IRQ" direction="out"/>
<pin name="MOSI" direction="in"/>
<pin name="SCK" direction="in"/>
</symbol>
<symbol name="2-TERM-BLOCK">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="TERMBLOCK-4">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="LCD-MULTI">
<pin name="GND" direction="pwr"/>
<pin name="V0" direction="pwr"/>
<pin name="R/W" direction="in"/>
<pin name="DB0"/>
<pin name="DB2"/>
<pin name="DB4"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="DB5"/>
<pin name="DB3"/>
<pin name="DB1"/>
<pin name="EN" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="5.0V" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="RESET/" direction="in"/>
<pin name="CS/" direction="in"/>
<pin name="D-ON" direction="in"/>
<pin name="BL+" direction="pwr"/>
<pin name="BL-" direction="pwr"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="PINH2X2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
<symbol name="SCHOTTKY">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="BALUN">
<pin name="UB"/>
<pin name="GND@1"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="GND@2"/>
<pin name="NC"/>
</symbol>
<symbol name="PIC18F67J11">
<pin name="E1"/>
<pin name="E0"/>
<pin name="G0"/>
<pin name="G1/TX2"/>
<pin name="G2/RX2"/>
<pin name="G3"/>
<pin name="MCLR"/>
<pin name="G4"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VCAP" direction="pas"/>
<pin name="F7"/>
<pin name="F6"/>
<pin name="F5"/>
<pin name="F4"/>
<pin name="F3"/>
<pin name="F2"/>
<pin name="F1"/>
<pin name="ENVREG" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="C1"/>
<pin name="C0"/>
<pin name="C6/TX1"/>
<pin name="C7/RX1"/>
<pin name="C2"/>
<pin name="C3/SCLK1"/>
<pin name="C4/SDI1"/>
<pin name="C5/SDO1"/>
<pin name="B7/PGD"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="A7/OSCI"/>
<pin name="A6/OSCO"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="B6/PGC"/>
<pin name="B5/PGM"/>
<pin name="B4"/>
<pin name="B3/INT3"/>
<pin name="B2/INT2"/>
<pin name="B1/INT1"/>
<pin name="B0/INT0"/>
<pin name="D7"/>
<pin name="D6/SCLK2"/>
<pin name="D5/SDI2"/>
<pin name="D4/SDO2"/>
<pin name="D3"/>
<pin name="D2"/>
<pin name="D1"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="D0"/>
<pin name="E7"/>
<pin name="E6"/>
<pin name="E5"/>
<pin name="E4"/>
<pin name="E3"/>
<pin name="E2"/>
</symbol>
<symbol name="CONNECTOR-1X5">
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
<pin name="P$3" direction="pas"/>
<pin name="P$4" direction="pas"/>
<pin name="P$5" direction="pas"/>
</symbol>
<symbol name="18F4620-SQ">
<pin name="!MCLR" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4/T0CKI"/>
<pin name="RA5/AN4"/>
<pin name="RE0/AN5"/>
<pin name="RE1/AN6"/>
<pin name="RE2/AN7"/>
<pin name="RA7/OX1"/>
<pin name="RA6/OX2"/>
<pin name="RC0"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3/SCK"/>
<pin name="RD0"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RC4/MISO"/>
<pin name="RC5/MOSI"/>
<pin name="RC6/TX"/>
<pin name="RC7/RX"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3/PGM"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6/PGC"/>
<pin name="RB7/PGD"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
</symbol>
<symbol name="N-MOS">
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="LCD2">
<pin name="GND" direction="pwr"/>
<pin name="V0" direction="pwr"/>
<pin name="R/W" direction="in"/>
<pin name="DB0"/>
<pin name="DB2"/>
<pin name="DB4"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="DB5"/>
<pin name="DB3"/>
<pin name="DB1"/>
<pin name="EN" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="5.0V" direction="pwr"/>
</symbol>
<symbol name="LCD-W/BL">
<pin name="GND" direction="pwr"/>
<pin name="V0" direction="pwr"/>
<pin name="R/!W" direction="in"/>
<pin name="DB0"/>
<pin name="DB2"/>
<pin name="DB4"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="DB5"/>
<pin name="DB3"/>
<pin name="DB1"/>
<pin name="EN" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="5.0V" direction="pwr"/>
<pin name="BL+" direction="pwr"/>
<pin name="BL-" direction="pwr"/>
</symbol>
<symbol name="DF11-CONNECTOR">
<pin name="4" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="1" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
</symbol>
<symbol name="CFA635-LCD">
<pin name="LCD-RX" direction="in"/>
<pin name="LCD-TX" direction="out"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="GND" direction="pwr"/>
<pin name="+5V" direction="pwr"/>
</symbol>
<symbol name="HB3-INTERFACE">
<pin name="PWMH" direction="in"/>
<pin name="PWML" direction="in"/>
<pin name="PHASE" direction="in"/>
<pin name="SR" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="FF1" direction="out"/>
<pin name="FF2" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="AT86RF231">
<pin name="DIG1"/>
<pin name="DIG2"/>
<pin name="AVSS@3" direction="pwr"/>
<pin name="RFP"/>
<pin name="RFN"/>
<pin name="AVSS@4" direction="pwr"/>
<pin name="DVSS@1" direction="pwr"/>
<pin name="RST/" direction="in"/>
<pin name="DIG3"/>
<pin name="DIG4"/>
<pin name="SLP" direction="in"/>
<pin name="DVSS@3" direction="pwr"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="DEVDD" direction="pwr"/>
<pin name="DVSS@4" direction="pwr"/>
<pin name="CLKM" direction="out"/>
<pin name="DVSS@5" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="MISO"/>
<pin name="DVSS@6" direction="pwr"/>
<pin name="MOSI" direction="out"/>
<pin name="SEL/" direction="in"/>
<pin name="IRQ" direction="out"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="AVSS@5" direction="pwr"/>
<pin name="EVDD" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS@6" direction="pwr"/>
<pin name="AVSS@7" direction="pwr"/>
<pin name="AVSS@8" direction="pwr"/>
<pin name="AVSS@0"/>
</symbol>
<symbol name="18F2520">
<pin name="E3/MCLR"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="A7"/>
<pin name="A6"/>
<pin name="C0"/>
<pin name="C1"/>
<pin name="C2"/>
<pin name="C3"/>
<pin name="C4"/>
<pin name="C5"/>
<pin name="C6"/>
<pin name="C7"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="B0"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
</symbol>
<symbol name="IOCONNECTOR">
<pin name="RXIN" direction="in"/>
<pin name="D0/K1"/>
<pin name="D2/K3"/>
<pin name="RS" direction="in"/>
<pin name="R/!W" direction="in"/>
<pin name="L1"/>
<pin name="L3"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="L4"/>
<pin name="L2"/>
<pin name="K5" direction="out"/>
<pin name="EN" direction="in"/>
<pin name="D3/K4"/>
<pin name="D1/K2"/>
<pin name="TXOUT" direction="out"/>
</symbol>
<symbol name="FLEXCON-16">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
</symbol>
<symbol name="CON2X2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
<symbol name="CON2X3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="CON2X5">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
</symbol>
<symbol name="IDC2X8">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="SWITCH-PB-TINY">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CON2X4">
<pin name="1" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
</symbol>
<symbol name="POT-VADJ">
<pin name="A" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="4620QFN">
<pin name="MCLR" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4"/>
<pin name="RA5/AN4"/>
<pin name="RE0/AN5"/>
<pin name="RE1/AN6"/>
<pin name="RE2/AN7"/>
<pin name="RA7/OX1"/>
<pin name="RA6/OX2"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3/SCK"/>
<pin name="RD0"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RC4/MISO"/>
<pin name="RC5/MOSI"/>
<pin name="RC6/TX"/>
<pin name="RC7/RX"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3/PGM"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6/PGC"/>
<pin name="RB7/PGD"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="RC0"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
</symbol>
<symbol name="LCD-1X16">
<pin name="GND" direction="pwr"/>
<pin name="+5V" direction="pwr"/>
<pin name="VO" direction="pwr"/>
<pin name="RS" direction="in"/>
<pin name="R/!W" direction="in"/>
<pin name="E" direction="in"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="BL+" direction="pwr"/>
<pin name="BL-" direction="pwr"/>
</symbol>
<symbol name="DIODE">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="ICSP">
<pin name="!MCLR" direction="pwr"/>
<pin name="PGC" direction="pwr"/>
<pin name="PGD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="FFC-8">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
</symbol>
<symbol name="JOYSTICK-2AX">
<pin name="R1B" direction="pas"/>
<pin name="R1T" direction="pas"/>
<pin name="R1C" direction="pas"/>
<pin name="R2L" direction="pas"/>
<pin name="R2R" direction="pas"/>
<pin name="R2C" direction="pas"/>
</symbol>
<symbol name="1V2+2">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
<pin name="+@1" direction="pas"/>
</symbol>
<symbol name="SW-DPDT">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
<pin name="P1" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="O1" direction="pas"/>
</symbol>
<symbol name="SW-SPDT-D">
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="U2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="SIS-">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="CONNECTOR-1X3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="MMA7455">
<pin name="VDD" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="NC@1" direction="nc"/>
<pin name="ADD" direction="in"/>
<pin name="GND@2" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="!CS" direction="in"/>
<pin name="INT1" direction="out"/>
<pin name="INT2" direction="out"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="MISO" direction="out"/>
<pin name="MOSI" direction="in"/>
<pin name="SCLK" direction="in"/>
</symbol>
<symbol name="CONNECTOR-1X2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CONNECTOR-1X4">
<pin name="P1" direction="pas"/>
<pin name="P2" direction="pas"/>
<pin name="P3" direction="pas"/>
<pin name="P4" direction="pas"/>
</symbol>
<symbol name="CONNECTOR-1X5-R">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="CONNECTOR-1X5-L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="IDC-2X5">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="PROG">
<pin name="NC@1" direction="nc"/>
<pin name="VPP" direction="out"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="PGD" direction="out"/>
<pin name="NC@4" direction="nc"/>
<pin name="PGC" direction="out"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="SIS">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="ABM3B-XTAL">
<pin name="X1" direction="pas"/>
<pin name="GND@2" direction="pwr"/>
<pin name="X2" direction="pas"/>
<pin name="GND@4" direction="pwr"/>
</symbol>
<symbol name="BNC-FGND">
<pin name="1" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="SW-DP3T">
<pin name="COM1" direction="pas"/>
<pin name="1A" direction="pas"/>
<pin name="1B" direction="pas"/>
<pin name="1C" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="2A" direction="pas"/>
<pin name="2B" direction="pas"/>
<pin name="2C" direction="pas"/>
</symbol>
<symbol name="SW-DPDT-SLIDE">
<pin name="A1" direction="pas"/>
<pin name="AC" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="BC" direction="pas"/>
<pin name="B1" direction="pas"/>
</symbol>
<symbol name="IDC-2X12">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="SW-PB-SPST">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="18F2420">
<pin name="!MCLR" direction="in"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="A7"/>
<pin name="A6"/>
<pin name="C0"/>
<pin name="C1"/>
<pin name="C2"/>
<pin name="C3/SCLK"/>
<pin name="C4/MISO"/>
<pin name="C5/MOSI"/>
<pin name="C6/MTX"/>
<pin name="C7/MRX"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="B0"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
</symbol>
<symbol name="18F2420-SQ">
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5/!SS"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="A7"/>
<pin name="A6"/>
<pin name="C0"/>
<pin name="C1"/>
<pin name="C2"/>
<pin name="C3/SCK"/>
<pin name="C4/MISO"/>
<pin name="C5/MOSI"/>
<pin name="C6/MTH"/>
<pin name="C7/MRX"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="B0"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="!MCLR" direction="in"/>
<pin name="A0"/>
<pin name="A1"/>
</symbol>
<symbol name="TP">
<pin name="P$1" direction="pas"/>
</symbol>
<symbol name="P-MOS">
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="DS1390">
<pin name="X1"/>
<pin name="X2"/>
<pin name="VBACKUP" direction="pwr"/>
<pin name="CS" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="SQW/INT"/>
<pin name="SCLK" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="DIN" direction="in"/>
</symbol>
<symbol name="GB">
<pin name="AC1" direction="pas"/>
<pin name="AC2" direction="pas"/>
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
<symbol name="K">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="U">
<pin name="NC" direction="pas"/>
<pin name="NO" direction="pas"/>
<pin name="P" direction="pas"/>
</symbol>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="4620QFN-G">
<pin name="MCLR" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4"/>
<pin name="RA5/AN4"/>
<pin name="RE0/AN5"/>
<pin name="RE1/AN6"/>
<pin name="RE2/AN7"/>
<pin name="RA7/OX1"/>
<pin name="RA6/OX2"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3/SCK"/>
<pin name="RD0"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RC4/MISO"/>
<pin name="RC5/MOSI"/>
<pin name="RC6/TX"/>
<pin name="RC7/RX"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3/PGM"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6/PGC"/>
<pin name="RB7/PGD"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="RC0"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
</symbol>
<symbol name="AC-IN">
<pin name="COM"/>
<pin name="HOT"/>
</symbol>
<symbol name="DIN-6">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="GND@1" direction="sup"/>
<pin name="GND@2" direction="sup"/>
<pin name="GND@3" direction="sup"/>
</symbol>
<symbol name="POWER-16GAUGE">
<pin name="+" direction="sup"/>
<pin name="-" direction="sup"/>
</symbol>
<symbol name="PHONO-JACK">
<pin name="SIG"/>
<pin name="GND@1" direction="sup"/>
<pin name="GND@2" direction="sup"/>
<pin name="GND@3" direction="sup"/>
</symbol>
<symbol name="LED-RGB">
<pin name="C1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="C3" direction="pas"/>
<pin name="A3" direction="pas"/>
</symbol>
<symbol name="LEDDRV-PCA9635">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="LED0"/>
<pin name="LED1"/>
<pin name="LED2"/>
<pin name="LED3"/>
<pin name="LED4"/>
<pin name="LED5"/>
<pin name="LED6"/>
<pin name="LED7"/>
<pin name="VSS" direction="pwr"/>
<pin name="LED8"/>
<pin name="LED9"/>
<pin name="LED10"/>
<pin name="LED11"/>
<pin name="LED12"/>
<pin name="LED13"/>
<pin name="LED14"/>
<pin name="LED15"/>
<pin name="!OE" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="SD-5638">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="P1/CS"/>
<pin name="P2/DI"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="P5/CLK"/>
<pin name="GND@3" direction="pwr"/>
<pin name="P7/DO"/>
<pin name="P8/IRQ"/>
<pin name="P9/DAT2"/>
<pin name="PCD"/>
<pin name="PWP"/>
</symbol>
<symbol name="OPAMP+-">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="CUR_SENSE_TAMURA">
<pin name="VOUT"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="LICAL-DECODER">
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="SBD0" direction="in"/>
<pin name="SBD1" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="LATCH" direction="in"/>
<pin name="RX_CTL"/>
<pin name="TX_ID" direction="out"/>
<pin name="MODE_IN" direction="out"/>
<pin name="LRN" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
</symbol>
<symbol name="ANT-315">
<pin name="P$1" direction="pas"/>
</symbol>
<symbol name="VR-TC1185">
<pin name="VIN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="pas"/>
<pin name="!SHDN" direction="in"/>
<pin name="BYP" direction="out"/>
</symbol>
<symbol name="CONNECTOR-1X6-R">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="LED-RG">
<pin name="CR" direction="pas"/>
<pin name="AR" direction="pas"/>
<pin name="CG" direction="pas"/>
<pin name="AG" direction="pas"/>
</symbol>
<symbol name="INV300X">
<pin name="ANT" direction="in"/>
<pin name="BAT" direction="sup"/>
<pin name="GP1" direction="in"/>
<pin name="ON" direction="in"/>
<pin name="TXA" direction="out"/>
<pin name="GP4" direction="in"/>
<pin name="TXB" direction="out"/>
<pin name="BOOT" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GP5" direction="in"/>
<pin name="RXB" direction="in"/>
<pin name="GP3" direction="in"/>
<pin name="RXA" direction="in"/>
<pin name="PCHK" direction="out"/>
<pin name="RESET" direction="in"/>
<pin name="TIME" direction="out"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="74LV1G07">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="I1" direction="in"/>
<pin name="O1" direction="oc"/>
</symbol>
<symbol name="L-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="TXB0108">
<pin name="A1"/>
<pin name="VA" direction="sup"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="OE" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="B8"/>
<pin name="B7"/>
<pin name="B6"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="VB" direction="sup"/>
<pin name="B1"/>
</symbol>
<symbol name="DIODE-ZENER">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="LEM-HAAS">
</symbol>
<symbol name="AC-OPTO-DUAL">
<pin name="AC1A" direction="pas"/>
<pin name="AC1B" direction="pas"/>
<pin name="AC2A" direction="pas"/>
<pin name="AC2B" direction="pas"/>
<pin name="E2" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="E1" direction="pas"/>
<pin name="C1" direction="pas"/>
</symbol>
<symbol name="LM317">
<pin name="IN" direction="in"/>
<pin name="VOUT" direction="pas"/>
<pin name="ADJ" direction="pas"/>
</symbol>
<symbol name="CONNECTOR-1X12-L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="CONNECTOR-1X12-R">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="CONNECTOR-1X8-R">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="MPU-6000">
<pin name="CLKIN" direction="in"/>
<pin name="NC$1" direction="nc"/>
<pin name="NC$2" direction="nc"/>
<pin name="NC$3" direction="nc"/>
<pin name="NC$4" direction="nc"/>
<pin name="AUX_DA"/>
<pin name="AUX_CL"/>
<pin name="!CS" direction="in"/>
<pin name="AD0/SDO"/>
<pin name="REGOUT" direction="out"/>
<pin name="FSYNC" direction="out"/>
<pin name="INT" direction="out"/>
<pin name="VDD" direction="sup"/>
<pin name="NC$5" direction="nc"/>
<pin name="NC$6" direction="nc"/>
<pin name="NC$7" direction="nc"/>
<pin name="NC$8" direction="nc"/>
<pin name="GND" direction="sup"/>
<pin name="RESV$1" direction="nc"/>
<pin name="CPOUT" direction="out"/>
<pin name="RESV$2" direction="nc"/>
<pin name="CLKOUT" direction="out"/>
<pin name="SCL/SCLK"/>
<pin name="SDA/SDI"/>
</symbol>
<symbol name="MPU-6050">
<pin name="CLKIN" direction="in"/>
<pin name="NC$1" direction="nc"/>
<pin name="NC$2" direction="nc"/>
<pin name="NC$3" direction="nc"/>
<pin name="NC$4" direction="nc"/>
<pin name="AUX_DA"/>
<pin name="AUX_CL"/>
<pin name="VLOGIC" direction="in"/>
<pin name="AD0"/>
<pin name="REGOUT" direction="out"/>
<pin name="FSYNC" direction="out"/>
<pin name="INT" direction="out"/>
<pin name="VDD" direction="sup"/>
<pin name="NC$5" direction="nc"/>
<pin name="NC$6" direction="nc"/>
<pin name="NC$7" direction="nc"/>
<pin name="NC$8" direction="nc"/>
<pin name="GND" direction="sup"/>
<pin name="RESV$1" direction="nc"/>
<pin name="CPOUT" direction="out"/>
<pin name="RESV$2" direction="nc"/>
<pin name="CLKOUT" direction="out"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
<symbol name="BMP085">
<pin name="GND" direction="sup"/>
<pin name="EOC" direction="out"/>
<pin name="VDDA" direction="sup"/>
<pin name="VDD" direction="sup"/>
<pin name="NC" direction="nc"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="XCLR" direction="in"/>
</symbol>
<symbol name="ADXL345">
<pin name="VDDIO" direction="out"/>
<pin name="GND@1" direction="out"/>
<pin name="RESV@1" direction="nc"/>
<pin name="GND@2" direction="sup"/>
<pin name="GND@3" direction="sup"/>
<pin name="VSS" direction="sup"/>
<pin name="!CS" direction="in"/>
<pin name="INT1" direction="out"/>
<pin name="INT2" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="RESV@2" direction="nc"/>
<pin name="SDO/ALT"/>
<pin name="SDA/SDI"/>
<pin name="SCL" direction="in"/>
</symbol>
<symbol name="ADMP405">
<pin name="GND"/>
<pin name="VDD"/>
<pin name="OUT"/>
</symbol>
<symbol name="MEDIATEK3329">
<pin name="VCC" direction="sup"/>
<pin name="EN" direction="in"/>
<pin name="GND@1" direction="sup"/>
<pin name="VBACK" direction="sup"/>
<pin name="3DFIX" direction="out"/>
<pin name="DPLUS" direction="out"/>
<pin name="DMINUS" direction="out"/>
<pin name="GND@2" direction="sup"/>
<pin name="TX" direction="out"/>
<pin name="RX" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
</symbol>
<symbol name="PIC24FJ256GB210">
<pin name="RB0/RP0/AN0/CN2/VR+/PGD1/PMA6"/>
<pin name="RB1/RP1/AN1/CN3/VR-/PGC1/EMUC1"/>
<pin name="RB2/RP13/AN2/CN4/SS1/C2IN-"/>
<pin name="RB3/AN3/CN5/C2IN+"/>
<pin name="RP28/RB4/AN4/CN6/C1IN-"/>
<pin name="RP18/RB5/AN5/CN7/C1IN+"/>
<pin name="RB6/AN6/OCFA/EMUC2/PGC2"/>
<pin name="RB7/AN7/EMUD2/PGD2"/>
<pin name="RB8/AN8/U2CTS/C1OUT"/>
<pin name="RB9/AN9/C2OUT/PMA7"/>
<pin name="RB10/AN10/TMS/CVREF/PMA13"/>
<pin name="RB11/AN11/TDO/PMA12"/>
<pin name="RB12/AN12/TCK/PMA11"/>
<pin name="RB13/AN13/TDI/PMA10"/>
<pin name="RB14/AN14/U2RTS/BCLK2/PMA1"/>
<pin name="RB15/AN15/CN12/OCFB/PMA0"/>
<pin name="RF1"/>
<pin name="RD1/OC2/RP24"/>
<pin name="RD2/OC3/RP23"/>
<pin name="RD3/OC4/PMBE/RP22"/>
<pin name="RD4/OC5/IC5/CN13/PMWR/RP25"/>
<pin name="RD5/CN14/PMRD/RP20"/>
<pin name="RD6/CN15"/>
<pin name="RD7/CN16"/>
<pin name="RD8/IC1/INT1/RTCC"/>
<pin name="RD9/SDA1/IC2/INT2/U1CTS"/>
<pin name="RD10/SCL1/IC3/INT3/PMCS2"/>
<pin name="RD11/IC4/INT4/PMCS1"/>
<pin name="RC15/CLKO/OSC2"/>
<pin name="RC12/CLKI/OSC1"/>
<pin name="PMD0/RE0"/>
<pin name="PMD1/RE1"/>
<pin name="SOSCI/CN1/RC13"/>
<pin name="SOSCO/T1CK/CN0/RC14"/>
<pin name="RF0"/>
<pin name="SDO1/U1TX/RF3"/>
<pin name="PMA9/SDA2/CN17/U2RX/RF4"/>
<pin name="PMA8/SCL2/CN18/U2TX/RF5"/>
<pin name="DHM/RP11/INT0/CN49/RD0"/>
<pin name="PMD2/RE2"/>
<pin name="PMD3/RE3"/>
<pin name="SCL1/RG2"/>
<pin name="SDA1/RG3"/>
<pin name="RG6/RP21/PMA5/CN8/SCK2"/>
<pin name="RP26/PMA4/CN9/SDI2/RG7"/>
<pin name="RP19/PMA3/CN10/SDO2/RG8"/>
<pin name="PMD4/RE4"/>
<pin name="PMD5/RE5"/>
<pin name="SCL3/PMD6/RE6"/>
<pin name="SDA3/PMD7/RE7"/>
<pin name="RP27/PMA2/SS2/CN11/RG9"/>
<pin name="!MCLR" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="ENVREG" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VBUS/RF7"/>
<pin name="VUSB"/>
<pin name="VCAP" direction="pas"/>
</symbol>
<symbol name="MINI-USB">
<pin name="1" direction="in"/>
<pin name="2" direction="in"/>
<pin name="3" direction="in"/>
<pin name="4" direction="in"/>
<pin name="5" direction="in"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
</symbol>
<symbol name="MICRO-USB">
<pin name="1" direction="in"/>
<pin name="2" direction="in"/>
<pin name="3" direction="in"/>
<pin name="4" direction="in"/>
<pin name="5" direction="in"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="GND3" direction="pas"/>
<pin name="GND4" direction="pas"/>
</symbol>
<symbol name="ACS714">
<pin name="IN@1" direction="pas"/>
<pin name="IN@2" direction="pas"/>
<pin name="OUT@1" direction="pas"/>
<pin name="OUT@2" direction="pas"/>
<pin name="GND" direction="sup"/>
<pin name="FIL" direction="pas"/>
<pin name="VAL" direction="pas"/>
<pin name="VCC" direction="sup"/>
</symbol>
<symbol name="FT230X">
<pin name="VCC" direction="pwr"/>
<pin name="3V3OUT" direction="out"/>
<pin name="USBDP"/>
<pin name="USBDM"/>
<pin name="GND" direction="pwr"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="RTS#" direction="out"/>
<pin name="CTS#" direction="in"/>
<pin name="CBUS0"/>
<pin name="CBUS1"/>
<pin name="CBUS2"/>
<pin name="CBUS3"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="RESET#" direction="in"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="PICKIT3">
<pin name="VPP/!MCLR" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="PGD"/>
<pin name="PGC"/>
<pin name="LVP(NC)"/>
</symbol>
<symbol name="PIC32MX795">
<pin name="RB0/AN0/CN2/VR+/PGD1/PMA6"/>
<pin name="RB1/AN1/CN3/VR-/PGC1/EMUC1"/>
<pin name="RB2/AN2/CN4/SS1/C2IN-"/>
<pin name="RB3/AN3/CN5/C2IN+"/>
<pin name="RB4/AN4/CN6/C1IN-"/>
<pin name="RB5/AN5/CN7/C1IN+"/>
<pin name="RB6/AN6/OCFA/PGC2"/>
<pin name="RB7/AN7/PGD2"/>
<pin name="RB8/U5RX/AN8/U2CTS/C1OUT"/>
<pin name="RB9/AN9/C2OUT/PMA7"/>
<pin name="RB10/AN10/TMS/CVREF/PMA13"/>
<pin name="RB11/AN11/TDO/PMA12"/>
<pin name="RB12/AN12/TCK/PMA11"/>
<pin name="RB13/AN13/TDI/PMA10"/>
<pin name="RB14/AN14/U2RTS/SCK4/PMA1"/>
<pin name="RB15/AN15/CN12/OCFB/PMA0"/>
<pin name="RF1"/>
<pin name="RD1/OC2/U4TX/SCL3"/>
<pin name="RD2/OC3/SDA3/SDI3/U1RX"/>
<pin name="RD3/OC4/PMBE/SDO3/SCL3/U1TX"/>
<pin name="RD4/OC5/IC5/CN13/PMWR/RP25"/>
<pin name="RD5/CN14/PMRD/RP20"/>
<pin name="RD6/CN15"/>
<pin name="RD7/CN16"/>
<pin name="RD8/IC1/INT1/RTCC"/>
<pin name="RD9/SDA1/IC2/INT2/U4RX"/>
<pin name="RD10/SCL1/IC3/INT3/PMCS2"/>
<pin name="RD11/IC4/INT4/PMCS1"/>
<pin name="RC15/CLKO/OSC2"/>
<pin name="RC12/CLKI/OSC1"/>
<pin name="PMD0/RE0"/>
<pin name="PMD1/RE1"/>
<pin name="SOSCI/CN1/RC13"/>
<pin name="SOSCO/T1CK/CN0/RC14"/>
<pin name="RF0"/>
<pin name="USBID/RF3"/>
<pin name="PMA9/SDA2/CN17/U2RX/RF4"/>
<pin name="PMA8/SCL5/SDO4/CN18/U2TX/RF5"/>
<pin name="OC1/INT0/RD0"/>
<pin name="PMD2/RE2"/>
<pin name="PMD3/RE3"/>
<pin name="D+/RG2"/>
<pin name="D-/RG3"/>
<pin name="RG6/U6TX/PMA5/CN8/SCK2"/>
<pin name="SDA4/U3RX/PMA4/CN9/SDI2/RG7"/>
<pin name="SCL4/U3TX/PMA3/CN10/SDO2/RG8"/>
<pin name="PMD4/RE4"/>
<pin name="PMD5/RE5"/>
<pin name="SCL3/PMD6/RE6"/>
<pin name="SDA3/PMD7/RE7"/>
<pin name="U6RX/PMA2/SS2/CN11/RG9"/>
<pin name="!MCLR" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@V" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VBUS"/>
<pin name="VUSB"/>
<pin name="VCAP" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MAX3323" prefix="IC">
<description>RS-232 level converter (3.3 - 5.0 VDD)</description>
<gates>
<gate name="G$1" symbol="MAX3323"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="RIN" pad="8"/>
<connect gate="G$1" pin="ROUT" pad="9"/>
<connect gate="G$1" pin="RXEN" pad="12"/>
<connect gate="G$1" pin="SHDN" pad="14"/>
<connect gate="G$1" pin="TIN" pad="10"/>
<connect gate="G$1" pin="TOUT" pad="7"/>
<connect gate="G$1" pin="TXEN" pad="11"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VL" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TSSOP" package="TSSOP16">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="RIN" pad="8"/>
<connect gate="G$1" pin="ROUT" pad="9"/>
<connect gate="G$1" pin="RXEN" pad="12"/>
<connect gate="G$1" pin="SHDN" pad="14"/>
<connect gate="G$1" pin="TIN" pad="10"/>
<connect gate="G$1" pin="TOUT" pad="7"/>
<connect gate="G$1" pin="TXEN" pad="11"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VL" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3378" prefix="IC">
<description>voltage level translator</description>
<gates>
<gate name="G$1" symbol="MAX3378"/>
</gates>
<devices>
<device name="" package="TSSOP14">
<connects>
<connect gate="G$1" pin="/TRI" pad="8"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="V3.3" pad="1"/>
<connect gate="G$1" pin="VC1" pad="13"/>
<connect gate="G$1" pin="VC2" pad="12"/>
<connect gate="G$1" pin="VC3" pad="11"/>
<connect gate="G$1" pin="VC4" pad="10"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VL1" pad="2"/>
<connect gate="G$1" pin="VL2" pad="3"/>
<connect gate="G$1" pin="VL3" pad="4"/>
<connect gate="G$1" pin="VL4" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIL-10X2-.05">
<gates>
<gate name="G$1" symbol="DIL-10X2-.05"/>
</gates>
<devices>
<device name="" package="DIX-10X2-.05">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$17" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DC-IN" prefix="P">
<gates>
<gate name="G$1" symbol="DC-POWERJACK"/>
</gates>
<devices>
<device name="" package="DC-POWERJACK">
<connects>
<connect gate="G$1" pin="+V" pad="+V"/>
<connect gate="G$1" pin="P$2" pad="G2"/>
<connect gate="G$1" pin="P$3" pad="G3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1.3MM" package="DC-IN-1.3MM">
<connects>
<connect gate="G$1" pin="+V" pad="+V"/>
<connect gate="G$1" pin="P$2" pad="G1"/>
<connect gate="G$1" pin="P$3" pad="G2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SFM2X10">
<gates>
<gate name="G$1" symbol="DIL-10X2-.05"/>
</gates>
<devices>
<device name="" package="SFM2X10">
<connects>
<connect gate="G$1" pin="P$1" pad="P20"/>
<connect gate="G$1" pin="P$10" pad="P11"/>
<connect gate="G$1" pin="P$11" pad="P10"/>
<connect gate="G$1" pin="P$12" pad="P9"/>
<connect gate="G$1" pin="P$13" pad="P8"/>
<connect gate="G$1" pin="P$14" pad="P7"/>
<connect gate="G$1" pin="P$15" pad="P6"/>
<connect gate="G$1" pin="P$16" pad="P5"/>
<connect gate="G$1" pin="P$17" pad="P4"/>
<connect gate="G$1" pin="P$18" pad="P3"/>
<connect gate="G$1" pin="P$19" pad="P2"/>
<connect gate="G$1" pin="P$2" pad="P19"/>
<connect gate="G$1" pin="P$20" pad="P1"/>
<connect gate="G$1" pin="P$3" pad="P18"/>
<connect gate="G$1" pin="P$4" pad="P17"/>
<connect gate="G$1" pin="P$5" pad="P16"/>
<connect gate="G$1" pin="P$6" pad="P15"/>
<connect gate="G$1" pin="P$7" pad="P14"/>
<connect gate="G$1" pin="P$8" pad="P13"/>
<connect gate="G$1" pin="P$9" pad="P12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937ET*" prefix="IC">
<description>&lt;font color="red"&gt;&lt;h2&gt;
400 and 500 mA Low Dropout Voltage Regulator
	&lt;/h2&gt;&lt;/font&gt;&lt;font color="blue"&gt;&lt;h1&gt;
NATIONAL SEMICONDUCTOR
	&lt;/h1&gt;&lt;hr&gt;&lt;/font&gt;&lt;p&gt;&lt;author&gt;created by &lt;a href="mailto:Reter.Hofmann@ph-tronic.de"&gt;Peter.Hofmann@ph-tronic.de&lt;/a&gt;&lt;/author&gt; &lt;p&gt;  
10-2004 Rev.0
	&lt;hr&gt;</description>
<gates>
<gate name="G$1" symbol="LM2937-3.3"/>
</gates>
<devices>
<device name="" package="TO220(V)">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="-10"/>
<technology name="-12"/>
<technology name="-15"/>
<technology name="-2.5"/>
<technology name="-3.3"/>
<technology name="-5.0"/>
<technology name="-8.0"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="78*" prefix="IC">
<description>Positive &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="A1" symbol="78XX"/>
</gates>
<devices>
<device name="Z" package="TO92">
<connects>
<connect gate="A1" pin="GND" pad="2"/>
<connect gate="A1" pin="V5.0" pad="1"/>
<connect gate="A1" pin="VI" pad="3"/>
</connects>
<technologies>
<technology name="L05"/>
<technology name="L08"/>
<technology name="L12"/>
<technology name="L15"/>
<technology name="L18"/>
<technology name="L24"/>
</technologies>
</device>
<device name="T" package="TO220H">
<connects>
<connect gate="A1" pin="GND" pad="2"/>
<connect gate="A1" pin="V5.0" pad="3"/>
<connect gate="A1" pin="VI" pad="1"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="06"/>
<technology name="08"/>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="24"/>
</technologies>
</device>
<device name="H" package="TO39">
<connects>
<connect gate="A1" pin="GND" pad="3"/>
<connect gate="A1" pin="V5.0" pad="2"/>
<connect gate="A1" pin="VI" pad="1"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="06"/>
<technology name="08"/>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="24"/>
</technologies>
</device>
<device name="L" package="TO92">
<connects>
<connect gate="A1" pin="GND" pad="2"/>
<connect gate="A1" pin="V5.0" pad="1"/>
<connect gate="A1" pin="VI" pad="3"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="06"/>
<technology name="08"/>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="24"/>
</technologies>
</device>
<device name="DT" package="TO252">
<connects>
<connect gate="A1" pin="GND" pad="3"/>
<connect gate="A1" pin="V5.0" pad="2"/>
<connect gate="A1" pin="VI" pad="1"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="06"/>
<technology name="08"/>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="24"/>
</technologies>
</device>
<device name="" package="TO220(V)">
<connects>
<connect gate="A1" pin="GND" pad="2"/>
<connect gate="A1" pin="V5.0" pad="3"/>
<connect gate="A1" pin="VI" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DPAK" package="DPAK">
<connects>
<connect gate="A1" pin="GND" pad="2"/>
<connect gate="A1" pin="V5.0" pad="3"/>
<connect gate="A1" pin="VI" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="18F4620" prefix="IC">
<description>&lt;B&gt;MICROCONTROLLER&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="18F4620"/>
</gates>
<devices>
<device name="L" package="PLCC-44">
<technologies>
<technology name="4"/>
<technology name="7"/>
</technologies>
</device>
<device name="PQ" package="MQFP44-2">
<connects>
<connect gate="G$1" pin="MCLR#" pad="18"/>
<connect gate="G$1" pin="RA0/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2" pad="21"/>
<connect gate="G$1" pin="RA3/AN3" pad="22"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="23"/>
<connect gate="G$1" pin="RA5/AN4" pad="24"/>
<connect gate="G$1" pin="RA6/OX2" pad="31"/>
<connect gate="G$1" pin="RA7/OX1" pad="30"/>
<connect gate="G$1" pin="RB0" pad="8"/>
<connect gate="G$1" pin="RB1" pad="9"/>
<connect gate="G$1" pin="RB2" pad="10"/>
<connect gate="G$1" pin="RB3/PGM" pad="11"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RB6/PGC" pad="16"/>
<connect gate="G$1" pin="RB7/PGD" pad="17"/>
<connect gate="G$1" pin="RC0" pad="32"/>
<connect gate="G$1" pin="RC1" pad="35"/>
<connect gate="G$1" pin="RC2" pad="36"/>
<connect gate="G$1" pin="RC3/SCK" pad="37"/>
<connect gate="G$1" pin="RC4/MISO" pad="42"/>
<connect gate="G$1" pin="RC5/MOSI" pad="43"/>
<connect gate="G$1" pin="RC6/TX" pad="44"/>
<connect gate="G$1" pin="RC7/RX" pad="1"/>
<connect gate="G$1" pin="RD0" pad="38"/>
<connect gate="G$1" pin="RD1" pad="39"/>
<connect gate="G$1" pin="RD2" pad="40"/>
<connect gate="G$1" pin="RD3" pad="41"/>
<connect gate="G$1" pin="RD4" pad="2"/>
<connect gate="G$1" pin="RD5" pad="3"/>
<connect gate="G$1" pin="RD6" pad="4"/>
<connect gate="G$1" pin="RD7" pad="5"/>
<connect gate="G$1" pin="RE0/AN5" pad="25"/>
<connect gate="G$1" pin="RE1/AN6" pad="26"/>
<connect gate="G$1" pin="RE2/AN7" pad="27"/>
<connect gate="G$1" pin="VDD@1" pad="7"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
<connect gate="G$1" pin="VSS@2" pad="29"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="7"/>
</technologies>
</device>
<device name="PT" package="TQFP44">
<connects>
<connect gate="G$1" pin="MCLR#" pad="18"/>
<connect gate="G$1" pin="RA0/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2" pad="21"/>
<connect gate="G$1" pin="RA3/AN3" pad="22"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="23"/>
<connect gate="G$1" pin="RA5/AN4" pad="24"/>
<connect gate="G$1" pin="RA6/OX2" pad="31"/>
<connect gate="G$1" pin="RA7/OX1" pad="30"/>
<connect gate="G$1" pin="RB0" pad="8"/>
<connect gate="G$1" pin="RB1" pad="9"/>
<connect gate="G$1" pin="RB2" pad="10"/>
<connect gate="G$1" pin="RB3/PGM" pad="11"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RB6/PGC" pad="16"/>
<connect gate="G$1" pin="RB7/PGD" pad="17"/>
<connect gate="G$1" pin="RC0" pad="32"/>
<connect gate="G$1" pin="RC1" pad="35"/>
<connect gate="G$1" pin="RC2" pad="36"/>
<connect gate="G$1" pin="RC3/SCK" pad="37"/>
<connect gate="G$1" pin="RC4/MISO" pad="42"/>
<connect gate="G$1" pin="RC5/MOSI" pad="43"/>
<connect gate="G$1" pin="RC6/TX" pad="44"/>
<connect gate="G$1" pin="RC7/RX" pad="1"/>
<connect gate="G$1" pin="RD0" pad="38"/>
<connect gate="G$1" pin="RD1" pad="39"/>
<connect gate="G$1" pin="RD2" pad="40"/>
<connect gate="G$1" pin="RD3" pad="41"/>
<connect gate="G$1" pin="RD4" pad="2"/>
<connect gate="G$1" pin="RD5" pad="3"/>
<connect gate="G$1" pin="RD6" pad="4"/>
<connect gate="G$1" pin="RD7" pad="5"/>
<connect gate="G$1" pin="RE0/AN5" pad="25"/>
<connect gate="G$1" pin="RE1/AN6" pad="26"/>
<connect gate="G$1" pin="RE2/AN7" pad="27"/>
<connect gate="G$1" pin="VDD@1" pad="7"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
<connect gate="G$1" pin="VSS@2" pad="29"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="7"/>
</technologies>
</device>
<device name="P" package="DIL40">
<connects>
<connect gate="G$1" pin="MCLR#" pad="1"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RA6/OX2" pad="14"/>
<connect gate="G$1" pin="RA7/OX1" pad="13"/>
<connect gate="G$1" pin="RB0" pad="33"/>
<connect gate="G$1" pin="RB1" pad="34"/>
<connect gate="G$1" pin="RB2" pad="35"/>
<connect gate="G$1" pin="RB3/PGM" pad="36"/>
<connect gate="G$1" pin="RB4" pad="37"/>
<connect gate="G$1" pin="RB5" pad="38"/>
<connect gate="G$1" pin="RB6/PGC" pad="39"/>
<connect gate="G$1" pin="RB7/PGD" pad="40"/>
<connect gate="G$1" pin="RC0" pad="15"/>
<connect gate="G$1" pin="RC1" pad="16"/>
<connect gate="G$1" pin="RC2" pad="17"/>
<connect gate="G$1" pin="RC3/SCK" pad="18"/>
<connect gate="G$1" pin="RC4/MISO" pad="23"/>
<connect gate="G$1" pin="RC5/MOSI" pad="24"/>
<connect gate="G$1" pin="RC6/TX" pad="25"/>
<connect gate="G$1" pin="RC7/RX" pad="26"/>
<connect gate="G$1" pin="RD0" pad="19"/>
<connect gate="G$1" pin="RD1" pad="20"/>
<connect gate="G$1" pin="RD2" pad="21"/>
<connect gate="G$1" pin="RD3" pad="22"/>
<connect gate="G$1" pin="RD4" pad="27"/>
<connect gate="G$1" pin="RD5" pad="28"/>
<connect gate="G$1" pin="RD6" pad="29"/>
<connect gate="G$1" pin="RD7" pad="30"/>
<connect gate="G$1" pin="RE0/AN5" pad="8"/>
<connect gate="G$1" pin="RE1/AN6" pad="9"/>
<connect gate="G$1" pin="RE2/AN7" pad="10"/>
<connect gate="G$1" pin="VDD@1" pad="11"/>
<connect gate="G$1" pin="VDD@2" pad="32"/>
<connect gate="G$1" pin="VSS@1" pad="12"/>
<connect gate="G$1" pin="VSS@2" pad="31"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="7"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JP2W" prefix="JP" uservalue="yes">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="JP3E"/>
</gates>
<devices>
<device name="" package="JP2W">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="3" pad="3"/>
<connect gate="1" pin="VDD" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X10" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X10"/>
</gates>
<devices>
<device name="" package="2X10">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC-1265" prefix="IC">
<gates>
<gate name="G$1" symbol="TC-1265"/>
</gates>
<devices>
<device name="" package="TO220H">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="V3.3" pad="3"/>
<connect gate="G$1" pin="VI" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V3.3">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="+3V3"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="10-XX" prefix="S" uservalue="yes">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="TS2"/>
</gates>
<devices>
<device name="" package="B3F-10XX">
<connects>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="P1" pad="4"/>
<connect gate="1" pin="S" pad="1"/>
<connect gate="1" pin="S1" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V5.0" prefix="V">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="V5.0" symbol="+05V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="24-*" prefix="IC">
<description>Serial &lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
32 K/64 K, 1.8 V, I2C</description>
<gates>
<gate name="G$1" symbol="24AA32"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA65"/>
<technology name="C32"/>
<technology name="C65"/>
<technology name="FC32"/>
<technology name="FC65"/>
<technology name="LC32"/>
<technology name="LC65"/>
</technologies>
</device>
<device name="SM" package="SO-08M">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA65"/>
<technology name="C32"/>
<technology name="C65"/>
<technology name="FC32"/>
<technology name="FC65"/>
<technology name="LC32"/>
<technology name="LC65"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="25*" prefix="IC">
<description>Serial &lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
4 K, SPI bus</description>
<gates>
<gate name="G$1" symbol="25SERIAL"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="!CS" pad="1"/>
<connect gate="G$1" pin="!HOLD" pad="7"/>
<connect gate="G$1" pin="!WP" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SI" pad="5"/>
<connect gate="G$1" pin="SO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA040"/>
<technology name="AA080"/>
<technology name="C040"/>
<technology name="C080"/>
<technology name="LC040"/>
<technology name="LC080"/>
</technologies>
</device>
<device name="ST" package="TSSOP8">
<connects>
<connect gate="G$1" pin="!CS" pad="1"/>
<connect gate="G$1" pin="!HOLD" pad="7"/>
<connect gate="G$1" pin="!WP" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SI" pad="5"/>
<connect gate="G$1" pin="SO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA040"/>
<technology name="C040"/>
<technology name="LC040"/>
</technologies>
</device>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="!CS" pad="1"/>
<connect gate="G$1" pin="!HOLD" pad="7"/>
<connect gate="G$1" pin="!WP" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SI" pad="5"/>
<connect gate="G$1" pin="SO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="AA080"/>
<technology name="C080"/>
<technology name="LC080"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="24FC515" prefix="IC">
<gates>
<gate name="G$1" symbol="24FC515"/>
</gates>
<devices>
<device name="" package="DIL8">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="24FC512" prefix="IC">
<description>I2C serial EPROM Microchip</description>
<gates>
<gate name="G$1" symbol="24FC512"/>
</gates>
<devices>
<device name="" package="DIL8">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SM" package="SO-08M">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SN" package="SO08">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="25LC640" prefix="IC">
<description>SPI serial EPROM microchip</description>
<gates>
<gate name="G$1" symbol="25LC640"/>
</gates>
<devices>
<device name="" package="DIL8">
<connects>
<connect gate="G$1" pin="CS/" pad="1"/>
<connect gate="G$1" pin="HD/" pad="7"/>
<connect gate="G$1" pin="SCLK" pad="6"/>
<connect gate="G$1" pin="SI" pad="5"/>
<connect gate="G$1" pin="SO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="WP/" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SM" package="SO-08M">
<connects>
<connect gate="G$1" pin="CS/" pad="1"/>
<connect gate="G$1" pin="HD/" pad="7"/>
<connect gate="G$1" pin="SCLK" pad="6"/>
<connect gate="G$1" pin="SI" pad="5"/>
<connect gate="G$1" pin="SO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="WP/" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS1337" prefix="IC">
<gates>
<gate name="G$1" symbol="DS1337"/>
</gates>
<devices>
<device name="" package="DIL8">
<connects>
<connect gate="G$1" pin="INTA" pad="3"/>
<connect gate="G$1" pin="INTB" pad="7"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1086CT-5" prefix="IC">
<description>1.5 A LDO regulator</description>
<gates>
<gate name="G$1" symbol="LM1086CT-5"/>
</gates>
<devices>
<device name="" package="TO220(V)">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="V5.0" pad="2"/>
<connect gate="G$1" pin="VI" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117*" prefix="IC">
<description>800 mA LDO regulator</description>
<gates>
<gate name="G$1" symbol="LM1086CT-5"/>
</gates>
<devices>
<device name="" package="TO220(V)">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="V5.0" pad="2"/>
<connect gate="G$1" pin="VI" pad="3"/>
</connects>
<technologies>
<technology name=""/>
<technology name="-3.3"/>
<technology name="-5,0"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937-5.0" prefix="IC">
<gates>
<gate name="G$1" symbol="LM2937-5.0"/>
</gates>
<devices>
<device name="" package="TO220(V)">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937-3.3" prefix="IC">
<gates>
<gate name="G$1" symbol="LM2937-3.3"/>
</gates>
<devices>
<device name="ET" package="TO220(V)">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IMP" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH">
<gates>
<gate name="G$1" symbol="E320PBSWITCH"/>
</gates>
<devices>
<device name="" package="PBSWITCH">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DT" prefix="S">
<description>&lt;b&gt;ITT SWITCH&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="TS2-1"/>
</gates>
<devices>
<device name="6" package="DT6">
<connects>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="P@1" pad="4"/>
<connect gate="1" pin="S" pad="1"/>
<connect gate="1" pin="S@1" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E6" package="DTE6">
<connects>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="P@1" pad="4"/>
<connect gate="1" pin="S" pad="1"/>
<connect gate="1" pin="S@1" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E6K" package="DTE6K">
<connects>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="P@1" pad="4"/>
<connect gate="1" pin="S" pad="1"/>
<connect gate="1" pin="S@1" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="PBSWITCH">
<connects>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="P@1" pad="4"/>
<connect gate="1" pin="S" pad="1"/>
<connect gate="1" pin="S@1" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1N4729" prefix="D">
<description>&lt;b&gt;Z DIODE&lt;/b&gt;&lt;p&gt;
3.3 V, 1W, 5 percent</description>
<gates>
<gate name="1" symbol="ZD"/>
</gates>
<devices>
<device name="" package="DO41Z10">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1N749A">
<gates>
<gate name="G$1" symbol="ZD"/>
</gates>
<devices>
<device name="" package="DO41Z10">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED10" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="LED10"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="X" package="LED10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIL20" prefix="IC" uservalue="yes">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DIL20"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SOCKED-20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X12" prefix="JP" uservalue="yes">
<gates>
<gate name="G$1" symbol="PINH2X12"/>
</gates>
<devices>
<device name="" package="2X12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="23"/>
<connect gate="G$1" pin="23" pad="22"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CC2420" prefix="IC">
<description>ZigBee Transciever</description>
<gates>
<gate name="G$1" symbol="CC2420"/>
</gates>
<devices>
<device name="" package="SQFP-S-7X7-48">
<connects>
<connect gate="G$1" pin="ATEST1" pad="47"/>
<connect gate="G$1" pin="ATEST2" pad="46"/>
<connect gate="G$1" pin="AVDD_IF1" pad="44"/>
<connect gate="G$1" pin="AV_ADC" pad="17"/>
<connect gate="G$1" pin="AV_CHP" pad="48"/>
<connect gate="G$1" pin="AV_IF2" pad="15"/>
<connect gate="G$1" pin="AV_PRE" pad="3"/>
<connect gate="G$1" pin="AV_RF1" pad="4"/>
<connect gate="G$1" pin="AV_RF2" pad="14"/>
<connect gate="G$1" pin="AV_SW" pad="10"/>
<connect gate="G$1" pin="AV_VCO" pad="2"/>
<connect gate="G$1" pin="AV_X16" pad="37"/>
<connect gate="G$1" pin="CCA" pad="28"/>
<connect gate="G$1" pin="CSN" pad="31"/>
<connect gate="G$1" pin="DGND" pad="22"/>
<connect gate="G$1" pin="DGND_GRD" pad="19"/>
<connect gate="G$1" pin="DGUARD" pad="20"/>
<connect gate="G$1" pin="DSUB_C" pad="24"/>
<connect gate="G$1" pin="DSUB_P" pad="23"/>
<connect gate="G$1" pin="DV1.8" pad="26"/>
<connect gate="G$1" pin="DV3.3" pad="25"/>
<connect gate="G$1" pin="DV_ADC" pad="18"/>
<connect gate="G$1" pin="DV_RAM" pad="35"/>
<connect gate="G$1" pin="FIFO" pad="30"/>
<connect gate="G$1" pin="FIFOP" pad="29"/>
<connect gate="G$1" pin="GND@1" pad="5"/>
<connect gate="G$1" pin="GND@2" pad="9"/>
<connect gate="G$1" pin="P$11" pad="40"/>
<connect gate="G$1" pin="P$12" pad="36"/>
<connect gate="G$1" pin="P$13" pad="16"/>
<connect gate="G$1" pin="P$16" pad="13"/>
<connect gate="G$1" pin="P$36" pad="12"/>
<connect gate="G$1" pin="P$40" pad="11"/>
<connect gate="G$1" pin="RESETN" pad="21"/>
<connect gate="G$1" pin="RF_N" pad="8"/>
<connect gate="G$1" pin="RF_P" pad="6"/>
<connect gate="G$1" pin="R_BIAS" pad="45"/>
<connect gate="G$1" pin="SCLK" pad="32"/>
<connect gate="G$1" pin="SFD" pad="27"/>
<connect gate="G$1" pin="SI" pad="33"/>
<connect gate="G$1" pin="SO" pad="34"/>
<connect gate="G$1" pin="TXRX_SW" pad="7"/>
<connect gate="G$1" pin="VCO_GRD" pad="1"/>
<connect gate="G$1" pin="VREG_EN" pad="41"/>
<connect gate="G$1" pin="VREG_IN" pad="43"/>
<connect gate="G$1" pin="VREG_OUT" pad="42"/>
<connect gate="G$1" pin="XOSCQ2" pad="38"/>
<connect gate="G$1" pin="XOSC_Q1" pad="39"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="F09HP" prefix="X" uservalue="yes">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="F09G"/>
</gates>
<devices>
<device name="" package="F09HP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="G1" pad="G1"/>
<connect gate="G$1" pin="G2" pad="G2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX-ZIG" prefix="IC">
<gates>
<gate name="1" symbol="ZIG-MOD"/>
</gates>
<devices>
<device name="" package="XBEE-MOD">
<connects>
<connect gate="1" pin="CTS/" pad="12"/>
<connect gate="1" pin="D04" pad="11"/>
<connect gate="1" pin="D08" pad="4"/>
<connect gate="1" pin="DIN" pad="3"/>
<connect gate="1" pin="DIO0" pad="20"/>
<connect gate="1" pin="DIO1" pad="19"/>
<connect gate="1" pin="DIO2" pad="18"/>
<connect gate="1" pin="DIO3" pad="17"/>
<connect gate="1" pin="DIO5" pad="15"/>
<connect gate="1" pin="DOUT" pad="2"/>
<connect gate="1" pin="DTR/" pad="9"/>
<connect gate="1" pin="GND" pad="10"/>
<connect gate="1" pin="ON" pad="13"/>
<connect gate="1" pin="P$7" pad="7"/>
<connect gate="1" pin="P$8" pad="8"/>
<connect gate="1" pin="RSET" pad="5"/>
<connect gate="1" pin="RSSI" pad="6"/>
<connect gate="1" pin="RTS/" pad="16"/>
<connect gate="1" pin="V3.3" pad="1"/>
<connect gate="1" pin="VREF" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3111" prefix="IC">
<gates>
<gate name="MAX3111" symbol="MAX311X"/>
</gates>
<devices>
<device name="DIP" package="DIL28-3">
<connects>
<connect gate="MAX3111" pin="C1+" pad="22"/>
<connect gate="MAX3111" pin="C1-" pad="23"/>
<connect gate="MAX3111" pin="C2+" pad="24"/>
<connect gate="MAX3111" pin="C2-" pad="25"/>
<connect gate="MAX3111" pin="CS/" pad="18"/>
<connect gate="MAX3111" pin="CTS/" pad="11"/>
<connect gate="MAX3111" pin="DIN" pad="15"/>
<connect gate="MAX3111" pin="DOUT" pad="16"/>
<connect gate="MAX3111" pin="GND" pad="27"/>
<connect gate="MAX3111" pin="IRQ/" pad="19"/>
<connect gate="MAX3111" pin="R1IN" pad="6"/>
<connect gate="MAX3111" pin="R1OUT" pad="5"/>
<connect gate="MAX3111" pin="R20UT" pad="2"/>
<connect gate="MAX3111" pin="R2IN" pad="1"/>
<connect gate="MAX3111" pin="RTS/" pad="12"/>
<connect gate="MAX3111" pin="RX" pad="13"/>
<connect gate="MAX3111" pin="SCLK" pad="17"/>
<connect gate="MAX3111" pin="SHDN/" pad="20"/>
<connect gate="MAX3111" pin="T1IN" pad="4"/>
<connect gate="MAX3111" pin="T1OUT" pad="7"/>
<connect gate="MAX3111" pin="T2IN" pad="3"/>
<connect gate="MAX3111" pin="T2OUT" pad="28"/>
<connect gate="MAX3111" pin="TX" pad="14"/>
<connect gate="MAX3111" pin="V+" pad="21"/>
<connect gate="MAX3111" pin="V-" pad="26"/>
<connect gate="MAX3111" pin="VDD" pad="8"/>
<connect gate="MAX3111" pin="X1" pad="10"/>
<connect gate="MAX3111" pin="X2" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SO-WIDE" package="SOIC-.3-28">
<connects>
<connect gate="MAX3111" pin="C1+" pad="22"/>
<connect gate="MAX3111" pin="C1-" pad="23"/>
<connect gate="MAX3111" pin="C2+" pad="24"/>
<connect gate="MAX3111" pin="C2-" pad="25"/>
<connect gate="MAX3111" pin="CS/" pad="18"/>
<connect gate="MAX3111" pin="CTS/" pad="11"/>
<connect gate="MAX3111" pin="DIN" pad="15"/>
<connect gate="MAX3111" pin="DOUT" pad="16"/>
<connect gate="MAX3111" pin="GND" pad="27"/>
<connect gate="MAX3111" pin="IRQ/" pad="19"/>
<connect gate="MAX3111" pin="R1IN" pad="6"/>
<connect gate="MAX3111" pin="R1OUT" pad="5"/>
<connect gate="MAX3111" pin="R20UT" pad="2"/>
<connect gate="MAX3111" pin="R2IN" pad="1"/>
<connect gate="MAX3111" pin="RTS/" pad="12"/>
<connect gate="MAX3111" pin="RX" pad="13"/>
<connect gate="MAX3111" pin="SCLK" pad="17"/>
<connect gate="MAX3111" pin="SHDN/" pad="20"/>
<connect gate="MAX3111" pin="T1IN" pad="4"/>
<connect gate="MAX3111" pin="T1OUT" pad="7"/>
<connect gate="MAX3111" pin="T2IN" pad="3"/>
<connect gate="MAX3111" pin="T2OUT" pad="28"/>
<connect gate="MAX3111" pin="TX" pad="14"/>
<connect gate="MAX3111" pin="V+" pad="21"/>
<connect gate="MAX3111" pin="V-" pad="26"/>
<connect gate="MAX3111" pin="VDD" pad="8"/>
<connect gate="MAX3111" pin="X1" pad="10"/>
<connect gate="MAX3111" pin="X2" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DC-DC-CONV">
<gates>
<gate name="G$1" symbol="DC-DC-CONV"/>
</gates>
<devices>
<device name="SOT" package="SOT23-5L">
<connects>
<connect gate="G$1" pin="C+" pad="4"/>
<connect gate="G$1" pin="C-" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3110" prefix="IC">
<gates>
<gate name="G$1" symbol="MAX311X"/>
</gates>
<devices>
<device name="SOIC" package="SOIC-.3-28">
<connects>
<connect gate="G$1" pin="C1+" pad="22"/>
<connect gate="G$1" pin="C1-" pad="23"/>
<connect gate="G$1" pin="C2+" pad="24"/>
<connect gate="G$1" pin="C2-" pad="25"/>
<connect gate="G$1" pin="CS/" pad="18"/>
<connect gate="G$1" pin="CTS/" pad="11"/>
<connect gate="G$1" pin="DIN" pad="15"/>
<connect gate="G$1" pin="DOUT" pad="16"/>
<connect gate="G$1" pin="GND" pad="27"/>
<connect gate="G$1" pin="IRQ/" pad="19"/>
<connect gate="G$1" pin="R1IN" pad="6"/>
<connect gate="G$1" pin="R1OUT" pad="5"/>
<connect gate="G$1" pin="R20UT" pad="2"/>
<connect gate="G$1" pin="R2IN" pad="1"/>
<connect gate="G$1" pin="RTS/" pad="12"/>
<connect gate="G$1" pin="RX" pad="13"/>
<connect gate="G$1" pin="SCLK" pad="17"/>
<connect gate="G$1" pin="SHDN/" pad="20"/>
<connect gate="G$1" pin="T1IN" pad="4"/>
<connect gate="G$1" pin="T1OUT" pad="7"/>
<connect gate="G$1" pin="T2IN" pad="3"/>
<connect gate="G$1" pin="T2OUT" pad="28"/>
<connect gate="G$1" pin="TX" pad="14"/>
<connect gate="G$1" pin="V+" pad="21"/>
<connect gate="G$1" pin="V-" pad="26"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="X1" pad="10"/>
<connect gate="G$1" pin="X2" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DIP" package="DIL28-3">
<connects>
<connect gate="G$1" pin="C1+" pad="22"/>
<connect gate="G$1" pin="C1-" pad="23"/>
<connect gate="G$1" pin="C2+" pad="24"/>
<connect gate="G$1" pin="C2-" pad="25"/>
<connect gate="G$1" pin="CS/" pad="18"/>
<connect gate="G$1" pin="CTS/" pad="11"/>
<connect gate="G$1" pin="DIN" pad="15"/>
<connect gate="G$1" pin="DOUT" pad="16"/>
<connect gate="G$1" pin="GND" pad="27"/>
<connect gate="G$1" pin="IRQ/" pad="19"/>
<connect gate="G$1" pin="R1IN" pad="6"/>
<connect gate="G$1" pin="R1OUT" pad="5"/>
<connect gate="G$1" pin="R20UT" pad="2"/>
<connect gate="G$1" pin="R2IN" pad="1"/>
<connect gate="G$1" pin="RTS/" pad="12"/>
<connect gate="G$1" pin="RX" pad="13"/>
<connect gate="G$1" pin="SCLK" pad="17"/>
<connect gate="G$1" pin="SHDN/" pad="20"/>
<connect gate="G$1" pin="T1IN" pad="4"/>
<connect gate="G$1" pin="T1OUT" pad="7"/>
<connect gate="G$1" pin="T2IN" pad="3"/>
<connect gate="G$1" pin="T2OUT" pad="28"/>
<connect gate="G$1" pin="TX" pad="14"/>
<connect gate="G$1" pin="V+" pad="21"/>
<connect gate="G$1" pin="V-" pad="26"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="X1" pad="10"/>
<connect gate="G$1" pin="X2" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X5" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X5"/>
</gates>
<devices>
<device name="" package="2X05">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-DISP">
<gates>
<gate name="G$1" symbol="LEDDSP"/>
</gates>
<devices>
<device name="" package="LEDDISP">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="B" pad="14"/>
<connect gate="G$1" pin="C" pad="12"/>
<connect gate="G$1" pin="CC1" pad="3"/>
<connect gate="G$1" pin="CC2" pad="5"/>
<connect gate="G$1" pin="CC3" pad="11"/>
<connect gate="G$1" pin="CC4" pad="16"/>
<connect gate="G$1" pin="D" pad="10"/>
<connect gate="G$1" pin="E" pad="4"/>
<connect gate="G$1" pin="F" pad="2"/>
<connect gate="G$1" pin="G" pad="13"/>
<connect gate="G$1" pin="LDP" pad="6"/>
<connect gate="G$1" pin="RDP" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX7221" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="MAX7221"/>
</gates>
<devices>
<device name="DIL" package="DIL24-3">
<connects>
<connect gate="G$1" pin="!CS" pad="12"/>
<connect gate="G$1" pin="CLK" pad="13"/>
<connect gate="G$1" pin="DIG0" pad="2"/>
<connect gate="G$1" pin="DIG1" pad="11"/>
<connect gate="G$1" pin="DIG2" pad="6"/>
<connect gate="G$1" pin="DIG3" pad="7"/>
<connect gate="G$1" pin="DIG4" pad="3"/>
<connect gate="G$1" pin="DIG5" pad="10"/>
<connect gate="G$1" pin="DIG6" pad="5"/>
<connect gate="G$1" pin="DIG7" pad="8"/>
<connect gate="G$1" pin="DIN" pad="1"/>
<connect gate="G$1" pin="DOUT" pad="24"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="9"/>
<connect gate="G$1" pin="ISET" pad="18"/>
<connect gate="G$1" pin="SEGA" pad="14"/>
<connect gate="G$1" pin="SEGB" pad="16"/>
<connect gate="G$1" pin="SEGC" pad="20"/>
<connect gate="G$1" pin="SEGD" pad="23"/>
<connect gate="G$1" pin="SEGDP" pad="22"/>
<connect gate="G$1" pin="SEGE" pad="21"/>
<connect gate="G$1" pin="SEGF" pad="15"/>
<connect gate="G$1" pin="SEGG" pad="17"/>
<connect gate="G$1" pin="VDD" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOIC" package="SO24W">
<connects>
<connect gate="G$1" pin="!CS" pad="12"/>
<connect gate="G$1" pin="CLK" pad="13"/>
<connect gate="G$1" pin="DIG0" pad="2"/>
<connect gate="G$1" pin="DIG1" pad="11"/>
<connect gate="G$1" pin="DIG2" pad="6"/>
<connect gate="G$1" pin="DIG3" pad="7"/>
<connect gate="G$1" pin="DIG4" pad="3"/>
<connect gate="G$1" pin="DIG5" pad="10"/>
<connect gate="G$1" pin="DIG6" pad="5"/>
<connect gate="G$1" pin="DIG7" pad="8"/>
<connect gate="G$1" pin="DIN" pad="1"/>
<connect gate="G$1" pin="DOUT" pad="24"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="9"/>
<connect gate="G$1" pin="ISET" pad="18"/>
<connect gate="G$1" pin="SEGA" pad="14"/>
<connect gate="G$1" pin="SEGB" pad="16"/>
<connect gate="G$1" pin="SEGC" pad="20"/>
<connect gate="G$1" pin="SEGD" pad="23"/>
<connect gate="G$1" pin="SEGDP" pad="22"/>
<connect gate="G$1" pin="SEGE" pad="21"/>
<connect gate="G$1" pin="SEGF" pad="15"/>
<connect gate="G$1" pin="SEGG" pad="17"/>
<connect gate="G$1" pin="VDD" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MODULAR-6" prefix="J" uservalue="yes">
<description>&lt;b&gt;AMP connector&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="JACK6"/>
</gates>
<devices>
<device name="" package="MODULAR-6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2N2222" prefix="T">
<description>&lt;b&gt;NPN TRANSISTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="TO18">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92" package="TO92-CBE">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X2S" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD2"/>
</gates>
<devices>
<device name="" package="1X02N">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD3"/>
</gates>
<devices>
<device name="" package="1X03N">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X4" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD4"/>
</gates>
<devices>
<device name="" package="1X04N">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X5" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD5"/>
</gates>
<devices>
<device name="" package="1X05N">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X10" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD10"/>
</gates>
<devices>
<device name="" package="1X10N">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X6" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD6"/>
</gates>
<devices>
<device name="" package="1X06N">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X9" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD9"/>
</gates>
<devices>
<device name="" package="1X09N">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="E4R" prefix="RN" uservalue="yes">
<description>&lt;b&gt;SIL RESISTOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="RNV"/>
<gate name="B" symbol="RNV"/>
<gate name="C" symbol="RNV"/>
<gate name="D" symbol="RNV"/>
</gates>
<devices>
<device name="" package="SIL8">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="B" pin="1" pad="3"/>
<connect gate="B" pin="2" pad="4"/>
<connect gate="C" pin="1" pad="5"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="7"/>
<connect gate="D" pin="2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G09R" prefix="RN" uservalue="yes">
<description>&lt;b&gt;SIL RESISTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="R9"/>
</gates>
<devices>
<device name="" package="SIL10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X8" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD8"/>
</gates>
<devices>
<device name="" package="1X08">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X3"/>
</gates>
<devices>
<device name="" package="2X03">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X4" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X4"/>
</gates>
<devices>
<device name="" package="2X04">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-DISP-3IN" prefix="LED-">
<gates>
<gate name="G$1" symbol="LEDDISPLRG"/>
</gates>
<devices>
<device name="" package="LEDDISPLRGPKG">
<connects>
<connect gate="G$1" pin="A" pad="7"/>
<connect gate="G$1" pin="B" pad="6"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="CC1" pad="1"/>
<connect gate="G$1" pin="CC2" pad="8"/>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="DP" pad="5"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="F" pad="9"/>
<connect gate="G$1" pin="G" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="E-320.01" prefix="SW" uservalue="yes">
<description>&lt;b&gt;SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="E320PBSWITCH"/>
</gates>
<devices>
<device name="" package="E-320">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADAPTER-28-SOIC">
<gates>
<gate name="G$1" symbol="ADAPTER-28"/>
</gates>
<devices>
<device name="" package="SOIC-ADAPT">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$17" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$21" pad="21"/>
<connect gate="G$1" pin="P$22" pad="22"/>
<connect gate="G$1" pin="P$23" pad="23"/>
<connect gate="G$1" pin="P$24" pad="24"/>
<connect gate="G$1" pin="P$25" pad="25"/>
<connect gate="G$1" pin="P$26" pad="26"/>
<connect gate="G$1" pin="P$27" pad="27"/>
<connect gate="G$1" pin="P$28" pad="28"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X14" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD14"/>
</gates>
<devices>
<device name="" package="1X14">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BRIDGEDRIVER3940">
<gates>
<gate name="G$1" symbol="BRIDGE-DRIVER3940"/>
</gates>
<devices>
<device name="" package="SOIC-.3-28">
<connects>
<connect gate="G$1" pin="CA" pad="9"/>
<connect gate="G$1" pin="CB" pad="6"/>
<connect gate="G$1" pin="CP1" pad="16"/>
<connect gate="G$1" pin="CP2" pad="14"/>
<connect gate="G$1" pin="EN" pad="23"/>
<connect gate="G$1" pin="FAULT" pad="18"/>
<connect gate="G$1" pin="GHA" pad="10"/>
<connect gate="G$1" pin="GHB" pad="5"/>
<connect gate="G$1" pin="GLA" pad="12"/>
<connect gate="G$1" pin="GLB" pad="3"/>
<connect gate="G$1" pin="GND" pad="17"/>
<connect gate="G$1" pin="IDEAD" pad="27"/>
<connect gate="G$1" pin="LONG" pad="26"/>
<connect gate="G$1" pin="LSS" pad="2"/>
<connect gate="G$1" pin="MODE" pad="21"/>
<connect gate="G$1" pin="OVSET" pad="19"/>
<connect gate="G$1" pin="PHASE" pad="24"/>
<connect gate="G$1" pin="RESET" pad="25"/>
<connect gate="G$1" pin="SA" pad="11"/>
<connect gate="G$1" pin="SB" pad="4"/>
<connect gate="G$1" pin="SR" pad="22"/>
<connect gate="G$1" pin="VBB" pad="13"/>
<connect gate="G$1" pin="VCP" pad="15"/>
<connect gate="G$1" pin="VDR" pad="1"/>
<connect gate="G$1" pin="VDSTH" pad="28"/>
<connect gate="G$1" pin="VIN" pad="7"/>
<connect gate="G$1" pin="VR13" pad="8"/>
<connect gate="G$1" pin="VR5" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FQP50N06" prefix="Q">
<description>&lt;b&gt;HEXFET Power MOSFET&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="P-MOSFET-N"/>
</gates>
<devices>
<device name="" package="TO220BV">
<connects>
<connect gate="G$1" pin="D" pad="D"/>
<connect gate="G$1" pin="G" pad="G"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPT4" prefix="X" uservalue="yes">
<description>&lt;b&gt;PHOENIX CONNECTOR&lt;/b&gt;</description>
<gates>
<gate name="-1" symbol="SKB"/>
<gate name="-2" symbol="SKB"/>
<gate name="-3" symbol="SKB"/>
<gate name="-4" symbol="SKBV"/>
</gates>
<devices>
<device name="" package="4POL254">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-2" pin="1" pad="2"/>
<connect gate="-3" pin="1" pad="3"/>
<connect gate="-4" pin="1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="18F4620V2">
<gates>
<gate name="G$1" symbol="4620V2"/>
</gates>
<devices>
<device name="PLCC44" package="PLCC-44">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FASTON-LUG" prefix="L" uservalue="yes">
<gates>
<gate name="G$1" symbol="LUG"/>
</gates>
<devices>
<device name="" package="SAPDELUG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICROFIT-6" prefix="CON" uservalue="yes">
<gates>
<gate name="G$1" symbol="MICROFIT-6"/>
</gates>
<devices>
<device name="" package="MW-MICROFIT-6">
<connects>
<connect gate="G$1" pin="P$1" pad="P$6"/>
<connect gate="G$1" pin="P$2" pad="P$5"/>
<connect gate="G$1" pin="P$3" pad="P$4"/>
<connect gate="G$1" pin="P$4" pad="P$3"/>
<connect gate="G$1" pin="P$5" pad="P$2"/>
<connect gate="G$1" pin="P$6" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ACS712">
<gates>
<gate name="G$1" symbol="ACS706"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN@1" pad="1"/>
<connect gate="G$1" pin="IN@2" pad="2"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="OUT@1" pad="3"/>
<connect gate="G$1" pin="OUT@2" pad="4"/>
<connect gate="G$1" pin="VAL" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="ACS714">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN@1" pad="1"/>
<connect gate="G$1" pin="IN@2" pad="2"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="OUT@1" pad="3"/>
<connect gate="G$1" pin="OUT@2" pad="4"/>
<connect gate="G$1" pin="VAL" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICROFIT-8">
<gates>
<gate name="G$1" symbol="MICROFIT-8"/>
</gates>
<devices>
<device name="" package="MW-MICROFIT-8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LINX-LC-S-TX">
<gates>
<gate name="G$1" symbol="LINX-LC-S-TX"/>
</gates>
<devices>
<device name="" package="LINX-LC-S-TX">
<connects>
<connect gate="G$1" pin="ANT" pad="5"/>
<connect gate="G$1" pin="DATA" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="3"/>
<connect gate="G$1" pin="GND@3" pad="6"/>
<connect gate="G$1" pin="GND@4" pad="8"/>
<connect gate="G$1" pin="LADJ" pad="4"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LINX-LC-S-RC">
<gates>
<gate name="G$1" symbol="LINX-LC-S-RC"/>
</gates>
<devices>
<device name="" package="LINX-LC-S-RX">
<connects>
<connect gate="G$1" pin="ANT" pad="16"/>
<connect gate="G$1" pin="DATA" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="15"/>
<connect gate="G$1" pin="NC@1" pad="1"/>
<connect gate="G$1" pin="NC@10" pad="14"/>
<connect gate="G$1" pin="NC@2" pad="2"/>
<connect gate="G$1" pin="NC@3" pad="3"/>
<connect gate="G$1" pin="NC@4" pad="7"/>
<connect gate="G$1" pin="NC@5" pad="9"/>
<connect gate="G$1" pin="NC@6" pad="10"/>
<connect gate="G$1" pin="NC@7" pad="11"/>
<connect gate="G$1" pin="NC@8" pad="12"/>
<connect gate="G$1" pin="NC@9" pad="13"/>
<connect gate="G$1" pin="PDN" pad="6"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOLEX-43045-8" prefix="CON">
<gates>
<gate name="G$1" symbol="MOLEX-43045-8"/>
</gates>
<devices>
<device name="" package="MOLEX-34045-8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA" package="MOLEX-34045-RA-8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADAPTER-16-SOIC">
<gates>
<gate name="G$1" symbol="ADAPTER-SOIC-16"/>
</gates>
<devices>
<device name="SOIC-16" package="SO16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ACS755" prefix="CS" uservalue="yes">
<gates>
<gate name="G$1" symbol="ACS755"/>
</gates>
<devices>
<device name="" package="ACS755">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IP+" pad="4"/>
<connect gate="G$1" pin="IP-" pad="5"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MRF24J40">
<gates>
<gate name="G$1" symbol="MRF24J40"/>
</gates>
<devices>
<device name="" package="QFN40">
<connects>
<connect gate="G$1" pin="CLKOUT" pad="26"/>
<connect gate="G$1" pin="CS/" pad="20"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="14"/>
<connect gate="G$1" pin="GND@3" pad="22"/>
<connect gate="G$1" pin="GND@4" pad="24"/>
<connect gate="G$1" pin="GND@5" pad="25"/>
<connect gate="G$1" pin="GND@6" pad="36"/>
<connect gate="G$1" pin="GPIO0" pad="7"/>
<connect gate="G$1" pin="GPIO1" pad="8"/>
<connect gate="G$1" pin="GPIO2" pad="11"/>
<connect gate="G$1" pin="GPIO3" pad="12"/>
<connect gate="G$1" pin="GPIO4" pad="10"/>
<connect gate="G$1" pin="GPIO5" pad="9"/>
<connect gate="G$1" pin="INT" pad="16"/>
<connect gate="G$1" pin="LCAP" pad="40"/>
<connect gate="G$1" pin="LPOSC1" pad="28"/>
<connect gate="G$1" pin="LPOSC2" pad="27"/>
<connect gate="G$1" pin="NC@1" pad="23"/>
<connect gate="G$1" pin="NC@2" pad="38"/>
<connect gate="G$1" pin="OSC1" pad="34"/>
<connect gate="G$1" pin="OSC2" pad="33"/>
<connect gate="G$1" pin="RESET/" pad="13"/>
<connect gate="G$1" pin="RFN" pad="3"/>
<connect gate="G$1" pin="RFP" pad="2"/>
<connect gate="G$1" pin="RXIP" pad="29"/>
<connect gate="G$1" pin="RXQP" pad="30"/>
<connect gate="G$1" pin="SCK" pad="19"/>
<connect gate="G$1" pin="SDI" pad="18"/>
<connect gate="G$1" pin="SDO" pad="17"/>
<connect gate="G$1" pin="VDD@1" pad="1"/>
<connect gate="G$1" pin="VDD@2" pad="4"/>
<connect gate="G$1" pin="VDD@3" pad="5"/>
<connect gate="G$1" pin="VDD@4" pad="21"/>
<connect gate="G$1" pin="VDD@5" pad="31"/>
<connect gate="G$1" pin="VDD@6" pad="32"/>
<connect gate="G$1" pin="VDD@7" pad="35"/>
<connect gate="G$1" pin="VDD@8" pad="37"/>
<connect gate="G$1" pin="VDD@9" pad="39"/>
<connect gate="G$1" pin="WAKE" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOLEX-43045-10">
<gates>
<gate name="G$1" symbol="MOLEX-34045-10"/>
</gates>
<devices>
<device name="" package="MOLEX-34045-10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA" package="MOLEX-34045-RA-10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOLEX-43045-4" prefix="CON">
<gates>
<gate name="G$1" symbol="MOLEX-43045-4"/>
</gates>
<devices>
<device name="" package="MOLEX-34045-4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA" package="MOLEX-34045-RA-4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LINX-LR-S-TX">
<gates>
<gate name="G$1" symbol="LINX-LR-S-TX"/>
</gates>
<devices>
<device name="" package="LINX-LC-S-TX">
<connects>
<connect gate="G$1" pin="ANT" pad="5"/>
<connect gate="G$1" pin="DATA" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="3"/>
<connect gate="G$1" pin="GND@3" pad="6"/>
<connect gate="G$1" pin="LADJ" pad="4"/>
<connect gate="G$1" pin="PDN" pad="8"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LINX-LR-S-RC" prefix="IC">
<gates>
<gate name="G$1" symbol="LINK-LR-S-RC"/>
</gates>
<devices>
<device name="" package="LINX-LC-S-RX">
<connects>
<connect gate="G$1" pin="ANT" pad="16"/>
<connect gate="G$1" pin="DATA" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="15"/>
<connect gate="G$1" pin="NC@1" pad="1"/>
<connect gate="G$1" pin="NC@10" pad="14"/>
<connect gate="G$1" pin="NC@2" pad="2"/>
<connect gate="G$1" pin="NC@3" pad="3"/>
<connect gate="G$1" pin="NC@5" pad="9"/>
<connect gate="G$1" pin="NC@6" pad="10"/>
<connect gate="G$1" pin="NC@7" pad="11"/>
<connect gate="G$1" pin="NC@8" pad="12"/>
<connect gate="G$1" pin="NC@9" pad="13"/>
<connect gate="G$1" pin="PDN" pad="6"/>
<connect gate="G$1" pin="RSSI" pad="7"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HAIS200">
<gates>
<gate name="G$1" symbol="HAIS200"/>
</gates>
<devices>
<device name="" package="HAIS200">
<connects>
<connect gate="G$1" pin="+5" pad="1"/>
<connect gate="G$1" pin="0V" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VREF" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PVOLTBAT">
<gates>
<gate name="G$1" symbol="9VOLTBAT"/>
</gates>
<devices>
<device name="" package="9VBATHOLDER">
<connects>
<connect gate="G$1" pin="MINUS" pad="-"/>
<connect gate="G$1" pin="PLUS" pad="+"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC1255">
<gates>
<gate name="G$1" symbol="LTC1255"/>
</gates>
<devices>
<device name="" package="DIL8">
<connects>
<connect gate="G$1" pin="DS1" pad="1"/>
<connect gate="G$1" pin="DS2" pad="8"/>
<connect gate="G$1" pin="G1" pad="2"/>
<connect gate="G$1" pin="G2" pad="7"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOIC" package="SO08">
<connects>
<connect gate="G$1" pin="DS1" pad="1"/>
<connect gate="G$1" pin="DS2" pad="8"/>
<connect gate="G$1" pin="G1" pad="2"/>
<connect gate="G$1" pin="G2" pad="7"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="3TERMINALBLOCK">
<gates>
<gate name="G$1" symbol="3TERMINALBLOCK"/>
</gates>
<devices>
<device name="" package="3TERMINALSTRIP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BIGLUG">
<description>Large Connection Lug</description>
<gates>
<gate name="G$1" symbol="BIGLUG"/>
</gates>
<devices>
<device name="" package="BIGLUG">
<connects>
<connect gate="G$1" pin="LUG1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMALL" package="1X01">
<connects>
<connect gate="G$1" pin="LUG1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FUSESOCKET">
<gates>
<gate name="G$1" symbol="FUSESOCKET"/>
</gates>
<devices>
<device name="" package="FUSESOCKET">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="12MMBUTTONBAT">
<gates>
<gate name="G$1" symbol="BUTTON-BAT-12MM"/>
</gates>
<devices>
<device name="" package="12MMBATSM">
<connects>
<connect gate="G$1" pin="+" pad="PLUS"/>
<connect gate="G$1" pin="N1" pad="N1"/>
<connect gate="G$1" pin="N2" pad="N2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRLM2402">
<gates>
<gate name="G$1" symbol="N-CHANNEL-MOSFET"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPDT-SLIDE-SMT">
<gates>
<gate name="G$1" symbol="SDPT-SLIDE"/>
</gates>
<devices>
<device name="" package="SPDT-SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT232BL" prefix="U">
<description>&lt;b&gt;USB UART&lt;/b&gt;
&lt;p&gt;
2&lt;sup&gt;nd&lt;/sup&gt; Generation USB UART (USB &amp;lt;-&amp;gt; Serial) Controller
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FT232BL"/>
</gates>
<devices>
<device name="" package="LQFP32">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="6"/>
<connect gate="G$1" pin="AGND" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="CTS#" pad="22"/>
<connect gate="G$1" pin="DCD#" pad="19"/>
<connect gate="G$1" pin="DSR#" pad="20"/>
<connect gate="G$1" pin="DTR#" pad="21"/>
<connect gate="G$1" pin="EECS" pad="32"/>
<connect gate="G$1" pin="EEDATA" pad="2"/>
<connect gate="G$1" pin="EESK" pad="1"/>
<connect gate="G$1" pin="GND1" pad="9"/>
<connect gate="G$1" pin="GND2" pad="17"/>
<connect gate="G$1" pin="PWRCTL" pad="14"/>
<connect gate="G$1" pin="PWREN#" pad="15"/>
<connect gate="G$1" pin="RESET#" pad="4"/>
<connect gate="G$1" pin="RI#" pad="18"/>
<connect gate="G$1" pin="RSTOUT#" pad="5"/>
<connect gate="G$1" pin="RTS#" pad="23"/>
<connect gate="G$1" pin="RXD" pad="24"/>
<connect gate="G$1" pin="RXLED#" pad="11"/>
<connect gate="G$1" pin="SLEEP#" pad="10"/>
<connect gate="G$1" pin="TEST" pad="31"/>
<connect gate="G$1" pin="TXD" pad="25"/>
<connect gate="G$1" pin="TXDEN" pad="16"/>
<connect gate="G$1" pin="TXLED#" pad="12"/>
<connect gate="G$1" pin="USBDM" pad="8"/>
<connect gate="G$1" pin="USBDP" pad="7"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="26"/>
<connect gate="G$1" pin="VCCIO" pad="13"/>
<connect gate="G$1" pin="XTIN" pad="27"/>
<connect gate="G$1" pin="XTOUT" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CSTCR-RESONATOR" uservalue="yes">
<gates>
<gate name="G$1" symbol="CSTCR-RESONATOR"/>
</gates>
<devices>
<device name="" package="CSTCR-RESONATOR">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1700" uservalue="yes">
<gates>
<gate name="G$1" symbol="MCP1700"/>
</gates>
<devices>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VI" pad="3"/>
<connect gate="G$1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT89" package="SOT89">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VI" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FERRITEBEAD">
<gates>
<gate name="G$1" symbol="FERRITEBEAD"/>
</gates>
<devices>
<device name="" package="C0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="93*" prefix="IC">
<description>Serial &lt;B&gt;EPROM&lt;/B&gt;&lt;p&gt;
1 K/2 K/4 K, low voltage, Microwire</description>
<gates>
<gate name="G$1" symbol="93LC46"/>
</gates>
<devices>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="NU" pad="7"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="AA46"/>
<technology name="AA56"/>
<technology name="AA66"/>
<technology name="LC45"/>
<technology name="LC46"/>
<technology name="LC66"/>
</technologies>
</device>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="NU" pad="7"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="AA46"/>
<technology name="AA56"/>
<technology name="AA66"/>
<technology name="LC46"/>
<technology name="LC56"/>
<technology name="LC66"/>
</technologies>
</device>
<device name="SM" package="SO-08M">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="NU" pad="7"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="AA46"/>
<technology name="AA56"/>
<technology name="AA66"/>
<technology name="LC46"/>
<technology name="LC56"/>
<technology name="LC66"/>
</technologies>
</device>
<device name="ST" package="TSSOP8">
<connects>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="NU" pad="7"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="LC46"/>
<technology name="LC56"/>
<technology name="LC66"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="18F8722" prefix="IC">
<gates>
<gate name="G$1" symbol="18F8722"/>
</gates>
<devices>
<device name="QFP" package="TQFP-80-12X12MM">
<connects>
<connect gate="G$1" pin="A0" pad="30"/>
<connect gate="G$1" pin="A1" pad="29"/>
<connect gate="G$1" pin="A2" pad="28"/>
<connect gate="G$1" pin="A3" pad="27"/>
<connect gate="G$1" pin="A4" pad="34"/>
<connect gate="G$1" pin="A5" pad="33"/>
<connect gate="G$1" pin="A6/OSCO" pad="50"/>
<connect gate="G$1" pin="A7/OSCI" pad="49"/>
<connect gate="G$1" pin="AVDD" pad="25"/>
<connect gate="G$1" pin="AVSS" pad="26"/>
<connect gate="G$1" pin="B0/INT0" pad="58"/>
<connect gate="G$1" pin="B1/INT1" pad="57"/>
<connect gate="G$1" pin="B2/INT2" pad="56"/>
<connect gate="G$1" pin="B3/INT3" pad="55"/>
<connect gate="G$1" pin="B4" pad="54"/>
<connect gate="G$1" pin="B5/PGM" pad="53"/>
<connect gate="G$1" pin="B6/PGC" pad="52"/>
<connect gate="G$1" pin="B7/PGD" pad="47"/>
<connect gate="G$1" pin="C0" pad="36"/>
<connect gate="G$1" pin="C1" pad="35"/>
<connect gate="G$1" pin="C2" pad="43"/>
<connect gate="G$1" pin="C3/SCLK1" pad="44"/>
<connect gate="G$1" pin="C4/SDI1" pad="45"/>
<connect gate="G$1" pin="C5/SDO1" pad="46"/>
<connect gate="G$1" pin="C6/TX1" pad="37"/>
<connect gate="G$1" pin="C7/RX1" pad="38"/>
<connect gate="G$1" pin="D0" pad="72"/>
<connect gate="G$1" pin="D1" pad="69"/>
<connect gate="G$1" pin="D2" pad="68"/>
<connect gate="G$1" pin="D3" pad="67"/>
<connect gate="G$1" pin="D4/SDO2" pad="66"/>
<connect gate="G$1" pin="D5/SDI2" pad="65"/>
<connect gate="G$1" pin="D6/SCLK2" pad="64"/>
<connect gate="G$1" pin="D7" pad="63"/>
<connect gate="G$1" pin="E0" pad="4"/>
<connect gate="G$1" pin="E1" pad="3"/>
<connect gate="G$1" pin="E2" pad="78"/>
<connect gate="G$1" pin="E3" pad="77"/>
<connect gate="G$1" pin="E4" pad="76"/>
<connect gate="G$1" pin="E5" pad="75"/>
<connect gate="G$1" pin="E6" pad="74"/>
<connect gate="G$1" pin="E7" pad="73"/>
<connect gate="G$1" pin="F0" pad="24"/>
<connect gate="G$1" pin="F1" pad="23"/>
<connect gate="G$1" pin="F2" pad="18"/>
<connect gate="G$1" pin="F3" pad="17"/>
<connect gate="G$1" pin="F4" pad="16"/>
<connect gate="G$1" pin="F5" pad="15"/>
<connect gate="G$1" pin="F6" pad="14"/>
<connect gate="G$1" pin="F7" pad="13"/>
<connect gate="G$1" pin="G0" pad="5"/>
<connect gate="G$1" pin="G1/TX2" pad="6"/>
<connect gate="G$1" pin="G2/RX2" pad="7"/>
<connect gate="G$1" pin="G3" pad="8"/>
<connect gate="G$1" pin="G4" pad="10"/>
<connect gate="G$1" pin="G5/!MCLR" pad="9"/>
<connect gate="G$1" pin="H0" pad="79"/>
<connect gate="G$1" pin="H1" pad="80"/>
<connect gate="G$1" pin="H2" pad="1"/>
<connect gate="G$1" pin="H3" pad="2"/>
<connect gate="G$1" pin="H4" pad="22"/>
<connect gate="G$1" pin="H5" pad="21"/>
<connect gate="G$1" pin="H6" pad="20"/>
<connect gate="G$1" pin="H7" pad="19"/>
<connect gate="G$1" pin="J0" pad="62"/>
<connect gate="G$1" pin="J1" pad="61"/>
<connect gate="G$1" pin="J2" pad="60"/>
<connect gate="G$1" pin="J3" pad="59"/>
<connect gate="G$1" pin="J4" pad="39"/>
<connect gate="G$1" pin="J5" pad="40"/>
<connect gate="G$1" pin="J6" pad="41"/>
<connect gate="G$1" pin="J7" pad="42"/>
<connect gate="G$1" pin="VDD@1" pad="12"/>
<connect gate="G$1" pin="VDD@2" pad="32"/>
<connect gate="G$1" pin="VDD@3" pad="48"/>
<connect gate="G$1" pin="VDD@4" pad="71"/>
<connect gate="G$1" pin="VSS@1" pad="11"/>
<connect gate="G$1" pin="VSS@2" pad="31"/>
<connect gate="G$1" pin="VSS@3" pad="51"/>
<connect gate="G$1" pin="VSS@4" pad="70"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RMS" package="TQFP80-12X12">
<connects>
<connect gate="G$1" pin="A0" pad="30"/>
<connect gate="G$1" pin="A1" pad="29"/>
<connect gate="G$1" pin="A2" pad="28"/>
<connect gate="G$1" pin="A3" pad="27"/>
<connect gate="G$1" pin="A4" pad="34"/>
<connect gate="G$1" pin="A5" pad="33"/>
<connect gate="G$1" pin="A6/OSCO" pad="50"/>
<connect gate="G$1" pin="A7/OSCI" pad="49"/>
<connect gate="G$1" pin="AVDD" pad="25"/>
<connect gate="G$1" pin="AVSS" pad="26"/>
<connect gate="G$1" pin="B0/INT0" pad="58"/>
<connect gate="G$1" pin="B1/INT1" pad="57"/>
<connect gate="G$1" pin="B2/INT2" pad="56"/>
<connect gate="G$1" pin="B3/INT3" pad="55"/>
<connect gate="G$1" pin="B4" pad="54"/>
<connect gate="G$1" pin="B5/PGM" pad="53"/>
<connect gate="G$1" pin="B6/PGC" pad="52"/>
<connect gate="G$1" pin="B7/PGD" pad="47"/>
<connect gate="G$1" pin="C0" pad="36"/>
<connect gate="G$1" pin="C1" pad="35"/>
<connect gate="G$1" pin="C2" pad="43"/>
<connect gate="G$1" pin="C3/SCLK1" pad="44"/>
<connect gate="G$1" pin="C4/SDI1" pad="45"/>
<connect gate="G$1" pin="C5/SDO1" pad="46"/>
<connect gate="G$1" pin="C6/TX1" pad="37"/>
<connect gate="G$1" pin="C7/RX1" pad="38"/>
<connect gate="G$1" pin="D0" pad="72"/>
<connect gate="G$1" pin="D1" pad="69"/>
<connect gate="G$1" pin="D2" pad="68"/>
<connect gate="G$1" pin="D3" pad="67"/>
<connect gate="G$1" pin="D4/SDO2" pad="66"/>
<connect gate="G$1" pin="D5/SDI2" pad="65"/>
<connect gate="G$1" pin="D6/SCLK2" pad="64"/>
<connect gate="G$1" pin="D7" pad="63"/>
<connect gate="G$1" pin="E0" pad="4"/>
<connect gate="G$1" pin="E1" pad="3"/>
<connect gate="G$1" pin="E2" pad="78"/>
<connect gate="G$1" pin="E3" pad="77"/>
<connect gate="G$1" pin="E4" pad="76"/>
<connect gate="G$1" pin="E5" pad="75"/>
<connect gate="G$1" pin="E6" pad="74"/>
<connect gate="G$1" pin="E7" pad="73"/>
<connect gate="G$1" pin="F0" pad="24"/>
<connect gate="G$1" pin="F1" pad="23"/>
<connect gate="G$1" pin="F2" pad="18"/>
<connect gate="G$1" pin="F3" pad="17"/>
<connect gate="G$1" pin="F4" pad="16"/>
<connect gate="G$1" pin="F5" pad="15"/>
<connect gate="G$1" pin="F6" pad="14"/>
<connect gate="G$1" pin="F7" pad="13"/>
<connect gate="G$1" pin="G0" pad="5"/>
<connect gate="G$1" pin="G1/TX2" pad="6"/>
<connect gate="G$1" pin="G2/RX2" pad="7"/>
<connect gate="G$1" pin="G3" pad="8"/>
<connect gate="G$1" pin="G4" pad="10"/>
<connect gate="G$1" pin="G5/!MCLR" pad="9"/>
<connect gate="G$1" pin="H0" pad="79"/>
<connect gate="G$1" pin="H1" pad="80"/>
<connect gate="G$1" pin="H2" pad="1"/>
<connect gate="G$1" pin="H3" pad="2"/>
<connect gate="G$1" pin="H4" pad="22"/>
<connect gate="G$1" pin="H5" pad="21"/>
<connect gate="G$1" pin="H6" pad="20"/>
<connect gate="G$1" pin="H7" pad="19"/>
<connect gate="G$1" pin="J0" pad="62"/>
<connect gate="G$1" pin="J1" pad="61"/>
<connect gate="G$1" pin="J2" pad="60"/>
<connect gate="G$1" pin="J3" pad="59"/>
<connect gate="G$1" pin="J4" pad="39"/>
<connect gate="G$1" pin="J5" pad="40"/>
<connect gate="G$1" pin="J6" pad="41"/>
<connect gate="G$1" pin="J7" pad="42"/>
<connect gate="G$1" pin="VDD@1" pad="12"/>
<connect gate="G$1" pin="VDD@2" pad="32"/>
<connect gate="G$1" pin="VDD@3" pad="48"/>
<connect gate="G$1" pin="VDD@4" pad="71"/>
<connect gate="G$1" pin="VSS@1" pad="11"/>
<connect gate="G$1" pin="VSS@2" pad="31"/>
<connect gate="G$1" pin="VSS@3" pad="51"/>
<connect gate="G$1" pin="VSS@4" pad="70"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CSTCE-RESONATOR">
<description>&lt;dl&gt;&lt;p&gt;&lt;strong&gt;Ceramic Resonator&lt;br /&gt;
&lt;/strong&gt;Murata&lt;br /&gt;
  Internal Capacitors &lt;/p&gt;
&lt;/dl&gt;</description>
<gates>
<gate name="G$1" symbol="CSTCR-RESONATOR"/>
</gates>
<devices>
<device name="10MOG" package="CSTCE-10M0G">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="20M0V" package="CSTCE-20M0V">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC(J)18F8*" prefix="IC">
<description>&lt;b&gt;PIC18F87J10 FAMILY&lt;/b&gt; 64/80-Pin, High-Performance, 1-Mbit Flash Microcontrollers with nanoWatt Technology&lt;p&gt;
Source: http://www.microchip.com/ .. 39663c.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F87J10"/>
</gates>
<devices>
<device name="" package="TQFP80-12X12">
<connects>
<connect gate="G$1" pin="!MCLR" pad="9"/>
<connect gate="G$1" pin="AVDD" pad="25"/>
<connect gate="G$1" pin="AVSS" pad="26"/>
<connect gate="G$1" pin="ENVREG" pad="24"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="49"/>
<connect gate="G$1" pin="OSC2/CLKO" pad="50"/>
<connect gate="G$1" pin="RA0/AN0" pad="30"/>
<connect gate="G$1" pin="RA1/AN1" pad="29"/>
<connect gate="G$1" pin="RA2/AN2/VREF-" pad="28"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="27"/>
<connect gate="G$1" pin="RA4/T0CK" pad="34"/>
<connect gate="G$1" pin="RA5/AN4" pad="33"/>
<connect gate="G$1" pin="RB0/INT0/FLT0" pad="58"/>
<connect gate="G$1" pin="RB1/INT1" pad="57"/>
<connect gate="G$1" pin="RB2/INT2" pad="56"/>
<connect gate="G$1" pin="RB3/INT3/ACCP2/P2A" pad="55"/>
<connect gate="G$1" pin="RB4/KBI0" pad="54"/>
<connect gate="G$1" pin="RB5/KBI1" pad="53"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="52"/>
<connect gate="G$1" pin="RB7/KBI2/PGD" pad="47"/>
<connect gate="G$1" pin="RC0/T1OSO/T13CKI" pad="36"/>
<connect gate="G$1" pin="RC1/T1OSI/ECCP2/P2A" pad="35"/>
<connect gate="G$1" pin="RC2/ECCP1/P1A" pad="43"/>
<connect gate="G$1" pin="RC3/SCK1/SCL1" pad="44"/>
<connect gate="G$1" pin="RC4/SDI1/SDA1" pad="45"/>
<connect gate="G$1" pin="RC5/SDO1" pad="46"/>
<connect gate="G$1" pin="RC6/TX1/CK1" pad="37"/>
<connect gate="G$1" pin="RC7/RX1/DT1" pad="38"/>
<connect gate="G$1" pin="RD0/AD0/PSP0" pad="72"/>
<connect gate="G$1" pin="RD1/AD1/PSP1" pad="69"/>
<connect gate="G$1" pin="RD2/AD2/PSP2" pad="68"/>
<connect gate="G$1" pin="RD3/AD3/PSP3" pad="67"/>
<connect gate="G$1" pin="RD4/AD4/PSP4/SDO2" pad="66"/>
<connect gate="G$1" pin="RD5/AD5/PSP5/SDI2/SDA2" pad="65"/>
<connect gate="G$1" pin="RD6/AD6/PSP6/SCK2/SCL2" pad="64"/>
<connect gate="G$1" pin="RD7/AD7/PSP7/!SS2" pad="63"/>
<connect gate="G$1" pin="RE0/AD8/!RD/P2D" pad="4"/>
<connect gate="G$1" pin="RE1/AD9/!WR/P2C" pad="3"/>
<connect gate="G$1" pin="RE2/!AD10CS/P2B" pad="78"/>
<connect gate="G$1" pin="RE3/AD11/P3C" pad="77"/>
<connect gate="G$1" pin="RE4/AD12/P3B" pad="76"/>
<connect gate="G$1" pin="RE5/AD13/P1C" pad="75"/>
<connect gate="G$1" pin="RE6/AD14/P1B" pad="74"/>
<connect gate="G$1" pin="RE7/AD15/ECCP2/P2A" pad="73"/>
<connect gate="G$1" pin="RF1/AN6/C2OUT" pad="23"/>
<connect gate="G$1" pin="RF2/AN7/C1OUT" pad="18"/>
<connect gate="G$1" pin="RF3/AN8" pad="17"/>
<connect gate="G$1" pin="RF4/AN9" pad="16"/>
<connect gate="G$1" pin="RF5/AN10/CVREF" pad="15"/>
<connect gate="G$1" pin="RF6/AN11" pad="14"/>
<connect gate="G$1" pin="RF7/!SS1" pad="13"/>
<connect gate="G$1" pin="RG0/ECCP3/P3A" pad="5"/>
<connect gate="G$1" pin="RG1/TX2/CK2" pad="6"/>
<connect gate="G$1" pin="RG2/RX2/DT2" pad="7"/>
<connect gate="G$1" pin="RG3/CCP4/P3D" pad="8"/>
<connect gate="G$1" pin="RG4/CCP5/P1D" pad="10"/>
<connect gate="G$1" pin="RH0/A16" pad="79"/>
<connect gate="G$1" pin="RH1/A17" pad="80"/>
<connect gate="G$1" pin="RH2/A18" pad="1"/>
<connect gate="G$1" pin="RH3/A19" pad="2"/>
<connect gate="G$1" pin="RH4/AN12/P3C" pad="22"/>
<connect gate="G$1" pin="RH5/AN13/P3B" pad="21"/>
<connect gate="G$1" pin="RH6/AN14/P1C" pad="20"/>
<connect gate="G$1" pin="RH7/AN15/P1B" pad="19"/>
<connect gate="G$1" pin="RJ0/ALE" pad="62"/>
<connect gate="G$1" pin="RJ1/!OE" pad="61"/>
<connect gate="G$1" pin="RJ2/!WRL" pad="60"/>
<connect gate="G$1" pin="RJ3/!WRH" pad="59"/>
<connect gate="G$1" pin="RJ4/BA0" pad="39"/>
<connect gate="G$1" pin="RJ5/!CE" pad="40"/>
<connect gate="G$1" pin="RJ6/!LB" pad="41"/>
<connect gate="G$1" pin="RJ7/!UB" pad="42"/>
<connect gate="G$1" pin="VDD" pad="48"/>
<connect gate="G$1" pin="VDD@1" pad="32"/>
<connect gate="G$1" pin="VDD@2" pad="71"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="12"/>
<connect gate="G$1" pin="VSS" pad="11"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
<connect gate="G$1" pin="VSS@2" pad="51"/>
<connect gate="G$1" pin="VSS@3" pad="70"/>
</connects>
<technologies>
<technology name="5J10"/>
<technology name="5J15"/>
<technology name="6J10"/>
<technology name="6J15"/>
<technology name="7J10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F8*" prefix="IC">
<description>&lt;p&gt;&lt;strong&gt;PIC8722 Family &lt;/strong&gt;&lt;/p&gt;
&lt;p&gt;80 pin TQFG&lt;br /&gt;
  Devices vary as shown below.&lt;br /&gt;
  LF versions work on low VDD, with limitations on clock speed
&lt;/p&gt;
&lt;table border="1" cellspacing="0" cellpadding="0"&gt;
  &lt;tr&gt;
    &lt;td width="106" valign="top"&gt;&lt;p&gt;&lt;strong&gt;Device&lt;/strong&gt;&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;&lt;strong&gt;Flash(bytes)&lt;/strong&gt;&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;&lt;strong&gt;SRAM(bytes)&lt;/strong&gt;&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;&lt;strong&gt;EEPROM(bytes)&lt;/strong&gt;&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;&lt;strong&gt;I/O&lt;/strong&gt;&lt;/p&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td width="106" valign="top"&gt;&lt;p&gt;PIC18F8527&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;48K&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;3936&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;1024&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;70&lt;/p&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td width="106" valign="top"&gt;&lt;p&gt;PIC18F8622&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;64K&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;3936&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;1024&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;70&lt;/p&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td width="106" valign="top"&gt;&lt;p&gt;PIC18F8627&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;96K&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;3936&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;1024&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;70&lt;/p&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td width="106" valign="top"&gt;&lt;p&gt;PIC18F8722&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;128K&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;3936&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;1024&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;70&lt;/p&gt;&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;</description>
<gates>
<gate name="G$1" symbol="18F8722"/>
</gates>
<devices>
<device name="" package="TQFP80-12X12">
<connects>
<connect gate="G$1" pin="A0" pad="30"/>
<connect gate="G$1" pin="A1" pad="29"/>
<connect gate="G$1" pin="A2" pad="28"/>
<connect gate="G$1" pin="A3" pad="27"/>
<connect gate="G$1" pin="A4" pad="34"/>
<connect gate="G$1" pin="A5" pad="33"/>
<connect gate="G$1" pin="A6/OSCO" pad="50"/>
<connect gate="G$1" pin="A7/OSCI" pad="49"/>
<connect gate="G$1" pin="AVDD" pad="25"/>
<connect gate="G$1" pin="AVSS" pad="26"/>
<connect gate="G$1" pin="B0/INT0" pad="57"/>
<connect gate="G$1" pin="B1/INT1" pad="56"/>
<connect gate="G$1" pin="B2/INT2" pad="55"/>
<connect gate="G$1" pin="B3/INT3" pad="54"/>
<connect gate="G$1" pin="B4" pad="53"/>
<connect gate="G$1" pin="B5/PGM" pad="52"/>
<connect gate="G$1" pin="B6/PGC" pad="51"/>
<connect gate="G$1" pin="B7/PGD" pad="47"/>
<connect gate="G$1" pin="C0" pad="36"/>
<connect gate="G$1" pin="C1" pad="35"/>
<connect gate="G$1" pin="C2" pad="43"/>
<connect gate="G$1" pin="C3/SCLK1" pad="44"/>
<connect gate="G$1" pin="C4/SDI1" pad="45"/>
<connect gate="G$1" pin="C5/SDO1" pad="46"/>
<connect gate="G$1" pin="C6/TX1" pad="37"/>
<connect gate="G$1" pin="C7/RX1" pad="38"/>
<connect gate="G$1" pin="D0" pad="72"/>
<connect gate="G$1" pin="D1" pad="68"/>
<connect gate="G$1" pin="D2" pad="67"/>
<connect gate="G$1" pin="D3" pad="66"/>
<connect gate="G$1" pin="D4/SDO2" pad="65"/>
<connect gate="G$1" pin="D5/SDI2" pad="64"/>
<connect gate="G$1" pin="D6/SCLK2" pad="63"/>
<connect gate="G$1" pin="D7" pad="62"/>
<connect gate="G$1" pin="E0" pad="4"/>
<connect gate="G$1" pin="E1" pad="3"/>
<connect gate="G$1" pin="E2" pad="78"/>
<connect gate="G$1" pin="E3" pad="77"/>
<connect gate="G$1" pin="E4" pad="76"/>
<connect gate="G$1" pin="E5" pad="75"/>
<connect gate="G$1" pin="E6" pad="74"/>
<connect gate="G$1" pin="E7" pad="73"/>
<connect gate="G$1" pin="F0" pad="24"/>
<connect gate="G$1" pin="F1" pad="23"/>
<connect gate="G$1" pin="F2" pad="18"/>
<connect gate="G$1" pin="F3" pad="17"/>
<connect gate="G$1" pin="F4" pad="16"/>
<connect gate="G$1" pin="F5" pad="15"/>
<connect gate="G$1" pin="F6" pad="14"/>
<connect gate="G$1" pin="F7" pad="13"/>
<connect gate="G$1" pin="G0" pad="5"/>
<connect gate="G$1" pin="G1/TX2" pad="6"/>
<connect gate="G$1" pin="G2/RX2" pad="7"/>
<connect gate="G$1" pin="G3" pad="8"/>
<connect gate="G$1" pin="G4" pad="10"/>
<connect gate="G$1" pin="G5/!MCLR" pad="9"/>
<connect gate="G$1" pin="H0" pad="79"/>
<connect gate="G$1" pin="H1" pad="80"/>
<connect gate="G$1" pin="H2" pad="1"/>
<connect gate="G$1" pin="H3" pad="2"/>
<connect gate="G$1" pin="H4" pad="22"/>
<connect gate="G$1" pin="H5" pad="21"/>
<connect gate="G$1" pin="H6" pad="20"/>
<connect gate="G$1" pin="H7" pad="19"/>
<connect gate="G$1" pin="J0" pad="61"/>
<connect gate="G$1" pin="J1" pad="60"/>
<connect gate="G$1" pin="J2" pad="59"/>
<connect gate="G$1" pin="J3" pad="58"/>
<connect gate="G$1" pin="J4" pad="39"/>
<connect gate="G$1" pin="J5" pad="40"/>
<connect gate="G$1" pin="J6" pad="41"/>
<connect gate="G$1" pin="J7" pad="42"/>
<connect gate="G$1" pin="VDD@1" pad="12"/>
<connect gate="G$1" pin="VDD@2" pad="32"/>
<connect gate="G$1" pin="VDD@3" pad="48"/>
<connect gate="G$1" pin="VDD@4" pad="71"/>
<connect gate="G$1" pin="VSS@1" pad="11"/>
<connect gate="G$1" pin="VSS@2" pad="31"/>
<connect gate="G$1" pin="VSS@3" pad="69"/>
<connect gate="G$1" pin="VSS@4" pad="70"/>
</connects>
<technologies>
<technology name="527"/>
<technology name="622"/>
<technology name="627"/>
<technology name="722"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F6*" prefix="IC">
<description>&lt;p&gt;&lt;strong&gt;PIC8722 Family &lt;/strong&gt;(64 Pin Devices)&lt;/p&gt;
&lt;p&gt;64 pin TQFG&lt;br /&gt;
  Devices vary as shown below.&lt;br /&gt;
  LF versions work on low VDD, with limitations on clock speed &lt;/p&gt;
&lt;table border="1" cellspacing="0" cellpadding="0"&gt;
  &lt;tr&gt;
    &lt;td width="106" valign="top"&gt;&lt;p&gt;&lt;strong&gt;Device&lt;/strong&gt;&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;&lt;strong&gt;Flash(bytes)&lt;/strong&gt;&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;&lt;strong&gt;SRAM(bytes)&lt;/strong&gt;&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;&lt;strong&gt;EEPROM(bytes)&lt;/strong&gt;&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;&lt;strong&gt;I/O&lt;/strong&gt;&lt;/p&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td width="106" valign="top"&gt;&lt;p&gt;PIC18F6527&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;48K&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;3936&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;1024&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;54&lt;/p&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td width="106" valign="top"&gt;&lt;p&gt;PIC18F6622&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;64K&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;3936&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;1024&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;54&lt;/p&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td width="106" valign="top"&gt;&lt;p&gt;PIC18F6627&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;96K&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;3936&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;1024&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;54&lt;/p&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td width="106" valign="top"&gt;&lt;p&gt;PIC18F6722&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;128K&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;3936&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;1024&lt;/p&gt;&lt;/td&gt;
    &lt;td width="106" valign="top"&gt;&lt;p align="center"&gt;54&lt;/p&gt;&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;</description>
<gates>
<gate name="G$1" symbol="PIC64PIN-SQ"/>
</gates>
<devices>
<device name="A" package="TQFP64-10X10">
<connects>
<connect gate="G$1" pin="A0" pad="24"/>
<connect gate="G$1" pin="A1" pad="23"/>
<connect gate="G$1" pin="A2" pad="22"/>
<connect gate="G$1" pin="A3" pad="21"/>
<connect gate="G$1" pin="A4" pad="28"/>
<connect gate="G$1" pin="A5" pad="27"/>
<connect gate="G$1" pin="A6/OSCO" pad="40"/>
<connect gate="G$1" pin="A7/OSCI" pad="39"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="B0/INT0" pad="48"/>
<connect gate="G$1" pin="B1/INT1" pad="47"/>
<connect gate="G$1" pin="B2/INT2" pad="46"/>
<connect gate="G$1" pin="B3/INT3" pad="45"/>
<connect gate="G$1" pin="B4" pad="44"/>
<connect gate="G$1" pin="B5/PGM" pad="43"/>
<connect gate="G$1" pin="B6/PGC" pad="42"/>
<connect gate="G$1" pin="B7/PGD" pad="37"/>
<connect gate="G$1" pin="C0" pad="30"/>
<connect gate="G$1" pin="C1" pad="29"/>
<connect gate="G$1" pin="C2" pad="33"/>
<connect gate="G$1" pin="C3/SCLK1" pad="34"/>
<connect gate="G$1" pin="C4/MISO1" pad="35"/>
<connect gate="G$1" pin="C5/MOSI1" pad="36"/>
<connect gate="G$1" pin="C6/TX1" pad="31"/>
<connect gate="G$1" pin="C7/RX1" pad="32"/>
<connect gate="G$1" pin="D0" pad="58"/>
<connect gate="G$1" pin="D1" pad="55"/>
<connect gate="G$1" pin="D2" pad="54"/>
<connect gate="G$1" pin="D3" pad="53"/>
<connect gate="G$1" pin="D4/MOSI2" pad="52"/>
<connect gate="G$1" pin="D5/MISO2" pad="51"/>
<connect gate="G$1" pin="D6/SCLK2" pad="50"/>
<connect gate="G$1" pin="D7" pad="49"/>
<connect gate="G$1" pin="E0" pad="2"/>
<connect gate="G$1" pin="E1" pad="1"/>
<connect gate="G$1" pin="E2" pad="64"/>
<connect gate="G$1" pin="E3" pad="63"/>
<connect gate="G$1" pin="E4" pad="62"/>
<connect gate="G$1" pin="E5" pad="61"/>
<connect gate="G$1" pin="E6" pad="60"/>
<connect gate="G$1" pin="E7" pad="59"/>
<connect gate="G$1" pin="F0" pad="18"/>
<connect gate="G$1" pin="F1" pad="17"/>
<connect gate="G$1" pin="F2" pad="16"/>
<connect gate="G$1" pin="F3" pad="15"/>
<connect gate="G$1" pin="F4" pad="14"/>
<connect gate="G$1" pin="F5" pad="13"/>
<connect gate="G$1" pin="F6" pad="12"/>
<connect gate="G$1" pin="F7" pad="11"/>
<connect gate="G$1" pin="G0" pad="3"/>
<connect gate="G$1" pin="G1/TX2" pad="4"/>
<connect gate="G$1" pin="G2/RX2" pad="5"/>
<connect gate="G$1" pin="G3" pad="6"/>
<connect gate="G$1" pin="G4" pad="8"/>
<connect gate="G$1" pin="G5/!MCLR" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="10"/>
<connect gate="G$1" pin="VDD@2" pad="26"/>
<connect gate="G$1" pin="VDD@3" pad="38"/>
<connect gate="G$1" pin="VDD@4" pad="57"/>
<connect gate="G$1" pin="VSS@1" pad="9"/>
<connect gate="G$1" pin="VSS@2" pad="25"/>
<connect gate="G$1" pin="VSS@3" pad="41"/>
<connect gate="G$1" pin="VSS@4" pad="56"/>
</connects>
<technologies>
<technology name="527"/>
<technology name="622"/>
<technology name="627"/>
<technology name="722"/>
</technologies>
</device>
<device name="RMS" package="TQFP64-10X10RMS">
<connects>
<connect gate="G$1" pin="A0" pad="24"/>
<connect gate="G$1" pin="A1" pad="23"/>
<connect gate="G$1" pin="A2" pad="22"/>
<connect gate="G$1" pin="A3" pad="21"/>
<connect gate="G$1" pin="A4" pad="28"/>
<connect gate="G$1" pin="A5" pad="27"/>
<connect gate="G$1" pin="A6/OSCO" pad="40"/>
<connect gate="G$1" pin="A7/OSCI" pad="39"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="B0/INT0" pad="48"/>
<connect gate="G$1" pin="B1/INT1" pad="47"/>
<connect gate="G$1" pin="B2/INT2" pad="46"/>
<connect gate="G$1" pin="B3/INT3" pad="45"/>
<connect gate="G$1" pin="B4" pad="44"/>
<connect gate="G$1" pin="B5/PGM" pad="43"/>
<connect gate="G$1" pin="B6/PGC" pad="42"/>
<connect gate="G$1" pin="B7/PGD" pad="37"/>
<connect gate="G$1" pin="C0" pad="30"/>
<connect gate="G$1" pin="C1" pad="29"/>
<connect gate="G$1" pin="C2" pad="33"/>
<connect gate="G$1" pin="C3/SCLK1" pad="34"/>
<connect gate="G$1" pin="C4/MISO1" pad="35"/>
<connect gate="G$1" pin="C5/MOSI1" pad="36"/>
<connect gate="G$1" pin="C6/TX1" pad="31"/>
<connect gate="G$1" pin="C7/RX1" pad="32"/>
<connect gate="G$1" pin="D0" pad="58"/>
<connect gate="G$1" pin="D1" pad="55"/>
<connect gate="G$1" pin="D2" pad="54"/>
<connect gate="G$1" pin="D3" pad="53"/>
<connect gate="G$1" pin="D4/MOSI2" pad="52"/>
<connect gate="G$1" pin="D5/MISO2" pad="51"/>
<connect gate="G$1" pin="D6/SCLK2" pad="50"/>
<connect gate="G$1" pin="D7" pad="49"/>
<connect gate="G$1" pin="E0" pad="2"/>
<connect gate="G$1" pin="E1" pad="1"/>
<connect gate="G$1" pin="E2" pad="64"/>
<connect gate="G$1" pin="E3" pad="63"/>
<connect gate="G$1" pin="E4" pad="62"/>
<connect gate="G$1" pin="E5" pad="61"/>
<connect gate="G$1" pin="E6" pad="60"/>
<connect gate="G$1" pin="E7" pad="59"/>
<connect gate="G$1" pin="F0" pad="18"/>
<connect gate="G$1" pin="F1" pad="17"/>
<connect gate="G$1" pin="F2" pad="16"/>
<connect gate="G$1" pin="F3" pad="15"/>
<connect gate="G$1" pin="F4" pad="14"/>
<connect gate="G$1" pin="F5" pad="13"/>
<connect gate="G$1" pin="F6" pad="12"/>
<connect gate="G$1" pin="F7" pad="11"/>
<connect gate="G$1" pin="G0" pad="3"/>
<connect gate="G$1" pin="G1/TX2" pad="4"/>
<connect gate="G$1" pin="G2/RX2" pad="5"/>
<connect gate="G$1" pin="G3" pad="6"/>
<connect gate="G$1" pin="G4" pad="8"/>
<connect gate="G$1" pin="G5/!MCLR" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="10"/>
<connect gate="G$1" pin="VDD@2" pad="26"/>
<connect gate="G$1" pin="VDD@3" pad="38"/>
<connect gate="G$1" pin="VDD@4" pad="57"/>
<connect gate="G$1" pin="VSS@1" pad="9"/>
<connect gate="G$1" pin="VSS@2" pad="25"/>
<connect gate="G$1" pin="VSS@3" pad="41"/>
<connect gate="G$1" pin="VSS@4" pad="56"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RMS2" package="TQFP64-10X10RMSSTOP">
<connects>
<connect gate="G$1" pin="A0" pad="24"/>
<connect gate="G$1" pin="A1" pad="23"/>
<connect gate="G$1" pin="A2" pad="22"/>
<connect gate="G$1" pin="A3" pad="21"/>
<connect gate="G$1" pin="A4" pad="28"/>
<connect gate="G$1" pin="A5" pad="27"/>
<connect gate="G$1" pin="A6/OSCO" pad="40"/>
<connect gate="G$1" pin="A7/OSCI" pad="39"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="B0/INT0" pad="48"/>
<connect gate="G$1" pin="B1/INT1" pad="47"/>
<connect gate="G$1" pin="B2/INT2" pad="46"/>
<connect gate="G$1" pin="B3/INT3" pad="45"/>
<connect gate="G$1" pin="B4" pad="44"/>
<connect gate="G$1" pin="B5/PGM" pad="43"/>
<connect gate="G$1" pin="B6/PGC" pad="42"/>
<connect gate="G$1" pin="B7/PGD" pad="37"/>
<connect gate="G$1" pin="C0" pad="30"/>
<connect gate="G$1" pin="C1" pad="29"/>
<connect gate="G$1" pin="C2" pad="33"/>
<connect gate="G$1" pin="C3/SCLK1" pad="34"/>
<connect gate="G$1" pin="C4/MISO1" pad="35"/>
<connect gate="G$1" pin="C5/MOSI1" pad="36"/>
<connect gate="G$1" pin="C6/TX1" pad="31"/>
<connect gate="G$1" pin="C7/RX1" pad="32"/>
<connect gate="G$1" pin="D0" pad="58"/>
<connect gate="G$1" pin="D1" pad="55"/>
<connect gate="G$1" pin="D2" pad="54"/>
<connect gate="G$1" pin="D3" pad="53"/>
<connect gate="G$1" pin="D4/MOSI2" pad="52"/>
<connect gate="G$1" pin="D5/MISO2" pad="51"/>
<connect gate="G$1" pin="D6/SCLK2" pad="50"/>
<connect gate="G$1" pin="D7" pad="49"/>
<connect gate="G$1" pin="E0" pad="2"/>
<connect gate="G$1" pin="E1" pad="1"/>
<connect gate="G$1" pin="E2" pad="64"/>
<connect gate="G$1" pin="E3" pad="63"/>
<connect gate="G$1" pin="E4" pad="62"/>
<connect gate="G$1" pin="E5" pad="61"/>
<connect gate="G$1" pin="E6" pad="60"/>
<connect gate="G$1" pin="E7" pad="59"/>
<connect gate="G$1" pin="F0" pad="18"/>
<connect gate="G$1" pin="F1" pad="17"/>
<connect gate="G$1" pin="F2" pad="16"/>
<connect gate="G$1" pin="F3" pad="15"/>
<connect gate="G$1" pin="F4" pad="14"/>
<connect gate="G$1" pin="F5" pad="13"/>
<connect gate="G$1" pin="F6" pad="12"/>
<connect gate="G$1" pin="F7" pad="11"/>
<connect gate="G$1" pin="G0" pad="3"/>
<connect gate="G$1" pin="G1/TX2" pad="4"/>
<connect gate="G$1" pin="G2/RX2" pad="5"/>
<connect gate="G$1" pin="G3" pad="6"/>
<connect gate="G$1" pin="G4" pad="8"/>
<connect gate="G$1" pin="G5/!MCLR" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="10"/>
<connect gate="G$1" pin="VDD@2" pad="26"/>
<connect gate="G$1" pin="VDD@3" pad="38"/>
<connect gate="G$1" pin="VDD@4" pad="57"/>
<connect gate="G$1" pin="VSS@1" pad="9"/>
<connect gate="G$1" pin="VSS@2" pad="25"/>
<connect gate="G$1" pin="VSS@3" pad="41"/>
<connect gate="G$1" pin="VSS@4" pad="56"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937-SOT223">
<gates>
<gate name="G$1" symbol="LM2937A-3.3"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="GND"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT232R" prefix="IC">
<description>Source: http://www.ftdichip.com/Documents/DataSheets/DS_FT232R_v104.pdf</description>
<gates>
<gate name="1" symbol="FT232R"/>
</gates>
<devices>
<device name="L" package="SSOP28">
<connects>
<connect gate="1" pin="3V3OUT" pad="17"/>
<connect gate="1" pin="CBUS0" pad="23"/>
<connect gate="1" pin="CBUS1" pad="22"/>
<connect gate="1" pin="CBUS2" pad="13"/>
<connect gate="1" pin="CBUS3" pad="14"/>
<connect gate="1" pin="CBUS4" pad="12"/>
<connect gate="1" pin="CTS#" pad="11"/>
<connect gate="1" pin="DCD#" pad="10"/>
<connect gate="1" pin="DSR#" pad="9"/>
<connect gate="1" pin="DTR#" pad="2"/>
<connect gate="1" pin="GND" pad="7"/>
<connect gate="1" pin="GND@1" pad="18"/>
<connect gate="1" pin="GND@2" pad="21"/>
<connect gate="1" pin="GND@A" pad="25"/>
<connect gate="1" pin="OSCI" pad="27"/>
<connect gate="1" pin="OSCO" pad="28"/>
<connect gate="1" pin="RESET#" pad="19"/>
<connect gate="1" pin="RI#" pad="6"/>
<connect gate="1" pin="RTS#" pad="3"/>
<connect gate="1" pin="RXD" pad="5"/>
<connect gate="1" pin="TEST" pad="26"/>
<connect gate="1" pin="TXD" pad="1"/>
<connect gate="1" pin="USBDM" pad="16"/>
<connect gate="1" pin="USBDP" pad="15"/>
<connect gate="1" pin="VCC" pad="20"/>
<connect gate="1" pin="VCCIO" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="Q" package="QFN32">
<connects>
<connect gate="1" pin="3V3OUT" pad="16"/>
<connect gate="1" pin="CBUS0" pad="22"/>
<connect gate="1" pin="CBUS1" pad="21"/>
<connect gate="1" pin="CBUS2" pad="10"/>
<connect gate="1" pin="CBUS3" pad="11"/>
<connect gate="1" pin="CBUS4" pad="9"/>
<connect gate="1" pin="CTS#" pad="8"/>
<connect gate="1" pin="DCD#" pad="7"/>
<connect gate="1" pin="DSR#" pad="6"/>
<connect gate="1" pin="DTR#" pad="31"/>
<connect gate="1" pin="GND" pad="4"/>
<connect gate="1" pin="GND@1" pad="17"/>
<connect gate="1" pin="GND@2" pad="20"/>
<connect gate="1" pin="GND@A" pad="24"/>
<connect gate="1" pin="OSCI" pad="27"/>
<connect gate="1" pin="OSCO" pad="28"/>
<connect gate="1" pin="RESET#" pad="18"/>
<connect gate="1" pin="RI#" pad="3"/>
<connect gate="1" pin="RTS#" pad="32"/>
<connect gate="1" pin="RXD" pad="2"/>
<connect gate="1" pin="TEST" pad="26"/>
<connect gate="1" pin="TXD" pad="30"/>
<connect gate="1" pin="USBDM" pad="15"/>
<connect gate="1" pin="USBDP" pad="14"/>
<connect gate="1" pin="VCC" pad="19"/>
<connect gate="1" pin="VCCIO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X6" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X6"/>
</gates>
<devices>
<device name="" package="2X06">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X12" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD12"/>
</gates>
<devices>
<device name="" package="1X12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X8" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X8"/>
</gates>
<devices>
<device name="" package="2X08">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2MM" package="HDR-2MM-2X08">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MA07-2" prefix="SV" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MA07-2"/>
</gates>
<devices>
<device name="" package="MA07-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD_CABLE">
<description>Connections to LCD display</description>
<gates>
<gate name="G$1" symbol="DM2023"/>
</gates>
<devices>
<device name="DIL" package="MA07-2">
<connects>
<connect gate="G$1" pin="5.0V" pad="2"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="EN" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="V0" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="2X07">
<connects>
<connect gate="G$1" pin="5.0V" pad="2"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="EN" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="V0" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A4-SMALL-DOCFIELD" prefix="FRAME">
<description>&lt;b&gt;FRAME&lt;/b&gt;&lt;p&gt;
DIN A4, with small doc field</description>
<gates>
<gate name="/1" symbol="DOCSMAL-L"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DOCSMAL-L" prefix="FRAME">
<gates>
<gate name="G$1" symbol="DOCSMAL-L"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PORT2" prefix="PORT">
<description>&lt;b&gt;PORT SYMBOL&lt;/b&gt;&lt;p&gt;
 for net name (2 characters)</description>
<gates>
<gate name="G$1" symbol="PORTOUT"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PORT3" prefix="PORT">
<description>&lt;b&gt;PORT SYMBOL&lt;/b&gt;&lt;p&gt;
 for net name (3 characters)</description>
<gates>
<gate name="G$1" symbol="PORT3"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PORT" prefix="PORT">
<gates>
<gate name="G$1" symbol="PORTBI"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PORTIN">
<gates>
<gate name="G$1" symbol="PORTIN"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PORTOUT">
<gates>
<gate name="G$1" symbol="PORTOUT"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PORTBI">
<gates>
<gate name="G$1" symbol="PORTBI"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB" prefix="X" uservalue="yes">
<description>&lt;b&gt;USB Connectors&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="-MB-S" package="USB-MB-S">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-H" package="USB-A-H">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-B-H" package="USB-B-H">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-S" package="USB-A-S">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MB-H" package="USB-MB-H">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-HU" package="USB-A-HU">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-B-S" package="USB-B-SMT">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VUSB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-B-V" package="USB-BV2">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB-SHIELDED">
<gates>
<gate name="G$1" symbol="USB-SHIELDED"/>
</gates>
<devices>
<device name="" package="USB-B-H">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="GND@2"/>
<connect gate="G$1" pin="GND@2" pad="GND@1"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LD1117">
<description>SMT voltage regulator</description>
<gates>
<gate name="G$1" symbol="LM2937-3.3"/>
</gates>
<devices>
<device name="D" package="DPAK">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LETTER_L" prefix="FRAME">
<description>&lt;b&gt;FRAME&lt;/b&gt;&lt;p&gt;
LETTER landscape</description>
<gates>
<gate name="G$1" symbol="LETTER_L"/>
<gate name="G$2" symbol="DOCFIELD"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GENERICSSOP28">
<gates>
<gate name="G$1" symbol="GENERIC28SSOP"/>
</gates>
<devices>
<device name="" package="SSOP28">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT86RF230">
<gates>
<gate name="G$1" symbol="AT86RF230"/>
</gates>
<devices>
<device name="" package="32QN1">
<connects>
<connect gate="G$1" pin="AVDD" pad="29"/>
<connect gate="G$1" pin="AVSS@1" pad="1"/>
<connect gate="G$1" pin="AVSS@2" pad="2"/>
<connect gate="G$1" pin="AVSS@3" pad="3"/>
<connect gate="G$1" pin="AVSS@4" pad="6"/>
<connect gate="G$1" pin="AVSS@5" pad="27"/>
<connect gate="G$1" pin="AVSS@6" pad="30"/>
<connect gate="G$1" pin="AVSS@7" pad="31"/>
<connect gate="G$1" pin="AVSS@8" pad="32"/>
<connect gate="G$1" pin="CLKM" pad="17"/>
<connect gate="G$1" pin="DEVDD" pad="15"/>
<connect gate="G$1" pin="DVDD@1" pad="13"/>
<connect gate="G$1" pin="DVDD@2" pad="14"/>
<connect gate="G$1" pin="DVSS@1" pad="9"/>
<connect gate="G$1" pin="DVSS@2" pad="10"/>
<connect gate="G$1" pin="DVSS@3" pad="12"/>
<connect gate="G$1" pin="DVSS@4" pad="16"/>
<connect gate="G$1" pin="DVSS@5" pad="18"/>
<connect gate="G$1" pin="DVSS@6" pad="21"/>
<connect gate="G$1" pin="EVDD" pad="28"/>
<connect gate="G$1" pin="IRQ" pad="24"/>
<connect gate="G$1" pin="MISO" pad="20"/>
<connect gate="G$1" pin="MOSI" pad="22"/>
<connect gate="G$1" pin="RFN" pad="5"/>
<connect gate="G$1" pin="RFP" pad="4"/>
<connect gate="G$1" pin="RST/" pad="8"/>
<connect gate="G$1" pin="SCLK" pad="19"/>
<connect gate="G$1" pin="SEL/" pad="23"/>
<connect gate="G$1" pin="SLP" pad="11"/>
<connect gate="G$1" pin="TST" pad="7"/>
<connect gate="G$1" pin="XTAL1" pad="25"/>
<connect gate="G$1" pin="XTAL2" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1" package="32QN1R1">
<connects>
<connect gate="G$1" pin="AVDD" pad="29"/>
<connect gate="G$1" pin="AVSS@1" pad="1"/>
<connect gate="G$1" pin="AVSS@2" pad="2"/>
<connect gate="G$1" pin="AVSS@3" pad="3"/>
<connect gate="G$1" pin="AVSS@4" pad="6"/>
<connect gate="G$1" pin="AVSS@5" pad="27"/>
<connect gate="G$1" pin="AVSS@6" pad="30"/>
<connect gate="G$1" pin="AVSS@7" pad="31"/>
<connect gate="G$1" pin="AVSS@8" pad="32"/>
<connect gate="G$1" pin="CLKM" pad="17"/>
<connect gate="G$1" pin="DEVDD" pad="15"/>
<connect gate="G$1" pin="DVDD@1" pad="13"/>
<connect gate="G$1" pin="DVDD@2" pad="14"/>
<connect gate="G$1" pin="DVSS@1" pad="9"/>
<connect gate="G$1" pin="DVSS@2" pad="10"/>
<connect gate="G$1" pin="DVSS@3" pad="12"/>
<connect gate="G$1" pin="DVSS@4" pad="16"/>
<connect gate="G$1" pin="DVSS@5" pad="18"/>
<connect gate="G$1" pin="DVSS@6" pad="21"/>
<connect gate="G$1" pin="EVDD" pad="28"/>
<connect gate="G$1" pin="IRQ" pad="24"/>
<connect gate="G$1" pin="MISO" pad="20"/>
<connect gate="G$1" pin="MOSI" pad="22"/>
<connect gate="G$1" pin="RFN" pad="5"/>
<connect gate="G$1" pin="RFP" pad="4"/>
<connect gate="G$1" pin="RST/" pad="8"/>
<connect gate="G$1" pin="SCLK" pad="19"/>
<connect gate="G$1" pin="SEL/" pad="23"/>
<connect gate="G$1" pin="SLP" pad="11"/>
<connect gate="G$1" pin="TST" pad="7"/>
<connect gate="G$1" pin="XTAL1" pad="25"/>
<connect gate="G$1" pin="XTAL2" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XTAL4025">
<gates>
<gate name="G$1" symbol="XTAL4025"/>
</gates>
<devices>
<device name="" package="XTAL4025">
<connects>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="4"/>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT86RF230R1">
<gates>
<gate name="G$1" symbol="AT86RF230R1"/>
</gates>
<devices>
<device name="" package="32QN1R1">
<connects>
<connect gate="G$1" pin="AVDD" pad="29"/>
<connect gate="G$1" pin="AVSS@0" pad="AVSS@0"/>
<connect gate="G$1" pin="AVSS@1" pad="1"/>
<connect gate="G$1" pin="AVSS@2" pad="2"/>
<connect gate="G$1" pin="AVSS@3" pad="3"/>
<connect gate="G$1" pin="AVSS@4" pad="6"/>
<connect gate="G$1" pin="AVSS@5" pad="27"/>
<connect gate="G$1" pin="AVSS@6" pad="30"/>
<connect gate="G$1" pin="AVSS@7" pad="31"/>
<connect gate="G$1" pin="AVSS@8" pad="32"/>
<connect gate="G$1" pin="CLKM" pad="17"/>
<connect gate="G$1" pin="DEVDD" pad="15"/>
<connect gate="G$1" pin="DVDD@1" pad="13"/>
<connect gate="G$1" pin="DVDD@2" pad="14"/>
<connect gate="G$1" pin="DVSS@1" pad="9"/>
<connect gate="G$1" pin="DVSS@2" pad="10"/>
<connect gate="G$1" pin="DVSS@3" pad="12"/>
<connect gate="G$1" pin="DVSS@4" pad="16"/>
<connect gate="G$1" pin="DVSS@5" pad="18"/>
<connect gate="G$1" pin="DVSS@6" pad="21"/>
<connect gate="G$1" pin="EVDD" pad="28"/>
<connect gate="G$1" pin="IRQ" pad="24"/>
<connect gate="G$1" pin="MISO" pad="20"/>
<connect gate="G$1" pin="MOSI" pad="22"/>
<connect gate="G$1" pin="RFN" pad="5"/>
<connect gate="G$1" pin="RFP" pad="4"/>
<connect gate="G$1" pin="RST/" pad="8"/>
<connect gate="G$1" pin="SCLK" pad="19"/>
<connect gate="G$1" pin="SEL/" pad="23"/>
<connect gate="G$1" pin="SLP" pad="11"/>
<connect gate="G$1" pin="TST" pad="7"/>
<connect gate="G$1" pin="XTAL1" pad="25"/>
<connect gate="G$1" pin="XTAL2" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIM_US-" prefix="R" uservalue="yes">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="POT_US-"/>
</gates>
<devices>
<device name="PT-10" package="PT-10">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PT-10S" package="PT-10S">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PT-SPIN" package="PT-SPIN">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B25P" package="B25P">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B25U" package="B25U">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B25V" package="B25V">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B25X" package="B25X">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B64W" package="B64W">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B64Y" package="B64Y">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B90P" package="SP19L">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CA6H" package="CA6H">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CA6V" package="CA6V">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CA9H" package="CA9H">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CA9V" package="CA9V">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CA14V" package="CA14V">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CA14H" package="CA14H">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CT6" package="CT6">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ECP10P" package="ECP10P">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ECP10S" package="ECP10S">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LI10" package="LI10">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LI15" package="LI15">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RJ6" package="RJ6">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RJ6S" package="RJ6S">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RJ9W" package="RJ9W">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RS3" package="RS3">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S43P" package="SP19L">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S63P" package="S63P">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S63S" package="S63S">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S63X" package="S63X">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S64W" package="S64W">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S64Y" package="S64Y">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S75H" package="S75H">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S75P" package="S75P">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SP19L" package="SP19L">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ST10" package="ST10">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ST15" package="ST15">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T189" package="SP19LKN">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PT10" package="PT-10">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PT10S" package="PT-10S">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTSPIN" package="PT-SPIN">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TC73" package="SMT-POT-TC73">
<connects>
<connect gate="1" pin="A" pad="P1"/>
<connect gate="1" pin="E" pad="P3"/>
<connect gate="1" pin="S" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIMPOT-SMT" prefix="POT">
<gates>
<gate name="G$1" symbol="POT_US-"/>
</gates>
<devices>
<device name="TC73" package="SMT-POT-TC73">
<connects>
<connect gate="G$1" pin="A" pad="P1"/>
<connect gate="G$1" pin="E" pad="P3"/>
<connect gate="G$1" pin="S" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BRIDGE-DRIVER-3941">
<gates>
<gate name="G$1" symbol="BRIDGE-DRIVER3941"/>
</gates>
<devices>
<device name="" package="TSSOP-3-28-L">
<connects>
<connect gate="G$1" pin="CA" pad="9"/>
<connect gate="G$1" pin="CB" pad="6"/>
<connect gate="G$1" pin="CP1" pad="16"/>
<connect gate="G$1" pin="CP2" pad="15"/>
<connect gate="G$1" pin="FF1" pad="25"/>
<connect gate="G$1" pin="FF2" pad="26"/>
<connect gate="G$1" pin="GHA" pad="10"/>
<connect gate="G$1" pin="GHB" pad="5"/>
<connect gate="G$1" pin="GLA" pad="12"/>
<connect gate="G$1" pin="GLB" pad="3"/>
<connect gate="G$1" pin="GND@1" pad="17"/>
<connect gate="G$1" pin="GND@2" pad="18"/>
<connect gate="G$1" pin="LSS" pad="2"/>
<connect gate="G$1" pin="PAD" pad="29"/>
<connect gate="G$1" pin="PHASE" pad="19"/>
<connect gate="G$1" pin="PWMH" pad="23"/>
<connect gate="G$1" pin="PWML" pad="22"/>
<connect gate="G$1" pin="RDEAD" pad="27"/>
<connect gate="G$1" pin="RESET" pad="24"/>
<connect gate="G$1" pin="SA" pad="11"/>
<connect gate="G$1" pin="SB" pad="4"/>
<connect gate="G$1" pin="SR" pad="21"/>
<connect gate="G$1" pin="V5" pad="20"/>
<connect gate="G$1" pin="VBB@1" pad="13"/>
<connect gate="G$1" pin="VBB@2" pad="14"/>
<connect gate="G$1" pin="VDR" pad="1"/>
<connect gate="G$1" pin="VDSTH" pad="28"/>
<connect gate="G$1" pin="VREG@1" pad="7"/>
<connect gate="G$1" pin="VREG@2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="N-MOSFET">
<gates>
<gate name="G$1" symbol="P-MOSFET-N"/>
</gates>
<devices>
<device name="DPAK" package="DPAK">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D2PAK" package="D2PAK(TO-263)">
<connects>
<connect gate="G$1" pin="D" pad="P2"/>
<connect gate="G$1" pin="G" pad="P1"/>
<connect gate="G$1" pin="S" pad="P3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO-220" package="TO220(V)">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1252" prefix="IC">
<description>&lt;b&gt;Positive-Regulated Charge Pump (3.3x5.0)&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="MCP1252/3"/>
</gates>
<devices>
<device name="" package="MSOP8">
<connects>
<connect gate="X" pin="C+" pad="6"/>
<connect gate="X" pin="C-" pad="5"/>
<connect gate="X" pin="GND" pad="4"/>
<connect gate="X" pin="PGOOD" pad="1"/>
<connect gate="X" pin="SELECT" pad="8"/>
<connect gate="X" pin="SHDN#" pad="7"/>
<connect gate="X" pin="VIN" pad="3"/>
<connect gate="X" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD_CABLE_CF">
<gates>
<gate name="G$1" symbol="CF-LCD-128"/>
</gates>
<devices>
<device name="" package="2X09">
<connects>
<connect gate="G$1" pin="5.0V" pad="2"/>
<connect gate="G$1" pin="CS/" pad="5"/>
<connect gate="G$1" pin="DB0" pad="11"/>
<connect gate="G$1" pin="DB1" pad="12"/>
<connect gate="G$1" pin="DB2" pad="13"/>
<connect gate="G$1" pin="DB3" pad="14"/>
<connect gate="G$1" pin="DB4" pad="15"/>
<connect gate="G$1" pin="DB5" pad="16"/>
<connect gate="G$1" pin="DB6" pad="17"/>
<connect gate="G$1" pin="DB7" pad="18"/>
<connect gate="G$1" pin="EN" pad="10"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="R/W" pad="9"/>
<connect gate="G$1" pin="RESET/" pad="7"/>
<connect gate="G$1" pin="RS" pad="8"/>
<connect gate="G$1" pin="V0" pad="3"/>
<connect gate="G$1" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X9" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X9"/>
</gates>
<devices>
<device name="" package="2X09">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZIG-DAUGHTER">
<gates>
<gate name="G$1" symbol="ZIG-DAUGHTER"/>
</gates>
<devices>
<device name="" package="2X05">
<connects>
<connect gate="G$1" pin="!RST" pad="3"/>
<connect gate="G$1" pin="!SEL" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IRQ" pad="5"/>
<connect gate="G$1" pin="MISO" pad="8"/>
<connect gate="G$1" pin="MOSI" pad="7"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="SCK" pad="9"/>
<connect gate="G$1" pin="SLP" pad="10"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A" package="ZIG-DAUGHTER">
<connects>
<connect gate="G$1" pin="!RST" pad="3"/>
<connect gate="G$1" pin="!SEL" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IRQ" pad="5"/>
<connect gate="G$1" pin="MISO" pad="8"/>
<connect gate="G$1" pin="MOSI" pad="7"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="SCK" pad="9"/>
<connect gate="G$1" pin="SLP" pad="10"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B" package="ZIG-DAUGHTER-SMALL">
<connects>
<connect gate="G$1" pin="!RST" pad="3"/>
<connect gate="G$1" pin="!SEL" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IRQ" pad="5"/>
<connect gate="G$1" pin="MISO" pad="8"/>
<connect gate="G$1" pin="MOSI" pad="7"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="SCK" pad="9"/>
<connect gate="G$1" pin="SLP" pad="10"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2TERMSCREWBLOCK">
<gates>
<gate name="G$1" symbol="2-TERM-BLOCK"/>
</gates>
<devices>
<device name="" package="2TERMINALSTRIP">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TERMBLOCK-4">
<gates>
<gate name="G$1" symbol="TERMBLOCK-4"/>
</gates>
<devices>
<device name="5.08MM" package="TERMBLOCK-5.08-4">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10MM" package="TERMBLOCK-10.0-4">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD-MULTI" prefix="LCD">
<gates>
<gate name="G$1" symbol="LCD-MULTI"/>
</gates>
<devices>
<device name="" package="LCD-MULTI">
<connects>
<connect gate="G$1" pin="5.0V" pad="2"/>
<connect gate="G$1" pin="BL+" pad="20"/>
<connect gate="G$1" pin="BL-" pad="19"/>
<connect gate="G$1" pin="CS/" pad="18"/>
<connect gate="G$1" pin="D-ON" pad="15"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="EN" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RESET/" pad="16"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="V0" pad="3"/>
<connect gate="G$1" pin="VEE" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R-US0805RMS" prefix="R">
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="RMS" package="R0805RMS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X2" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X2"/>
</gates>
<devices>
<device name="" package="2X02">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1N5638" prefix="D">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
schottky</description>
<gates>
<gate name="1" symbol="SCHOTTKY"/>
</gates>
<devices>
<device name="" package="DO13M">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE-SHOTKEY" prefix="D">
<gates>
<gate name="G$1" symbol="SCHOTTKY"/>
</gates>
<devices>
<device name="SMA" package="SMA">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMB" package="SMB">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMC" package="SMC">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DO41" package="DO41Z10">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOD123" package="SOD123">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BALUN">
<gates>
<gate name="G$1" symbol="BALUN"/>
</gates>
<devices>
<device name="" package="BALUN-0805">
<connects>
<connect gate="G$1" pin="B1" pad="P3"/>
<connect gate="G$1" pin="B2" pad="P4"/>
<connect gate="G$1" pin="GND@1" pad="P2"/>
<connect gate="G$1" pin="GND@2" pad="P5"/>
<connect gate="G$1" pin="NC" pad="P6"/>
<connect gate="G$1" pin="UB" pad="P1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F67J11">
<gates>
<gate name="G$1" symbol="PIC18F67J11"/>
</gates>
<devices>
<device name="" package="TQFP64-10X10RMS">
<connects>
<connect gate="G$1" pin="A0" pad="24"/>
<connect gate="G$1" pin="A1" pad="23"/>
<connect gate="G$1" pin="A2" pad="22"/>
<connect gate="G$1" pin="A3" pad="21"/>
<connect gate="G$1" pin="A4" pad="28"/>
<connect gate="G$1" pin="A5" pad="27"/>
<connect gate="G$1" pin="A6/OSCO" pad="40"/>
<connect gate="G$1" pin="A7/OSCI" pad="39"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="B0/INT0" pad="48"/>
<connect gate="G$1" pin="B1/INT1" pad="47"/>
<connect gate="G$1" pin="B2/INT2" pad="46"/>
<connect gate="G$1" pin="B3/INT3" pad="45"/>
<connect gate="G$1" pin="B4" pad="44"/>
<connect gate="G$1" pin="B5/PGM" pad="43"/>
<connect gate="G$1" pin="B6/PGC" pad="42"/>
<connect gate="G$1" pin="B7/PGD" pad="37"/>
<connect gate="G$1" pin="C0" pad="30"/>
<connect gate="G$1" pin="C1" pad="29"/>
<connect gate="G$1" pin="C2" pad="33"/>
<connect gate="G$1" pin="C3/SCLK1" pad="34"/>
<connect gate="G$1" pin="C4/SDI1" pad="35"/>
<connect gate="G$1" pin="C5/SDO1" pad="36"/>
<connect gate="G$1" pin="C6/TX1" pad="31"/>
<connect gate="G$1" pin="C7/RX1" pad="32"/>
<connect gate="G$1" pin="D0" pad="58"/>
<connect gate="G$1" pin="D1" pad="55"/>
<connect gate="G$1" pin="D2" pad="54"/>
<connect gate="G$1" pin="D3" pad="53"/>
<connect gate="G$1" pin="D4/SDO2" pad="52"/>
<connect gate="G$1" pin="D5/SDI2" pad="51"/>
<connect gate="G$1" pin="D6/SCLK2" pad="50"/>
<connect gate="G$1" pin="D7" pad="49"/>
<connect gate="G$1" pin="E0" pad="2"/>
<connect gate="G$1" pin="E1" pad="1"/>
<connect gate="G$1" pin="E2" pad="64"/>
<connect gate="G$1" pin="E3" pad="63"/>
<connect gate="G$1" pin="E4" pad="62"/>
<connect gate="G$1" pin="E5" pad="61"/>
<connect gate="G$1" pin="E6" pad="60"/>
<connect gate="G$1" pin="E7" pad="59"/>
<connect gate="G$1" pin="ENVREG" pad="18"/>
<connect gate="G$1" pin="F1" pad="17"/>
<connect gate="G$1" pin="F2" pad="16"/>
<connect gate="G$1" pin="F3" pad="15"/>
<connect gate="G$1" pin="F4" pad="14"/>
<connect gate="G$1" pin="F5" pad="13"/>
<connect gate="G$1" pin="F6" pad="12"/>
<connect gate="G$1" pin="F7" pad="11"/>
<connect gate="G$1" pin="G0" pad="3"/>
<connect gate="G$1" pin="G1/TX2" pad="4"/>
<connect gate="G$1" pin="G2/RX2" pad="5"/>
<connect gate="G$1" pin="G3" pad="6"/>
<connect gate="G$1" pin="G4" pad="8"/>
<connect gate="G$1" pin="MCLR" pad="7"/>
<connect gate="G$1" pin="VCAP" pad="10"/>
<connect gate="G$1" pin="VDD@2" pad="26"/>
<connect gate="G$1" pin="VDD@3" pad="38"/>
<connect gate="G$1" pin="VDD@4" pad="57"/>
<connect gate="G$1" pin="VSS@1" pad="9"/>
<connect gate="G$1" pin="VSS@2" pad="25"/>
<connect gate="G$1" pin="VSS@3" pad="41"/>
<connect gate="G$1" pin="VSS@4" pad="56"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONNECTOR-1X5">
<gates>
<gate name="G$1" symbol="CONNECTOR-1X5"/>
</gates>
<devices>
<device name="MINI-JR-RA" package="MOLEX-MINIFIT-RA-1-5">
<connects>
<connect gate="G$1" pin="P$1" pad="P1"/>
<connect gate="G$1" pin="P$2" pad="P2"/>
<connect gate="G$1" pin="P$3" pad="P3"/>
<connect gate="G$1" pin="P$4" pad="P4"/>
<connect gate="G$1" pin="P$5" pad="P5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="18F4620-SQ" prefix="IC">
<gates>
<gate name="G$1" symbol="18F4620-SQ"/>
</gates>
<devices>
<device name="" package="TQFP44">
<connects>
<connect gate="G$1" pin="!MCLR" pad="18"/>
<connect gate="G$1" pin="NC@1" pad="12"/>
<connect gate="G$1" pin="NC@2" pad="13"/>
<connect gate="G$1" pin="NC@3" pad="33"/>
<connect gate="G$1" pin="NC@4" pad="34"/>
<connect gate="G$1" pin="RA0/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2" pad="21"/>
<connect gate="G$1" pin="RA3/AN3" pad="22"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="23"/>
<connect gate="G$1" pin="RA5/AN4" pad="24"/>
<connect gate="G$1" pin="RA6/OX2" pad="31"/>
<connect gate="G$1" pin="RA7/OX1" pad="30"/>
<connect gate="G$1" pin="RB0" pad="8"/>
<connect gate="G$1" pin="RB1" pad="9"/>
<connect gate="G$1" pin="RB2" pad="10"/>
<connect gate="G$1" pin="RB3/PGM" pad="11"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RB6/PGC" pad="16"/>
<connect gate="G$1" pin="RB7/PGD" pad="17"/>
<connect gate="G$1" pin="RC0" pad="32"/>
<connect gate="G$1" pin="RC1" pad="35"/>
<connect gate="G$1" pin="RC2" pad="36"/>
<connect gate="G$1" pin="RC3/SCK" pad="37"/>
<connect gate="G$1" pin="RC4/MISO" pad="42"/>
<connect gate="G$1" pin="RC5/MOSI" pad="43"/>
<connect gate="G$1" pin="RC6/TX" pad="44"/>
<connect gate="G$1" pin="RC7/RX" pad="1"/>
<connect gate="G$1" pin="RD0" pad="38"/>
<connect gate="G$1" pin="RD1" pad="39"/>
<connect gate="G$1" pin="RD2" pad="40"/>
<connect gate="G$1" pin="RD3" pad="41"/>
<connect gate="G$1" pin="RD4" pad="2"/>
<connect gate="G$1" pin="RD5" pad="3"/>
<connect gate="G$1" pin="RD6" pad="4"/>
<connect gate="G$1" pin="RD7" pad="5"/>
<connect gate="G$1" pin="RE0/AN5" pad="25"/>
<connect gate="G$1" pin="RE1/AN6" pad="26"/>
<connect gate="G$1" pin="RE2/AN7" pad="27"/>
<connect gate="G$1" pin="VDD@1" pad="7"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
<connect gate="G$1" pin="VSS@2" pad="29"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C" package="TQFP44C">
<connects>
<connect gate="G$1" pin="!MCLR" pad="18"/>
<connect gate="G$1" pin="NC@1" pad="12"/>
<connect gate="G$1" pin="NC@2" pad="13"/>
<connect gate="G$1" pin="NC@3" pad="33"/>
<connect gate="G$1" pin="NC@4" pad="34"/>
<connect gate="G$1" pin="RA0/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2" pad="21"/>
<connect gate="G$1" pin="RA3/AN3" pad="22"/>
<connect gate="G$1" pin="RA4/T0CKI" pad="23"/>
<connect gate="G$1" pin="RA5/AN4" pad="24"/>
<connect gate="G$1" pin="RA6/OX2" pad="31"/>
<connect gate="G$1" pin="RA7/OX1" pad="30"/>
<connect gate="G$1" pin="RB0" pad="8"/>
<connect gate="G$1" pin="RB1" pad="9"/>
<connect gate="G$1" pin="RB2" pad="10"/>
<connect gate="G$1" pin="RB3/PGM" pad="11"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RB6/PGC" pad="16"/>
<connect gate="G$1" pin="RB7/PGD" pad="17"/>
<connect gate="G$1" pin="RC0" pad="32"/>
<connect gate="G$1" pin="RC1" pad="35"/>
<connect gate="G$1" pin="RC2" pad="36"/>
<connect gate="G$1" pin="RC3/SCK" pad="37"/>
<connect gate="G$1" pin="RC4/MISO" pad="42"/>
<connect gate="G$1" pin="RC5/MOSI" pad="43"/>
<connect gate="G$1" pin="RC6/TX" pad="44"/>
<connect gate="G$1" pin="RC7/RX" pad="1"/>
<connect gate="G$1" pin="RD0" pad="38"/>
<connect gate="G$1" pin="RD1" pad="39"/>
<connect gate="G$1" pin="RD2" pad="40"/>
<connect gate="G$1" pin="RD3" pad="41"/>
<connect gate="G$1" pin="RD4" pad="2"/>
<connect gate="G$1" pin="RD5" pad="3"/>
<connect gate="G$1" pin="RD6" pad="4"/>
<connect gate="G$1" pin="RD7" pad="5"/>
<connect gate="G$1" pin="RE0/AN5" pad="25"/>
<connect gate="G$1" pin="RE1/AN6" pad="26"/>
<connect gate="G$1" pin="RE2/AN7" pad="27"/>
<connect gate="G$1" pin="VDD@1" pad="7"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
<connect gate="G$1" pin="VSS@2" pad="29"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="N-MOSFET-MED" prefix="Q">
<description>&lt;b&gt;N-CHANNEL MOS FET&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="N-MOS"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD-W/BL" prefix="CON">
<gates>
<gate name="G$1" symbol="LCD-W/BL"/>
</gates>
<devices>
<device name="2X0.1HEADER" package="2X08">
<connects>
<connect gate="G$1" pin="5.0V" pad="2"/>
<connect gate="G$1" pin="BL+" pad="15"/>
<connect gate="G$1" pin="BL-" pad="16"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="EN" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="R/!W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="V0" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2X0.1-FLIP" package="2X08">
<connects>
<connect gate="G$1" pin="5.0V" pad="1"/>
<connect gate="G$1" pin="BL+" pad="16"/>
<connect gate="G$1" pin="BL-" pad="15"/>
<connect gate="G$1" pin="DB0" pad="8"/>
<connect gate="G$1" pin="DB1" pad="7"/>
<connect gate="G$1" pin="DB2" pad="10"/>
<connect gate="G$1" pin="DB3" pad="9"/>
<connect gate="G$1" pin="DB4" pad="12"/>
<connect gate="G$1" pin="DB5" pad="11"/>
<connect gate="G$1" pin="DB6" pad="14"/>
<connect gate="G$1" pin="DB7" pad="13"/>
<connect gate="G$1" pin="EN" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="R/!W" pad="6"/>
<connect gate="G$1" pin="RS" pad="3"/>
<connect gate="G$1" pin="V0" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IDC" package="IDC-NL-ASSMAN-NL">
<connects>
<connect gate="G$1" pin="5.0V" pad="2"/>
<connect gate="G$1" pin="BL+" pad="15"/>
<connect gate="G$1" pin="BL-" pad="16"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="EN" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="R/!W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="V0" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DF11-16">
<gates>
<gate name="G$1" symbol="DF11-CONNECTOR"/>
</gates>
<devices>
<device name="THV" package="DF11-TH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMV" package="DF-11-SM-16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CFA635LCD" prefix="CON">
<gates>
<gate name="G$1" symbol="CFA635-LCD"/>
</gates>
<devices>
<device name="" package="DF11-TH">
<connects>
<connect gate="G$1" pin="+5V" pad="16"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="LCD-RX" pad="1"/>
<connect gate="G$1" pin="LCD-TX" pad="2"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HB3-INTERFACE" prefix="CON" uservalue="yes">
<gates>
<gate name="G$1" symbol="HB3-INTERFACE"/>
</gates>
<devices>
<device name="V" package="MOLEX-34045-8">
<connects>
<connect gate="G$1" pin="FF1" pad="2"/>
<connect gate="G$1" pin="FF2" pad="5"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="PHASE" pad="8"/>
<connect gate="G$1" pin="PWMH" pad="3"/>
<connect gate="G$1" pin="PWML" pad="7"/>
<connect gate="G$1" pin="RESET" pad="6"/>
<connect gate="G$1" pin="SR" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA" package="MOLEX-34045-RA-8">
<connects>
<connect gate="G$1" pin="FF1" pad="2"/>
<connect gate="G$1" pin="FF2" pad="5"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="PHASE" pad="8"/>
<connect gate="G$1" pin="PWMH" pad="3"/>
<connect gate="G$1" pin="PWML" pad="7"/>
<connect gate="G$1" pin="RESET" pad="6"/>
<connect gate="G$1" pin="SR" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AR86RF231">
<gates>
<gate name="G$1" symbol="AT86RF231"/>
</gates>
<devices>
<device name="" package="32QN1R1">
<connects>
<connect gate="G$1" pin="AVDD" pad="29"/>
<connect gate="G$1" pin="AVSS@0" pad="AVSS@0"/>
<connect gate="G$1" pin="AVSS@3" pad="3"/>
<connect gate="G$1" pin="AVSS@4" pad="6"/>
<connect gate="G$1" pin="AVSS@5" pad="27"/>
<connect gate="G$1" pin="AVSS@6" pad="30"/>
<connect gate="G$1" pin="AVSS@7" pad="31"/>
<connect gate="G$1" pin="AVSS@8" pad="32"/>
<connect gate="G$1" pin="CLKM" pad="17"/>
<connect gate="G$1" pin="DEVDD" pad="15"/>
<connect gate="G$1" pin="DIG1" pad="9"/>
<connect gate="G$1" pin="DIG2" pad="10"/>
<connect gate="G$1" pin="DIG3" pad="1"/>
<connect gate="G$1" pin="DIG4" pad="2"/>
<connect gate="G$1" pin="DVDD@1" pad="13"/>
<connect gate="G$1" pin="DVDD@2" pad="14"/>
<connect gate="G$1" pin="DVSS@1" pad="7"/>
<connect gate="G$1" pin="DVSS@3" pad="12"/>
<connect gate="G$1" pin="DVSS@4" pad="16"/>
<connect gate="G$1" pin="DVSS@5" pad="18"/>
<connect gate="G$1" pin="DVSS@6" pad="21"/>
<connect gate="G$1" pin="EVDD" pad="28"/>
<connect gate="G$1" pin="IRQ" pad="24"/>
<connect gate="G$1" pin="MISO" pad="20"/>
<connect gate="G$1" pin="MOSI" pad="22"/>
<connect gate="G$1" pin="RFN" pad="5"/>
<connect gate="G$1" pin="RFP" pad="4"/>
<connect gate="G$1" pin="RST/" pad="8"/>
<connect gate="G$1" pin="SCLK" pad="19"/>
<connect gate="G$1" pin="SEL/" pad="23"/>
<connect gate="G$1" pin="SLP" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="25"/>
<connect gate="G$1" pin="XTAL2" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DUAL-N-MOSFET" prefix="Q">
<gates>
<gate name="G1" symbol="N-MOS"/>
<gate name="G2" symbol="N-MOS"/>
</gates>
<devices>
<device name="" package="SOT363_PHILIPS">
<connects>
<connect gate="G1" pin="D" pad="3"/>
<connect gate="G1" pin="G" pad="5"/>
<connect gate="G1" pin="S" pad="4"/>
<connect gate="G2" pin="D" pad="6"/>
<connect gate="G2" pin="G" pad="2"/>
<connect gate="G2" pin="S" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZENER-SMT" prefix="D" uservalue="yes">
<gates>
<gate name="G$1" symbol="ZD"/>
</gates>
<devices>
<device name="SMA" package="SMA">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMB" package="SMB">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="18F2520">
<gates>
<gate name="G$1" symbol="18F2520"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="A3" pad="5"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="10"/>
<connect gate="G$1" pin="A7" pad="9"/>
<connect gate="G$1" pin="B0" pad="21"/>
<connect gate="G$1" pin="B1" pad="22"/>
<connect gate="G$1" pin="B2" pad="23"/>
<connect gate="G$1" pin="B3" pad="24"/>
<connect gate="G$1" pin="B4" pad="25"/>
<connect gate="G$1" pin="B5" pad="26"/>
<connect gate="G$1" pin="B6" pad="27"/>
<connect gate="G$1" pin="B7" pad="28"/>
<connect gate="G$1" pin="C0" pad="11"/>
<connect gate="G$1" pin="C1" pad="12"/>
<connect gate="G$1" pin="C2" pad="13"/>
<connect gate="G$1" pin="C3" pad="14"/>
<connect gate="G$1" pin="C4" pad="15"/>
<connect gate="G$1" pin="C5" pad="16"/>
<connect gate="G$1" pin="C6" pad="17"/>
<connect gate="G$1" pin="C7" pad="18"/>
<connect gate="G$1" pin="E3/MCLR" pad="1"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BS170-NMOS" prefix="Q">
<gates>
<gate name="G$1" symbol="N-MOS"/>
</gates>
<devices>
<device name="" package="TO92">
<connects>
<connect gate="G$1" pin="D" pad="1"/>
<connect gate="G$1" pin="G" pad="2"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IO-CABLE-RMS" prefix="CON">
<gates>
<gate name="G$1" symbol="IOCONNECTOR"/>
</gates>
<devices>
<device name="NL" package="IDC-NL-ASSMAN-NL">
<connects>
<connect gate="G$1" pin="D0/K1" pad="3"/>
<connect gate="G$1" pin="D1/K2" pad="4"/>
<connect gate="G$1" pin="D2/K3" pad="5"/>
<connect gate="G$1" pin="D3/K4" pad="6"/>
<connect gate="G$1" pin="EN" pad="8"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="K5" pad="10"/>
<connect gate="G$1" pin="L1" pad="11"/>
<connect gate="G$1" pin="L2" pad="12"/>
<connect gate="G$1" pin="L3" pad="13"/>
<connect gate="G$1" pin="L4" pad="14"/>
<connect gate="G$1" pin="R/!W" pad="9"/>
<connect gate="G$1" pin="RS" pad="7"/>
<connect gate="G$1" pin="RXIN" pad="1"/>
<connect gate="G$1" pin="TXOUT" pad="2"/>
<connect gate="G$1" pin="VDD" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FL" package="ICD-FL">
<connects>
<connect gate="G$1" pin="D0/K1" pad="3"/>
<connect gate="G$1" pin="D1/K2" pad="4"/>
<connect gate="G$1" pin="D2/K3" pad="5"/>
<connect gate="G$1" pin="D3/K4" pad="6"/>
<connect gate="G$1" pin="EN" pad="8"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="K5" pad="10"/>
<connect gate="G$1" pin="L1" pad="11"/>
<connect gate="G$1" pin="L2" pad="12"/>
<connect gate="G$1" pin="L3" pad="13"/>
<connect gate="G$1" pin="L4" pad="14"/>
<connect gate="G$1" pin="R/!W" pad="9"/>
<connect gate="G$1" pin="RS" pad="7"/>
<connect gate="G$1" pin="RXIN" pad="1"/>
<connect gate="G$1" pin="TXOUT" pad="2"/>
<connect gate="G$1" pin="VDD" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FLEX-16-1MM" prefix="CON">
<gates>
<gate name="G$1" symbol="FLEXCON-16"/>
</gates>
<devices>
<device name="" package="FFC-1MMTHRA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AMP2X2" prefix="CON">
<gates>
<gate name="G$1" symbol="CON2X2"/>
</gates>
<devices>
<device name=".1IN" package="AMP2X2-.1IN">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AMP2X3" prefix="CON">
<gates>
<gate name="G$1" symbol="CON2X3"/>
</gates>
<devices>
<device name=".1IN" package="AMP2X3-.1IN">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA" package="AMP2X3-.1IN-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AMP2X5" prefix="CON">
<gates>
<gate name="G$1" symbol="CON2X5"/>
</gates>
<devices>
<device name="" package="AMP2X5-.1IN">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA" package="AMP2X5-.1IN-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IDC-2X8" prefix="CON">
<gates>
<gate name="G$1" symbol="IDC2X8"/>
</gates>
<devices>
<device name="" package="IDC-NL-ASSMAN-NL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-PB" prefix="SW">
<gates>
<gate name="G$1" symbol="SWITCH-PB-TINY"/>
</gates>
<devices>
<device name="" package="PBSWITCH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TYCO" package="PB-TYCO">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AMP2X4">
<gates>
<gate name="G$1" symbol="CON2X4"/>
</gates>
<devices>
<device name="" package="AMP2X4-.1IN">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="6"/>
<connect gate="G$1" pin="5" pad="3"/>
<connect gate="G$1" pin="6" pad="7"/>
<connect gate="G$1" pin="7" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA" package="AMP2X4-.1IN-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="6"/>
<connect gate="G$1" pin="5" pad="3"/>
<connect gate="G$1" pin="6" pad="7"/>
<connect gate="G$1" pin="7" pad="4"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POT-VADJ">
<gates>
<gate name="G$1" symbol="POT-VADJ"/>
</gates>
<devices>
<device name="TH" package="POT-VADJ">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="18F4620QFN">
<gates>
<gate name="G$1" symbol="4620QFN"/>
</gates>
<devices>
<device name="" package="QFN44ML8X8-2">
<connects>
<connect gate="G$1" pin="MCLR" pad="18"/>
<connect gate="G$1" pin="NC" pad="13"/>
<connect gate="G$1" pin="RA0/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2" pad="21"/>
<connect gate="G$1" pin="RA3/AN3" pad="22"/>
<connect gate="G$1" pin="RA4" pad="23"/>
<connect gate="G$1" pin="RA5/AN4" pad="24"/>
<connect gate="G$1" pin="RA6/OX2" pad="33"/>
<connect gate="G$1" pin="RA7/OX1" pad="32"/>
<connect gate="G$1" pin="RB0" pad="9"/>
<connect gate="G$1" pin="RB1" pad="10"/>
<connect gate="G$1" pin="RB2" pad="11"/>
<connect gate="G$1" pin="RB3/PGM" pad="12"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RB6/PGC" pad="16"/>
<connect gate="G$1" pin="RB7/PGD" pad="17"/>
<connect gate="G$1" pin="RC0" pad="34"/>
<connect gate="G$1" pin="RC1" pad="35"/>
<connect gate="G$1" pin="RC2" pad="36"/>
<connect gate="G$1" pin="RC3/SCK" pad="37"/>
<connect gate="G$1" pin="RC4/MISO" pad="42"/>
<connect gate="G$1" pin="RC5/MOSI" pad="43"/>
<connect gate="G$1" pin="RC6/TX" pad="44"/>
<connect gate="G$1" pin="RC7/RX" pad="1"/>
<connect gate="G$1" pin="RD0" pad="38"/>
<connect gate="G$1" pin="RD1" pad="39"/>
<connect gate="G$1" pin="RD2" pad="40"/>
<connect gate="G$1" pin="RD3" pad="41"/>
<connect gate="G$1" pin="RD4" pad="2"/>
<connect gate="G$1" pin="RD5" pad="3"/>
<connect gate="G$1" pin="RD6" pad="4"/>
<connect gate="G$1" pin="RD7" pad="5"/>
<connect gate="G$1" pin="RE0/AN5" pad="25"/>
<connect gate="G$1" pin="RE1/AN6" pad="26"/>
<connect gate="G$1" pin="RE2/AN7" pad="27"/>
<connect gate="G$1" pin="VDD" pad="28"/>
<connect gate="G$1" pin="VDD@1" pad="7"/>
<connect gate="G$1" pin="VDD@2" pad="8"/>
<connect gate="G$1" pin="VDD@3" pad="29"/>
<connect gate="G$1" pin="VSS" pad="31"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
<connect gate="G$1" pin="VSS@2" pad="30"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD-16X1">
<gates>
<gate name="G$1" symbol="LCD-1X16"/>
</gates>
<devices>
<device name="" package="1X16">
<connects>
<connect gate="G$1" pin="+5V" pad="2"/>
<connect gate="G$1" pin="BL+" pad="15"/>
<connect gate="G$1" pin="BL-" pad="16"/>
<connect gate="G$1" pin="D0" pad="7"/>
<connect gate="G$1" pin="D1" pad="8"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="10"/>
<connect gate="G$1" pin="D4" pad="11"/>
<connect gate="G$1" pin="D5" pad="12"/>
<connect gate="G$1" pin="D6" pad="13"/>
<connect gate="G$1" pin="D7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="R/!W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE" prefix="D">
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="SOD323-W">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICSP-1X4" prefix="PROG">
<gates>
<gate name="G$1" symbol="ICSP"/>
</gates>
<devices>
<device name="" package="1X04L">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PGC" pad="3"/>
<connect gate="G$1" pin="PGD" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FFC-8" prefix="CON">
<gates>
<gate name="G$1" symbol="FFC-8"/>
</gates>
<devices>
<device name="1MM" package="FFC-8-1MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JOUSTICK-252">
<description>2 axis joystick</description>
<gates>
<gate name="G$1" symbol="JOYSTICK-2AX"/>
</gates>
<devices>
<device name="" package="JOY-252">
<connects>
<connect gate="G$1" pin="R1B" pad="R1B"/>
<connect gate="G$1" pin="R1C" pad="R1C"/>
<connect gate="G$1" pin="R1T" pad="R1T"/>
<connect gate="G$1" pin="R2C" pad="R2C"/>
<connect gate="G$1" pin="R2L" pad="R2L"/>
<connect gate="G$1" pin="R2R" pad="R2R"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="9VOLT_BATTERY">
<gates>
<gate name="G$1" symbol="9VOLTBAT"/>
</gates>
<devices>
<device name="" package="9VBATHOLDER">
<connects>
<connect gate="G$1" pin="MINUS" pad="-"/>
<connect gate="G$1" pin="PLUS" pad="+"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW-SLIDE-EG1918" prefix="SW">
<gates>
<gate name="G$1" symbol="SW-SPDT-D"/>
</gates>
<devices>
<device name="" package="SW-SPDT-2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A68-A31" prefix="S" uservalue="yes">
<description>&lt;b&gt;SLIDING SWITCH&lt;/b&gt;&lt;p&gt;
Siemens, distributor Buerklin, 11G766</description>
<gates>
<gate name="B" symbol="U2"/>
<gate name="A" symbol="SIS-"/>
</gates>
<devices>
<device name="" package="A68-A31">
<connects>
<connect gate="A" pin="O" pad="1"/>
<connect gate="A" pin="P" pad="2"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="B" pin="P" pad="5"/>
<connect gate="B" pin="S" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCREW-TERM-1X3" prefix="CON" uservalue="yes">
<gates>
<gate name="G$1" symbol="CONNECTOR-1X3"/>
</gates>
<devices>
<device name="SCREW3-.325" package="SCREW-TERM-3">
<connects>
<connect gate="G$1" pin="1" pad="P1"/>
<connect gate="G$1" pin="2" pad="P2"/>
<connect gate="G$1" pin="3" pad="P3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5.08MM" package="TYCO-5.08MM-3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM" package="TYCO-3.5MM-3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-3.81" package="TYCO-3.81MM-3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5.00MM" package="TYCO-5.00MM-3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MMA7455" prefix="IC">
<gates>
<gate name="G$1" symbol="MMA7455"/>
</gates>
<devices>
<device name="" package="LGA5X3">
<connects>
<connect gate="G$1" pin="!CS" pad="7"/>
<connect gate="G$1" pin="ADD" pad="4"/>
<connect gate="G$1" pin="AVDD" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="INT1" pad="8"/>
<connect gate="G$1" pin="INT2" pad="9"/>
<connect gate="G$1" pin="MISO" pad="12"/>
<connect gate="G$1" pin="MOSI" pad="13"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="NC@2" pad="10"/>
<connect gate="G$1" pin="NC@3" pad="11"/>
<connect gate="G$1" pin="SCLK" pad="14"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCREW-TERM-1X2" prefix="CON">
<gates>
<gate name="G$1" symbol="CONNECTOR-1X2"/>
</gates>
<devices>
<device name="5.08MM" package="TYCO-5.08MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-3.81" package="TYCO-3.81MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5.00MM" package="TYCO-5.00MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BARRIER-.325" package="SCREW-TERM-.325-2">
<connects>
<connect gate="G$1" pin="1" pad="P1"/>
<connect gate="G$1" pin="2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCREW-TERM-1X4" prefix="CON">
<gates>
<gate name="G$1" symbol="CONNECTOR-1X4"/>
</gates>
<devices>
<device name=".325IN" package="SCREW-TERM-1X4">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="P3" pad="P3"/>
<connect gate="G$1" pin="P4" pad="P4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="PHOE-5MM-4">
<connects>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P3" pad="3"/>
<connect gate="G$1" pin="P4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5.08MM" package="TYCO-5.08MM-4">
<connects>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P3" pad="3"/>
<connect gate="G$1" pin="P4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.81MM" package="TYCO-3.81MM-4">
<connects>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P3" pad="3"/>
<connect gate="G$1" pin="P4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T-5MM" package="TYCO-5.00MM-4">
<connects>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P3" pad="3"/>
<connect gate="G$1" pin="P4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM" package="TYCO-3.5MM-4">
<connects>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P3" pad="3"/>
<connect gate="G$1" pin="P4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCREW-TERM-1X5" prefix="CON" uservalue="yes">
<description>Buchanan screw terminal</description>
<gates>
<gate name="G$1" symbol="CONNECTOR-1X5-R"/>
</gates>
<devices>
<device name="5MM" package="PHOE-5MM-5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5.08MM" package="TYCO-5.08MM-5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T-5MM" package="TYCO-5.00MM-5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-3.5MM" package="TYCO-3.5MM-5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-3.81" package="TYCO-3.81MM-5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IDC-2X5" prefix="CON">
<description>10 (2x5) IDC</description>
<gates>
<gate name="G$1" symbol="IDC-2X5"/>
</gates>
<devices>
<device name="-RA" package="IDC-10-RA">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="10" pad="P$10"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="IDC-10">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="10" pad="P$10"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA-F" package="IDC-10-RA-F">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="10" pad="P$10"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA-M" package="IDC-10-RA-M">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="10" pad="P$10"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PROGRAMMER" prefix="PROG">
<gates>
<gate name="G$1" symbol="PROG"/>
</gates>
<devices>
<device name="" package="PROGRAMMER">
<connects>
<connect gate="G$1" pin="GND@1" pad="9"/>
<connect gate="G$1" pin="GND@2" pad="10"/>
<connect gate="G$1" pin="NC@1" pad="1"/>
<connect gate="G$1" pin="NC@2" pad="3"/>
<connect gate="G$1" pin="NC@3" pad="5"/>
<connect gate="G$1" pin="NC@4" pad="7"/>
<connect gate="G$1" pin="NC@5" pad="4"/>
<connect gate="G$1" pin="PGC" pad="8"/>
<connect gate="G$1" pin="PGD" pad="6"/>
<connect gate="G$1" pin="VPP" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="255SB" prefix="S" uservalue="yes">
<description>&lt;b&gt;SLIDING SWITCH&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="1" symbol="SIS"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SLIDE-SWITCH" prefix="SW">
<gates>
<gate name="G$1" symbol="SDPT-SLIDE"/>
</gates>
<devices>
<device name="-EG1218" package="EG1218">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ABM3B-XTAL">
<gates>
<gate name="G$1" symbol="ABM3B-XTAL"/>
</gates>
<devices>
<device name="" package="ABM3B-XTAL">
<connects>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BU-SMA-V" prefix="X" uservalue="yes">
<description>FEMALE &lt;b&gt;SMA CONNECTOR&lt;/b&gt;&lt;p&gt;
Radiall&lt;p&gt;
distributor RS 112-3794</description>
<gates>
<gate name="G$1" symbol="BNC-FGND"/>
<gate name="G2" symbol="GND"/>
<gate name="G1" symbol="GND"/>
<gate name="G3" symbol="GND"/>
</gates>
<devices>
<device name="" package="BU-SMA-V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G1" pin="GND" pad="3"/>
<connect gate="G2" pin="GND" pad="4"/>
<connect gate="G3" pin="GND" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SLIDE-DP3T" prefix="SW">
<gates>
<gate name="G$1" symbol="SW-DP3T"/>
</gates>
<devices>
<device name="-V" package="EG2301">
<connects>
<connect gate="G$1" pin="1A" pad="1"/>
<connect gate="G$1" pin="1B" pad="2"/>
<connect gate="G$1" pin="1C" pad="4"/>
<connect gate="G$1" pin="2A" pad="5"/>
<connect gate="G$1" pin="2B" pad="6"/>
<connect gate="G$1" pin="2C" pad="8"/>
<connect gate="G$1" pin="COM1" pad="3"/>
<connect gate="G$1" pin="COM2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-RA" package="EG2308">
<connects>
<connect gate="G$1" pin="1A" pad="1"/>
<connect gate="G$1" pin="1B" pad="2"/>
<connect gate="G$1" pin="1C" pad="4"/>
<connect gate="G$1" pin="2A" pad="5"/>
<connect gate="G$1" pin="2B" pad="6"/>
<connect gate="G$1" pin="2C" pad="8"/>
<connect gate="G$1" pin="COM1" pad="3"/>
<connect gate="G$1" pin="COM2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SLIDE-DPDT" prefix="SW">
<gates>
<gate name="G$1" symbol="SW-DPDT-SLIDE"/>
</gates>
<devices>
<device name="-V" package="EG2201">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="AC" pad="2"/>
<connect gate="G$1" pin="B1" pad="4"/>
<connect gate="G$1" pin="B2" pad="6"/>
<connect gate="G$1" pin="BC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-RA" package="EG2208">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="AC" pad="2"/>
<connect gate="G$1" pin="B1" pad="4"/>
<connect gate="G$1" pin="B2" pad="6"/>
<connect gate="G$1" pin="BC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-V2209" package="EG2209">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="AC" pad="2"/>
<connect gate="G$1" pin="B1" pad="4"/>
<connect gate="G$1" pin="B2" pad="6"/>
<connect gate="G$1" pin="BC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V2" package="EG2201-2">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="AC" pad="2"/>
<connect gate="G$1" pin="B1" pad="4"/>
<connect gate="G$1" pin="B2" pad="6"/>
<connect gate="G$1" pin="BC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IDC-2X12">
<gates>
<gate name="G$1" symbol="IDC-2X12"/>
</gates>
<devices>
<device name="" package="IDC-24">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="10" pad="P$10"/>
<connect gate="G$1" pin="11" pad="P$11"/>
<connect gate="G$1" pin="12" pad="P$12"/>
<connect gate="G$1" pin="13" pad="P$13"/>
<connect gate="G$1" pin="14" pad="P$14"/>
<connect gate="G$1" pin="15" pad="P$15"/>
<connect gate="G$1" pin="16" pad="P$16"/>
<connect gate="G$1" pin="17" pad="P$17"/>
<connect gate="G$1" pin="18" pad="P$18"/>
<connect gate="G$1" pin="19" pad="P$19"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="20" pad="P$20"/>
<connect gate="G$1" pin="21" pad="P$21"/>
<connect gate="G$1" pin="22" pad="P$22"/>
<connect gate="G$1" pin="23" pad="P$23"/>
<connect gate="G$1" pin="24" pad="P$24"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW-PB-SPST" prefix="SW">
<gates>
<gate name="G$1" symbol="SW-PB-SPST"/>
</gates>
<devices>
<device name="-RA" package="SPST-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="18F2420" prefix="IC">
<gates>
<gate name="G$1" symbol="18F2420"/>
</gates>
<devices>
<device name="-SOIC" package="SO28W">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="A3" pad="5"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="10"/>
<connect gate="G$1" pin="A7" pad="9"/>
<connect gate="G$1" pin="B0" pad="21"/>
<connect gate="G$1" pin="B1" pad="22"/>
<connect gate="G$1" pin="B2" pad="23"/>
<connect gate="G$1" pin="B3" pad="24"/>
<connect gate="G$1" pin="B4" pad="25"/>
<connect gate="G$1" pin="B5" pad="26"/>
<connect gate="G$1" pin="B6" pad="27"/>
<connect gate="G$1" pin="B7" pad="28"/>
<connect gate="G$1" pin="C0" pad="11"/>
<connect gate="G$1" pin="C1" pad="12"/>
<connect gate="G$1" pin="C2" pad="13"/>
<connect gate="G$1" pin="C3/SCLK" pad="14"/>
<connect gate="G$1" pin="C4/MISO" pad="15"/>
<connect gate="G$1" pin="C5/MOSI" pad="16"/>
<connect gate="G$1" pin="C6/MTX" pad="17"/>
<connect gate="G$1" pin="C7/MRX" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-QFN" package="QFN28-ML_6X6MM">
<connects>
<connect gate="G$1" pin="!MCLR" pad="26"/>
<connect gate="G$1" pin="A0" pad="27"/>
<connect gate="G$1" pin="A1" pad="28"/>
<connect gate="G$1" pin="A2" pad="1"/>
<connect gate="G$1" pin="A3" pad="2"/>
<connect gate="G$1" pin="A4" pad="3"/>
<connect gate="G$1" pin="A5" pad="4"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="6"/>
<connect gate="G$1" pin="B0" pad="18"/>
<connect gate="G$1" pin="B1" pad="19"/>
<connect gate="G$1" pin="B2" pad="20"/>
<connect gate="G$1" pin="B3" pad="21"/>
<connect gate="G$1" pin="B4" pad="22"/>
<connect gate="G$1" pin="B5" pad="23"/>
<connect gate="G$1" pin="B6" pad="24"/>
<connect gate="G$1" pin="B7" pad="25"/>
<connect gate="G$1" pin="C0" pad="8"/>
<connect gate="G$1" pin="C1" pad="9"/>
<connect gate="G$1" pin="C2" pad="10"/>
<connect gate="G$1" pin="C3/SCLK" pad="11"/>
<connect gate="G$1" pin="C4/MISO" pad="12"/>
<connect gate="G$1" pin="C5/MOSI" pad="13"/>
<connect gate="G$1" pin="C6/MTX" pad="14"/>
<connect gate="G$1" pin="C7/MRX" pad="15"/>
<connect gate="G$1" pin="VDD" pad="17"/>
<connect gate="G$1" pin="VSS@1" pad="5"/>
<connect gate="G$1" pin="VSS@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="18F2420-SQ" prefix="IC">
<gates>
<gate name="G$1" symbol="18F2420-SQ"/>
</gates>
<devices>
<device name="-QFN" package="QFN6X6-.55">
<connects>
<connect gate="G$1" pin="!MCLR" pad="26"/>
<connect gate="G$1" pin="A0" pad="27"/>
<connect gate="G$1" pin="A1" pad="28"/>
<connect gate="G$1" pin="A2" pad="1"/>
<connect gate="G$1" pin="A3" pad="2"/>
<connect gate="G$1" pin="A4" pad="3"/>
<connect gate="G$1" pin="A5/!SS" pad="4"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="6"/>
<connect gate="G$1" pin="B0" pad="18"/>
<connect gate="G$1" pin="B1" pad="19"/>
<connect gate="G$1" pin="B2" pad="20"/>
<connect gate="G$1" pin="B3" pad="21"/>
<connect gate="G$1" pin="B4" pad="22"/>
<connect gate="G$1" pin="B5" pad="23"/>
<connect gate="G$1" pin="B6" pad="24"/>
<connect gate="G$1" pin="B7" pad="25"/>
<connect gate="G$1" pin="C0" pad="8"/>
<connect gate="G$1" pin="C1" pad="9"/>
<connect gate="G$1" pin="C2" pad="10"/>
<connect gate="G$1" pin="C3/SCK" pad="11"/>
<connect gate="G$1" pin="C4/MISO" pad="12"/>
<connect gate="G$1" pin="C5/MOSI" pad="13"/>
<connect gate="G$1" pin="C6/MTH" pad="14"/>
<connect gate="G$1" pin="C7/MRX" pad="15"/>
<connect gate="G$1" pin="VDD" pad="17"/>
<connect gate="G$1" pin="VSS@1" pad="5"/>
<connect gate="G$1" pin="VSS@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TP" prefix="TP-">
<gates>
<gate name="G$1" symbol="TP"/>
</gates>
<devices>
<device name="" package="TP">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P-MOSFET-MED" prefix="Q">
<gates>
<gate name="G$1" symbol="P-MOS"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS1390">
<gates>
<gate name="G$1" symbol="DS1390"/>
</gates>
<devices>
<device name="" package="UMAX-10">
<connects>
<connect gate="G$1" pin="CS" pad="CS"/>
<connect gate="G$1" pin="DIN" pad="DIN"/>
<connect gate="G$1" pin="DOUT" pad="DOUT"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SCLK" pad="SCLK"/>
<connect gate="G$1" pin="SQW/INT" pad="SQW/INT"/>
<connect gate="G$1" pin="VBACKUP" pad="VBACKUP"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="X1" pad="X1"/>
<connect gate="G$1" pin="X2" pad="X2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RECTIFIER" prefix="B" uservalue="yes">
<description>&lt;b&gt;GENERAL INSTRUMENT RECTIFIER&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GB"/>
</gates>
<devices>
<device name="" package="GBU4S">
<connects>
<connect gate="1" pin="+" pad="+"/>
<connect gate="1" pin="-" pad="-"/>
<connect gate="1" pin="AC1" pad="AC2"/>
<connect gate="1" pin="AC2" pad="AC1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GBJ" package="GBJ">
<connects>
<connect gate="1" pin="+" pad="+"/>
<connect gate="1" pin="-" pad="-"/>
<connect gate="1" pin="AC1" pad="AC2"/>
<connect gate="1" pin="AC2" pad="AC1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OMROMSPDT" prefix="R">
<description>OMRON SPST</description>
<gates>
<gate name="G$1" symbol="K"/>
<gate name="G$2" symbol="U"/>
</gates>
<devices>
<device name="OMRON" package="OMRONSPDT">
<connects>
<connect gate="G$1" pin="1" pad="A1"/>
<connect gate="G$1" pin="2" pad="A2"/>
<connect gate="G$2" pin="NC" pad="NC"/>
<connect gate="G$2" pin="NO" pad="NO"/>
<connect gate="G$2" pin="P" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RT42?*" prefix="K">
<description>&lt;b&gt;Power PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
2 pole 8 A, DC and AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5842.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="4" package="RT2C/O">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="NC" pad="NC2"/>
<connect gate="2" pin="NO" pad="NO2"/>
<connect gate="2" pin="P" pad="P2"/>
<connect gate="3" pin="NC" pad="NC1"/>
<connect gate="3" pin="NO" pad="NO1"/>
<connect gate="3" pin="P" pad="P1"/>
</connects>
<technologies>
<technology name="005"/>
<technology name="006"/>
<technology name="012"/>
<technology name="024"/>
<technology name="048"/>
<technology name="060"/>
<technology name="110"/>
<technology name="524"/>
<technology name="615"/>
<technology name="730"/>
</technologies>
</device>
<device name="5" package="RT2C/O">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="NC" pad="NC1"/>
<connect gate="2" pin="NO" pad="NO1"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="3" pin="NC" pad="NC2"/>
<connect gate="3" pin="NO" pad="NO2"/>
<connect gate="3" pin="P" pad="P2"/>
</connects>
<technologies>
<technology name="005"/>
<technology name="006"/>
<technology name="012"/>
<technology name="024"/>
<technology name="048"/>
<technology name="060"/>
<technology name="110"/>
<technology name="524"/>
<technology name="615"/>
<technology name="730"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RT174*" prefix="K">
<description>&lt;b&gt;Power PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
sensitive 1 pole 10 A, highly sensitive version&lt;br&gt;
Source: http://www.schrack.com/.. 5822.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="RT-C/O12A3.5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="NC" pad="POL"/>
<connect gate="2" pin="NO" pad="NO"/>
<connect gate="2" pin="P" pad="NC"/>
</connects>
<technologies>
<technology name="005"/>
<technology name="006"/>
<technology name="012"/>
<technology name="024"/>
<technology name="048"/>
<technology name="060"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TYCODPDT" prefix="R">
<description>TYCO DPDT</description>
<gates>
<gate name="G$1" symbol="K"/>
<gate name="G$2" symbol="U"/>
<gate name="G$3" symbol="U"/>
</gates>
<devices>
<device name="" package="RT2C/O">
<connects>
<connect gate="G$1" pin="1" pad="A1"/>
<connect gate="G$1" pin="2" pad="A2"/>
<connect gate="G$2" pin="NC" pad="NC1"/>
<connect gate="G$2" pin="NO" pad="NO1"/>
<connect gate="G$2" pin="P" pad="P1"/>
<connect gate="G$3" pin="NC" pad="NC2"/>
<connect gate="G$3" pin="NO" pad="NO2"/>
<connect gate="G$3" pin="P" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" prefix="LED" uservalue="yes">
<description>&lt;b&gt;LED&lt;/b&gt;&lt;p&gt;
&lt;u&gt;OSRAM&lt;/u&gt;:&lt;br&gt;

- &lt;u&gt;CHIPLED&lt;/u&gt;&lt;br&gt;
LG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971
LH N974, LH R974&lt;br&gt;
LS Q976, LO Q976, LY Q976&lt;br&gt;
LO Q996&lt;br&gt;

- &lt;u&gt;Hyper CHIPLED&lt;/u&gt;&lt;br&gt;
LW Q18S&lt;br&gt;
LB Q993, LB Q99A, LB R99A&lt;br&gt;

- &lt;u&gt;SideLED&lt;/u&gt;&lt;br&gt;
LS A670, LO A670, LY A670, LG A670, LP A670&lt;br&gt;
LB A673, LV A673, LT A673, LW A673&lt;br&gt;
LH A674&lt;br&gt;
LY A675&lt;br&gt;
LS A676, LA A676, LO A676, LY A676, LW A676&lt;br&gt;
LS A679, LY A679, LG A679&lt;br&gt;

-  &lt;u&gt;Hyper Micro SIDELED®&lt;/u&gt;&lt;br&gt;
LS Y876, LA Y876, LO Y876, LY Y876&lt;br&gt;
LT Y87S&lt;br&gt;

- &lt;u&gt;SmartLED&lt;/u&gt;&lt;br&gt;
LW L88C, LW L88S&lt;br&gt;
LB L89C, LB L89S, LG L890&lt;br&gt;
LS L89K, LO L89K, LY L89K&lt;br&gt;
LS L896, LA L896, LO L896, LY L896&lt;br&gt;

- &lt;u&gt;TOPLED&lt;/u&gt;&lt;br&gt;
LS T670, LO T670, LY T670, LG T670, LP T670&lt;br&gt;
LSG T670, LSP T670, LSY T670, LOP T670, LYG T670&lt;br&gt;
LG T671, LOG T671, LSG T671&lt;br&gt;
LB T673, LV T673, LT T673, LW T673&lt;br&gt;
LH T674&lt;br&gt;
LS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676&lt;br&gt;
LB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C&lt;br&gt;
LS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C&lt;br&gt;
LW T67C&lt;br&gt;
LS T679, LY T679, LG T679&lt;br&gt;
LS T770, LO T770, LY T770, LG T770, LP T770&lt;br&gt;
LB T773, LV T773, LT T773, LW T773&lt;br&gt;
LH T774&lt;br&gt;
LS E675, LA E675, LY E675, LS T675&lt;br&gt;
LS T776, LA T776, LO T776, LY T776, LB T776&lt;br&gt;
LHGB T686&lt;br&gt;
LT T68C, LB T68C&lt;br&gt;

- &lt;u&gt;Hyper Mini TOPLED®&lt;/u&gt;&lt;br&gt;
LB M676&lt;br&gt;

- &lt;u&gt;Mini TOPLED Santana®&lt;/u&gt;&lt;br&gt;
LG M470&lt;br&gt;
LS M47K, LO M47K, LY M47K&lt;br&gt;
&lt;p&gt;
Source: http://www.osram.convergy.de&lt;p&gt;

- &lt;u&gt;LUMILED®&lt;/u&gt;&lt;br&gt;
LXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00&lt;br&gt;
LXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00&lt;br&gt;
LXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00&lt;br&gt;
LXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00&lt;br&gt;
LXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00&lt;br&gt;
LXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00&lt;br&gt;
LXK2-PH12-R00, LXK2-PH12-S00&lt;br&gt;
LXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00&lt;br&gt;
&lt;p&gt;
Source: www.luxeon.com&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="SMT1206" package="1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LD260" package="LD260">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SQR2X5" package="LED2X5">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3MM" package="LED3MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="LED5MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LSU260" package="LSU260">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LZR181" package="LZR181">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B152" package="Q62902-B152">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B153" package="Q62902-B153">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B155" package="Q62902-B155">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B156" package="Q62902-B156">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SFH480" package="SFH480">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SFH482" package="SFH482">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SQR5.7X3.2" package="U57X32">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IRL80A" package="IRL80A">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-2" package="P-LCC-2">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MINI-TOP" package="OSRAM-MINI-TOP-LED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SIDELED" package="OSRAM-SIDELED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-2-BACK" package="P-LCC-2-TOPLED-RG">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MICRO-SIDELED" package="MICRO-SIDELED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-4" package="P-LCC-4">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C@4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIP-LED0603" package="CHIP-LED0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIP-LED0805" package="CHIP-LED0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TOPLED-SANTANA" package="MINI-TOPLED-SANTANA">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_0805" package="CHIPLED_0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_1206" package="CHIPLED_1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_0603" package="CHIPLED_0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED-0603-TTW" package="CHIPLED-0603-TTW">
<connects>
<connect gate="G$1" pin="A" pad="A@1"/>
<connect gate="G$1" pin="C" pad="C@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LUMILED+" package="LUMILED+">
<connects>
<connect gate="G$1" pin="A" pad="2+"/>
<connect gate="G$1" pin="C" pad="4-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LUMILED" package="LUMILED">
<connects>
<connect gate="G$1" pin="A" pad="2+"/>
<connect gate="G$1" pin="C" pad="4-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="18F4620QFN-G">
<gates>
<gate name="G$1" symbol="4620QFN-G"/>
</gates>
<devices>
<device name="" package="QFN44ML8X8-2G">
<connects>
<connect gate="G$1" pin="MCLR" pad="18"/>
<connect gate="G$1" pin="NC" pad="13"/>
<connect gate="G$1" pin="RA0/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2" pad="21"/>
<connect gate="G$1" pin="RA3/AN3" pad="22"/>
<connect gate="G$1" pin="RA4" pad="23"/>
<connect gate="G$1" pin="RA5/AN4" pad="24"/>
<connect gate="G$1" pin="RA6/OX2" pad="33"/>
<connect gate="G$1" pin="RA7/OX1" pad="32"/>
<connect gate="G$1" pin="RB0" pad="9"/>
<connect gate="G$1" pin="RB1" pad="10"/>
<connect gate="G$1" pin="RB2" pad="11"/>
<connect gate="G$1" pin="RB3/PGM" pad="12"/>
<connect gate="G$1" pin="RB4" pad="14"/>
<connect gate="G$1" pin="RB5" pad="15"/>
<connect gate="G$1" pin="RB6/PGC" pad="16"/>
<connect gate="G$1" pin="RB7/PGD" pad="17"/>
<connect gate="G$1" pin="RC0" pad="34"/>
<connect gate="G$1" pin="RC1" pad="35"/>
<connect gate="G$1" pin="RC2" pad="36"/>
<connect gate="G$1" pin="RC3/SCK" pad="37"/>
<connect gate="G$1" pin="RC4/MISO" pad="42"/>
<connect gate="G$1" pin="RC5/MOSI" pad="43"/>
<connect gate="G$1" pin="RC6/TX" pad="44"/>
<connect gate="G$1" pin="RC7/RX" pad="1"/>
<connect gate="G$1" pin="RD0" pad="38"/>
<connect gate="G$1" pin="RD1" pad="39"/>
<connect gate="G$1" pin="RD2" pad="40"/>
<connect gate="G$1" pin="RD3" pad="41"/>
<connect gate="G$1" pin="RD4" pad="2"/>
<connect gate="G$1" pin="RD5" pad="3"/>
<connect gate="G$1" pin="RD6" pad="4"/>
<connect gate="G$1" pin="RD7" pad="5"/>
<connect gate="G$1" pin="RE0/AN5" pad="25"/>
<connect gate="G$1" pin="RE1/AN6" pad="26"/>
<connect gate="G$1" pin="RE2/AN7" pad="27"/>
<connect gate="G$1" pin="VDD" pad="28"/>
<connect gate="G$1" pin="VDD@1" pad="7"/>
<connect gate="G$1" pin="VDD@2" pad="8"/>
<connect gate="G$1" pin="VDD@3" pad="29"/>
<connect gate="G$1" pin="VSS" pad="31"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
<connect gate="G$1" pin="VSS@2" pad="30"/>
<connect gate="G$1" pin="VSS@3" pad="PAD"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AC-IN">
<gates>
<gate name="G$1" symbol="AC-IN"/>
</gates>
<devices>
<device name="" package="ACPOWER">
<connects>
<connect gate="G$1" pin="COM" pad="P$2"/>
<connect gate="G$1" pin="HOT" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIN-6">
<gates>
<gate name="G$1" symbol="DIN-6"/>
</gates>
<devices>
<device name="" package="DIN-6">
<connects>
<connect gate="G$1" pin="1" pad="P1"/>
<connect gate="G$1" pin="2" pad="P2"/>
<connect gate="G$1" pin="3" pad="P3"/>
<connect gate="G$1" pin="4" pad="P4"/>
<connect gate="G$1" pin="5" pad="P5"/>
<connect gate="G$1" pin="6" pad="P6"/>
<connect gate="G$1" pin="GND@1" pad="P$1"/>
<connect gate="G$1" pin="GND@2" pad="P$2"/>
<connect gate="G$1" pin="GND@3" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POWER-16GUAGE">
<gates>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POWER-16GAUGE">
<gates>
<gate name="G$1" symbol="POWER-16GAUGE"/>
</gates>
<devices>
<device name="" package="POWER-16GAUGE">
<connects>
<connect gate="G$1" pin="+" pad="P$1"/>
<connect gate="G$1" pin="-" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PHONO-JACK">
<gates>
<gate name="G$1" symbol="PHONO-JACK"/>
</gates>
<devices>
<device name="RA" package="PHONO-JACK-RA">
<connects>
<connect gate="G$1" pin="GND@1" pad="G$1"/>
<connect gate="G$1" pin="GND@2" pad="G$2"/>
<connect gate="G$1" pin="GND@3" pad="G$3"/>
<connect gate="G$1" pin="SIG" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-RGB" prefix="LED" uservalue="yes">
<gates>
<gate name="G$1" symbol="LED-RGB"/>
</gates>
<devices>
<device name="" package="LED-RGB">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
<connect gate="G$1" pin="C3" pad="C3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOPOUR" package="LED-RGB2">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
<connect gate="G$1" pin="C3" pad="C3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LEDDRV-9635">
<gates>
<gate name="G$1" symbol="LEDDRV-PCA9635"/>
</gates>
<devices>
<device name="" package="TSSOP28">
<connects>
<connect gate="G$1" pin="!OE" pad="23"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="24"/>
<connect gate="G$1" pin="A6" pad="25"/>
<connect gate="G$1" pin="LED0" pad="6"/>
<connect gate="G$1" pin="LED1" pad="7"/>
<connect gate="G$1" pin="LED10" pad="17"/>
<connect gate="G$1" pin="LED11" pad="18"/>
<connect gate="G$1" pin="LED12" pad="19"/>
<connect gate="G$1" pin="LED13" pad="20"/>
<connect gate="G$1" pin="LED14" pad="21"/>
<connect gate="G$1" pin="LED15" pad="22"/>
<connect gate="G$1" pin="LED2" pad="8"/>
<connect gate="G$1" pin="LED3" pad="9"/>
<connect gate="G$1" pin="LED4" pad="10"/>
<connect gate="G$1" pin="LED5" pad="11"/>
<connect gate="G$1" pin="LED6" pad="12"/>
<connect gate="G$1" pin="LED7" pad="13"/>
<connect gate="G$1" pin="LED8" pad="15"/>
<connect gate="G$1" pin="LED9" pad="16"/>
<connect gate="G$1" pin="SCL" pad="26"/>
<connect gate="G$1" pin="SDA" pad="27"/>
<connect gate="G$1" pin="VDD" pad="28"/>
<connect gate="G$1" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SD-5638">
<gates>
<gate name="G$1" symbol="SD-5638"/>
</gates>
<devices>
<device name="" package="SD-5638">
<connects>
<connect gate="G$1" pin="GND" pad="P3"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="GND@3" pad="P6"/>
<connect gate="G$1" pin="P1/CS" pad="P1"/>
<connect gate="G$1" pin="P2/DI" pad="P2"/>
<connect gate="G$1" pin="P5/CLK" pad="P5"/>
<connect gate="G$1" pin="P7/DO" pad="P7"/>
<connect gate="G$1" pin="P8/IRQ" pad="P8"/>
<connect gate="G$1" pin="P9/DAT2" pad="P9"/>
<connect gate="G$1" pin="PCD" pad="PCD"/>
<connect gate="G$1" pin="PWP" pad="PWP"/>
<connect gate="G$1" pin="VDD" pad="P4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA*-SOT23" prefix="IC">
<description>&lt;b&gt;Single Operational Amplifier&lt;/b&gt;&lt;p&gt;
Low Power, Single-Supply, Rail-To-Rail Operational Amplifier&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/opa2345.pdf</description>
<gates>
<gate name="P" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="P" pin="+IN" pad="3"/>
<connect gate="P" pin="-IN" pad="4"/>
<connect gate="P" pin="OUT" pad="1"/>
<connect gate="P" pin="V+" pad="5"/>
<connect gate="P" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="344N"/>
<technology name="345N"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CUR_SEN_TAMURA">
<gates>
<gate name="G$1" symbol="CUR_SENSE_TAMURA"/>
</gates>
<devices>
<device name="" package="CUR_SENS_TAMURA">
<connects>
<connect gate="G$1" pin="GND" pad="P2"/>
<connect gate="G$1" pin="VCC" pad="P3"/>
<connect gate="G$1" pin="VOUT" pad="P1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LICAL-DECODER">
<gates>
<gate name="G$1" symbol="LICAL-DECODER"/>
</gates>
<devices>
<device name="" package="SSOP20">
<connects>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="17"/>
<connect gate="G$1" pin="D3" pad="18"/>
<connect gate="G$1" pin="D4" pad="19"/>
<connect gate="G$1" pin="D5" pad="20"/>
<connect gate="G$1" pin="D6" pad="1"/>
<connect gate="G$1" pin="D7" pad="2"/>
<connect gate="G$1" pin="DIN" pad="12"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="LATCH" pad="7"/>
<connect gate="G$1" pin="LRN" pad="11"/>
<connect gate="G$1" pin="MODE_IN" pad="10"/>
<connect gate="G$1" pin="RX_CTL" pad="8"/>
<connect gate="G$1" pin="SBD0" pad="3"/>
<connect gate="G$1" pin="SBD1" pad="4"/>
<connect gate="G$1" pin="TX_ID" pad="9"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VDD@1" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ANT-315">
<gates>
<gate name="G$1" symbol="ANT-315"/>
</gates>
<devices>
<device name="" package="ANT-315-SCREW">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VR-TC1185">
<gates>
<gate name="G$1" symbol="VR-TC1185"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="!SHDN" pad="3"/>
<connect gate="G$1" pin="BYP" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCREW-TERM-1X6">
<gates>
<gate name="G$1" symbol="CONNECTOR-1X6-R"/>
</gates>
<devices>
<device name="" package="TYCO-5.00MM-6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-RG" prefix="LED">
<gates>
<gate name="G$1" symbol="LED-RG"/>
</gates>
<devices>
<device name="" package="LED2-0606">
<connects>
<connect gate="G$1" pin="AG" pad="1"/>
<connect gate="G$1" pin="AR" pad="2"/>
<connect gate="G$1" pin="CG" pad="3"/>
<connect gate="G$1" pin="CR" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INV300X" prefix="IC">
<gates>
<gate name="G$1" symbol="INV300X"/>
</gates>
<devices>
<device name="" package="INV300X">
<connects>
<connect gate="G$1" pin="ANT" pad="1"/>
<connect gate="G$1" pin="BAT" pad="2"/>
<connect gate="G$1" pin="BOOT" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="9"/>
<connect gate="G$1" pin="GND@2" pad="10"/>
<connect gate="G$1" pin="GP1" pad="3"/>
<connect gate="G$1" pin="GP3" pad="13"/>
<connect gate="G$1" pin="GP4" pad="6"/>
<connect gate="G$1" pin="GP5" pad="11"/>
<connect gate="G$1" pin="ON" pad="4"/>
<connect gate="G$1" pin="PCHK" pad="15"/>
<connect gate="G$1" pin="RESET" pad="16"/>
<connect gate="G$1" pin="RXA" pad="14"/>
<connect gate="G$1" pin="RXB" pad="12"/>
<connect gate="G$1" pin="TIME" pad="17"/>
<connect gate="G$1" pin="TXA" pad="5"/>
<connect gate="G$1" pin="TXB" pad="7"/>
<connect gate="G$1" pin="VCC" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74LVG107" prefix="IC">
<gates>
<gate name="G$1" symbol="74LV1G07"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="I1" pad="2"/>
<connect gate="G$1" pin="O1" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L-US" prefix="L">
<gates>
<gate name="G$1" symbol="L-US"/>
</gates>
<devices>
<device name="" package="LUS-0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TXB0108" prefix="IC">
<gates>
<gate name="G$1" symbol="TXB0108"/>
</gates>
<devices>
<device name="" package="TSSOP20">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="8"/>
<connect gate="G$1" pin="A8" pad="9"/>
<connect gate="G$1" pin="B1" pad="20"/>
<connect gate="G$1" pin="B2" pad="18"/>
<connect gate="G$1" pin="B3" pad="17"/>
<connect gate="G$1" pin="B4" pad="16"/>
<connect gate="G$1" pin="B5" pad="15"/>
<connect gate="G$1" pin="B6" pad="14"/>
<connect gate="G$1" pin="B7" pad="13"/>
<connect gate="G$1" pin="B8" pad="12"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="OE" pad="10"/>
<connect gate="G$1" pin="VA" pad="2"/>
<connect gate="G$1" pin="VB" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE-ZENER" prefix="D">
<gates>
<gate name="G$1" symbol="DIODE-ZENER"/>
</gates>
<devices>
<device name="SMA" package="DIODE-SMA">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-MOLEX-43XX-3" prefix="CON">
<description>Molex 4300 series - 3 pin</description>
<gates>
<gate name="G$1" symbol="CONNECTOR-1X3"/>
</gates>
<devices>
<device name="RA" package="MOLEX-4301">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="MOLEX-4201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-MOLEX-43XX-4" prefix="CON">
<description>Molex 4300 series 4 pin</description>
<gates>
<gate name="G$1" symbol="CONNECTOR-1X4"/>
</gates>
<devices>
<device name="M43XX-RA" package="MOLEX-4302">
<connects>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P3" pad="3"/>
<connect gate="G$1" pin="P4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M42XX-V" package="MOLEX-4202">
<connects>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P3" pad="3"/>
<connect gate="G$1" pin="P4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-MOLEX-43XX-6" prefix="CON">
<description>molex 43xx 6-pin</description>
<gates>
<gate name="G$1" symbol="CONNECTOR-1X6-R"/>
</gates>
<devices>
<device name="RA" package="MOLEX-4304">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4204-V" package="WM-4204">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LEM-HAAS">
<gates>
<gate name="G$1" symbol="LEM-HAAS"/>
</gates>
<devices>
<device name="" package="CUR-SEN-LEM">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPTO-AC-DUAL" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="AC-OPTO-DUAL"/>
</gates>
<devices>
<device name="" package="DIL8">
<connects>
<connect gate="G$1" pin="AC1A" pad="1"/>
<connect gate="G$1" pin="AC1B" pad="2"/>
<connect gate="G$1" pin="AC2A" pad="3"/>
<connect gate="G$1" pin="AC2B" pad="4"/>
<connect gate="G$1" pin="C1" pad="8"/>
<connect gate="G$1" pin="C2" pad="6"/>
<connect gate="G$1" pin="E1" pad="7"/>
<connect gate="G$1" pin="E2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="8-SMD" package="8-SMD">
<connects>
<connect gate="G$1" pin="AC1A" pad="1"/>
<connect gate="G$1" pin="AC1B" pad="2"/>
<connect gate="G$1" pin="AC2A" pad="3"/>
<connect gate="G$1" pin="AC2B" pad="4"/>
<connect gate="G$1" pin="C1" pad="8"/>
<connect gate="G$1" pin="C2" pad="6"/>
<connect gate="G$1" pin="E1" pad="7"/>
<connect gate="G$1" pin="E2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM317">
<gates>
<gate name="G$1" symbol="LM317"/>
</gates>
<devices>
<device name="DPAK" package="DPAK">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCREW-TERM-1X12R" prefix="CON" uservalue="yes">
<gates>
<gate name="G$1" symbol="CONNECTOR-1X12-R"/>
</gates>
<devices>
<device name="L" package="TYCO-5.00MM-12L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R" package="TYCO-5.00MM-12R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCREW-TERM-1X12-L" prefix="CON" uservalue="yes">
<gates>
<gate name="G$1" symbol="CONNECTOR-1X12-L"/>
</gates>
<devices>
<device name="L" package="TYCO-5.00MM-12L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R" package="TYCO-5.00MM-12R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-MOLEX-42XX-2" prefix="CON">
<gates>
<gate name="G$1" symbol="CONNECTOR-1X2"/>
</gates>
<devices>
<device name="WM-4200-V" package="MOLEX-4200">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA" package="MOLEX-4300">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-MOLEX-43XX-8" prefix="CON" uservalue="yes">
<gates>
<gate name="G$1" symbol="CONNECTOR-1X8-R"/>
</gates>
<devices>
<device name="4306-RA" package="MOLEX-4306">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="MOLEX-4206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPU-6000" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="MPU-6000"/>
</gates>
<devices>
<device name="" package="MPU-60X0">
<connects>
<connect gate="G$1" pin="!CS" pad="8"/>
<connect gate="G$1" pin="AD0/SDO" pad="9"/>
<connect gate="G$1" pin="AUX_CL" pad="7"/>
<connect gate="G$1" pin="AUX_DA" pad="6"/>
<connect gate="G$1" pin="CLKIN" pad="1"/>
<connect gate="G$1" pin="CLKOUT" pad="22"/>
<connect gate="G$1" pin="CPOUT" pad="20"/>
<connect gate="G$1" pin="FSYNC" pad="11"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="INT" pad="12"/>
<connect gate="G$1" pin="NC$1" pad="2"/>
<connect gate="G$1" pin="NC$2" pad="3"/>
<connect gate="G$1" pin="NC$3" pad="4"/>
<connect gate="G$1" pin="NC$4" pad="5"/>
<connect gate="G$1" pin="NC$5" pad="14"/>
<connect gate="G$1" pin="NC$6" pad="15"/>
<connect gate="G$1" pin="NC$7" pad="16"/>
<connect gate="G$1" pin="NC$8" pad="17"/>
<connect gate="G$1" pin="REGOUT" pad="10"/>
<connect gate="G$1" pin="RESV$1" pad="19"/>
<connect gate="G$1" pin="RESV$2" pad="21"/>
<connect gate="G$1" pin="SCL/SCLK" pad="23"/>
<connect gate="G$1" pin="SDA/SDI" pad="24"/>
<connect gate="G$1" pin="VDD" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPU-6050" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="MPU-6050"/>
</gates>
<devices>
<device name="" package="MPU-60X0">
<connects>
<connect gate="G$1" pin="AD0" pad="9"/>
<connect gate="G$1" pin="AUX_CL" pad="7"/>
<connect gate="G$1" pin="AUX_DA" pad="6"/>
<connect gate="G$1" pin="CLKIN" pad="1"/>
<connect gate="G$1" pin="CLKOUT" pad="22"/>
<connect gate="G$1" pin="CPOUT" pad="20"/>
<connect gate="G$1" pin="FSYNC" pad="11"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="INT" pad="12"/>
<connect gate="G$1" pin="NC$1" pad="2"/>
<connect gate="G$1" pin="NC$2" pad="3"/>
<connect gate="G$1" pin="NC$3" pad="4"/>
<connect gate="G$1" pin="NC$4" pad="5"/>
<connect gate="G$1" pin="NC$5" pad="14"/>
<connect gate="G$1" pin="NC$6" pad="15"/>
<connect gate="G$1" pin="NC$7" pad="16"/>
<connect gate="G$1" pin="NC$8" pad="17"/>
<connect gate="G$1" pin="REGOUT" pad="10"/>
<connect gate="G$1" pin="RESV$1" pad="19"/>
<connect gate="G$1" pin="RESV$2" pad="21"/>
<connect gate="G$1" pin="SCL" pad="23"/>
<connect gate="G$1" pin="SDA" pad="24"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VLOGIC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BMP085" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="BMP085"/>
</gates>
<devices>
<device name="" package="LCC8">
<connects>
<connect gate="G$1" pin="EOC" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="7"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VDDA" pad="3"/>
<connect gate="G$1" pin="XCLR" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADXL345" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="ADXL345"/>
</gates>
<devices>
<device name="" package="LGA14">
<connects>
<connect gate="G$1" pin="!CS" pad="7"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="4"/>
<connect gate="G$1" pin="GND@3" pad="5"/>
<connect gate="G$1" pin="INT1" pad="8"/>
<connect gate="G$1" pin="INT2" pad="9"/>
<connect gate="G$1" pin="NC" pad="10"/>
<connect gate="G$1" pin="RESV@1" pad="3"/>
<connect gate="G$1" pin="RESV@2" pad="11"/>
<connect gate="G$1" pin="SCL" pad="14"/>
<connect gate="G$1" pin="SDA/SDI" pad="13"/>
<connect gate="G$1" pin="SDO/ALT" pad="12"/>
<connect gate="G$1" pin="VDDIO" pad="1"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADMP405" prefix="MIC">
<gates>
<gate name="G$1" symbol="ADMP405"/>
</gates>
<devices>
<device name="" package="ADMP405">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEDIATEK3329" prefix="IC">
<gates>
<gate name="G$1" symbol="MEDIATEK3329"/>
</gates>
<devices>
<device name="" package="MEDIATEK3329">
<connects>
<connect gate="G$1" pin="3DFIX" pad="5"/>
<connect gate="G$1" pin="DMINUS" pad="7"/>
<connect gate="G$1" pin="DPLUS" pad="6"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="8"/>
<connect gate="G$1" pin="NC@1" pad="11"/>
<connect gate="G$1" pin="NC@2" pad="12"/>
<connect gate="G$1" pin="RX" pad="10"/>
<connect gate="G$1" pin="TX" pad="9"/>
<connect gate="G$1" pin="VBACK" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-MOLEX-CGRIDIII-5X2" prefix="CON" uservalue="yes">
<gates>
<gate name="G$1" symbol="CON2X5"/>
</gates>
<devices>
<device name="V" package="CON-CGRIDIII-5X2-V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA" package="CON-CGRIDIII-5X2-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-MOLEX-CGRIDIII-4X2" prefix="CON">
<gates>
<gate name="G$1" symbol="CON2X4"/>
</gates>
<devices>
<device name="V" package="CON-CGRIDIII-4X2-V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA" package="CON-CGRIDIII-4X2-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FJ256GB210" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="PIC24FJ256GB210"/>
</gates>
<devices>
<device name="TQFP" package="TQFP64-10X10RMS">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="DHM/RP11/INT0/CN49/RD0" pad="46"/>
<connect gate="G$1" pin="ENVREG" pad="57"/>
<connect gate="G$1" pin="PMA8/SCL2/CN18/U2TX/RF5" pad="32"/>
<connect gate="G$1" pin="PMA9/SDA2/CN17/U2RX/RF4" pad="31"/>
<connect gate="G$1" pin="PMD0/RE0" pad="60"/>
<connect gate="G$1" pin="PMD1/RE1" pad="61"/>
<connect gate="G$1" pin="PMD2/RE2" pad="62"/>
<connect gate="G$1" pin="PMD3/RE3" pad="63"/>
<connect gate="G$1" pin="PMD4/RE4" pad="64"/>
<connect gate="G$1" pin="PMD5/RE5" pad="1"/>
<connect gate="G$1" pin="RB0/RP0/AN0/CN2/VR+/PGD1/PMA6" pad="16"/>
<connect gate="G$1" pin="RB1/RP1/AN1/CN3/VR-/PGC1/EMUC1" pad="15"/>
<connect gate="G$1" pin="RB10/AN10/TMS/CVREF/PMA13" pad="23"/>
<connect gate="G$1" pin="RB11/AN11/TDO/PMA12" pad="24"/>
<connect gate="G$1" pin="RB12/AN12/TCK/PMA11" pad="27"/>
<connect gate="G$1" pin="RB13/AN13/TDI/PMA10" pad="28"/>
<connect gate="G$1" pin="RB14/AN14/U2RTS/BCLK2/PMA1" pad="29"/>
<connect gate="G$1" pin="RB15/AN15/CN12/OCFB/PMA0" pad="30"/>
<connect gate="G$1" pin="RB2/RP13/AN2/CN4/SS1/C2IN-" pad="14"/>
<connect gate="G$1" pin="RB3/AN3/CN5/C2IN+" pad="13"/>
<connect gate="G$1" pin="RB6/AN6/OCFA/EMUC2/PGC2" pad="17"/>
<connect gate="G$1" pin="RB7/AN7/EMUD2/PGD2" pad="18"/>
<connect gate="G$1" pin="RB8/AN8/U2CTS/C1OUT" pad="21"/>
<connect gate="G$1" pin="RB9/AN9/C2OUT/PMA7" pad="22"/>
<connect gate="G$1" pin="RC12/CLKI/OSC1" pad="39"/>
<connect gate="G$1" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="G$1" pin="RD1/OC2/RP24" pad="49"/>
<connect gate="G$1" pin="RD10/SCL1/IC3/INT3/PMCS2" pad="44"/>
<connect gate="G$1" pin="RD11/IC4/INT4/PMCS1" pad="45"/>
<connect gate="G$1" pin="RD2/OC3/RP23" pad="50"/>
<connect gate="G$1" pin="RD3/OC4/PMBE/RP22" pad="51"/>
<connect gate="G$1" pin="RD4/OC5/IC5/CN13/PMWR/RP25" pad="52"/>
<connect gate="G$1" pin="RD5/CN14/PMRD/RP20" pad="53"/>
<connect gate="G$1" pin="RD6/CN15" pad="54"/>
<connect gate="G$1" pin="RD7/CN16" pad="55"/>
<connect gate="G$1" pin="RD8/IC1/INT1/RTCC" pad="42"/>
<connect gate="G$1" pin="RD9/SDA1/IC2/INT2/U1CTS" pad="43"/>
<connect gate="G$1" pin="RF0" pad="58"/>
<connect gate="G$1" pin="RF1" pad="59"/>
<connect gate="G$1" pin="RG6/RP21/PMA5/CN8/SCK2" pad="4"/>
<connect gate="G$1" pin="RP18/RB5/AN5/CN7/C1IN+" pad="11"/>
<connect gate="G$1" pin="RP19/PMA3/CN10/SDO2/RG8" pad="6"/>
<connect gate="G$1" pin="RP26/PMA4/CN9/SDI2/RG7" pad="5"/>
<connect gate="G$1" pin="RP27/PMA2/SS2/CN11/RG9" pad="8"/>
<connect gate="G$1" pin="RP28/RB4/AN4/CN6/C1IN-" pad="12"/>
<connect gate="G$1" pin="SCL1/RG2" pad="37"/>
<connect gate="G$1" pin="SCL3/PMD6/RE6" pad="2"/>
<connect gate="G$1" pin="SDA1/RG3" pad="36"/>
<connect gate="G$1" pin="SDA3/PMD7/RE7" pad="3"/>
<connect gate="G$1" pin="SDO1/U1TX/RF3" pad="33"/>
<connect gate="G$1" pin="SOSCI/CN1/RC13" pad="47"/>
<connect gate="G$1" pin="SOSCO/T1CK/CN0/RC14" pad="48"/>
<connect gate="G$1" pin="VBUS/RF7" pad="34"/>
<connect gate="G$1" pin="VCAP" pad="56"/>
<connect gate="G$1" pin="VDD" pad="10"/>
<connect gate="G$1" pin="VDD@1" pad="26"/>
<connect gate="G$1" pin="VDD@2" pad="38"/>
<connect gate="G$1" pin="VSS" pad="9"/>
<connect gate="G$1" pin="VSS@1" pad="25"/>
<connect gate="G$1" pin="VSS@2" pad="41"/>
<connect gate="G$1" pin="VUSB" pad="35"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOLEX-47346-0001" prefix="USB">
<description>MICRO USB B, BOTTOM MOUNT</description>
<gates>
<gate name="G$1" symbol="MINI-USB"/>
</gates>
<devices>
<device name="" package="MOLEX-47364-0001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND3"/>
<connect gate="G$1" pin="GND4" pad="GND4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB-MICRO-B" prefix="USB" uservalue="yes">
<gates>
<gate name="G$1" symbol="MICRO-USB"/>
</gates>
<devices>
<device name="FCI" package="USC-MICRO-FCI">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="GND1" pad="P$1"/>
<connect gate="G$1" pin="GND2" pad="P$2"/>
<connect gate="G$1" pin="GND3" pad="P$3"/>
<connect gate="G$1" pin="GND4" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ACS714">
<gates>
<gate name="G$1" symbol="ACS714"/>
</gates>
<devices>
<device name="" package="ACS714">
<connects>
<connect gate="G$1" pin="FIL" pad="6"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN@1" pad="1"/>
<connect gate="G$1" pin="IN@2" pad="2"/>
<connect gate="G$1" pin="OUT@1" pad="3"/>
<connect gate="G$1" pin="OUT@2" pad="4"/>
<connect gate="G$1" pin="VAL" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT230X">
<gates>
<gate name="G$1" symbol="FT230X"/>
</gates>
<devices>
<device name="SSOP16" package="SSOP16">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="10"/>
<connect gate="G$1" pin="CBUS0" pad="15"/>
<connect gate="G$1" pin="CBUS1" pad="14"/>
<connect gate="G$1" pin="CBUS2" pad="7"/>
<connect gate="G$1" pin="CBUS3" pad="16"/>
<connect gate="G$1" pin="CTS#" pad="6"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="13"/>
<connect gate="G$1" pin="RESET#" pad="11"/>
<connect gate="G$1" pin="RTS#" pad="2"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="USBDM" pad="9"/>
<connect gate="G$1" pin="USBDP" pad="8"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VCCIO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PICKIT3">
<gates>
<gate name="G$1" symbol="PICKIT3"/>
</gates>
<devices>
<device name="" package="PICKIT3">
<connects>
<connect gate="G$1" pin="LVP(NC)" pad="6"/>
<connect gate="G$1" pin="PGC" pad="5"/>
<connect gate="G$1" pin="PGD" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VPP/!MCLR" pad="1"/>
<connect gate="G$1" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC32MX795" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="PIC32MX795"/>
</gates>
<devices>
<device name="" package="TQFP64-10X10RMS">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="D+/RG2" pad="37"/>
<connect gate="G$1" pin="D-/RG3" pad="36"/>
<connect gate="G$1" pin="OC1/INT0/RD0" pad="46"/>
<connect gate="G$1" pin="PMA8/SCL5/SDO4/CN18/U2TX/RF5" pad="32"/>
<connect gate="G$1" pin="PMA9/SDA2/CN17/U2RX/RF4" pad="31"/>
<connect gate="G$1" pin="PMD0/RE0" pad="60"/>
<connect gate="G$1" pin="PMD1/RE1" pad="61"/>
<connect gate="G$1" pin="PMD2/RE2" pad="62"/>
<connect gate="G$1" pin="PMD3/RE3" pad="63"/>
<connect gate="G$1" pin="PMD4/RE4" pad="64"/>
<connect gate="G$1" pin="PMD5/RE5" pad="1"/>
<connect gate="G$1" pin="RB0/AN0/CN2/VR+/PGD1/PMA6" pad="16"/>
<connect gate="G$1" pin="RB1/AN1/CN3/VR-/PGC1/EMUC1" pad="15"/>
<connect gate="G$1" pin="RB10/AN10/TMS/CVREF/PMA13" pad="23"/>
<connect gate="G$1" pin="RB11/AN11/TDO/PMA12" pad="24"/>
<connect gate="G$1" pin="RB12/AN12/TCK/PMA11" pad="27"/>
<connect gate="G$1" pin="RB13/AN13/TDI/PMA10" pad="28"/>
<connect gate="G$1" pin="RB14/AN14/U2RTS/SCK4/PMA1" pad="29"/>
<connect gate="G$1" pin="RB15/AN15/CN12/OCFB/PMA0" pad="30"/>
<connect gate="G$1" pin="RB2/AN2/CN4/SS1/C2IN-" pad="14"/>
<connect gate="G$1" pin="RB3/AN3/CN5/C2IN+" pad="13"/>
<connect gate="G$1" pin="RB4/AN4/CN6/C1IN-" pad="12"/>
<connect gate="G$1" pin="RB5/AN5/CN7/C1IN+" pad="11"/>
<connect gate="G$1" pin="RB6/AN6/OCFA/PGC2" pad="17"/>
<connect gate="G$1" pin="RB7/AN7/PGD2" pad="18"/>
<connect gate="G$1" pin="RB8/U5RX/AN8/U2CTS/C1OUT" pad="21"/>
<connect gate="G$1" pin="RB9/AN9/C2OUT/PMA7" pad="22"/>
<connect gate="G$1" pin="RC12/CLKI/OSC1" pad="39"/>
<connect gate="G$1" pin="RC15/CLKO/OSC2" pad="40"/>
<connect gate="G$1" pin="RD1/OC2/U4TX/SCL3" pad="49"/>
<connect gate="G$1" pin="RD10/SCL1/IC3/INT3/PMCS2" pad="44"/>
<connect gate="G$1" pin="RD11/IC4/INT4/PMCS1" pad="45"/>
<connect gate="G$1" pin="RD2/OC3/SDA3/SDI3/U1RX" pad="50"/>
<connect gate="G$1" pin="RD3/OC4/PMBE/SDO3/SCL3/U1TX" pad="51"/>
<connect gate="G$1" pin="RD4/OC5/IC5/CN13/PMWR/RP25" pad="52"/>
<connect gate="G$1" pin="RD5/CN14/PMRD/RP20" pad="53"/>
<connect gate="G$1" pin="RD6/CN15" pad="54"/>
<connect gate="G$1" pin="RD7/CN16" pad="55"/>
<connect gate="G$1" pin="RD8/IC1/INT1/RTCC" pad="42"/>
<connect gate="G$1" pin="RD9/SDA1/IC2/INT2/U4RX" pad="43"/>
<connect gate="G$1" pin="RF0" pad="58"/>
<connect gate="G$1" pin="RF1" pad="59"/>
<connect gate="G$1" pin="RG6/U6TX/PMA5/CN8/SCK2" pad="4"/>
<connect gate="G$1" pin="SCL3/PMD6/RE6" pad="2"/>
<connect gate="G$1" pin="SCL4/U3TX/PMA3/CN10/SDO2/RG8" pad="6"/>
<connect gate="G$1" pin="SDA3/PMD7/RE7" pad="3"/>
<connect gate="G$1" pin="SDA4/U3RX/PMA4/CN9/SDI2/RG7" pad="5"/>
<connect gate="G$1" pin="SOSCI/CN1/RC13" pad="47"/>
<connect gate="G$1" pin="SOSCO/T1CK/CN0/RC14" pad="48"/>
<connect gate="G$1" pin="U6RX/PMA2/SS2/CN11/RG9" pad="8"/>
<connect gate="G$1" pin="USBID/RF3" pad="33"/>
<connect gate="G$1" pin="VBUS" pad="34"/>
<connect gate="G$1" pin="VCAP" pad="56"/>
<connect gate="G$1" pin="VDD" pad="10"/>
<connect gate="G$1" pin="VDD@1" pad="26"/>
<connect gate="G$1" pin="VDD@2" pad="38"/>
<connect gate="G$1" pin="VDD@V" pad="57"/>
<connect gate="G$1" pin="VSS" pad="9"/>
<connect gate="G$1" pin="VSS@1" pad="25"/>
<connect gate="G$1" pin="VSS@2" pad="41"/>
<connect gate="G$1" pin="VUSB" pad="35"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
