SD Transceiver Board 2 is the version that was implemented. 6 blank boards were ordered.
SD Transceiver Board 2.1,2,2,2,3 have modified versions of the matching network for the power amplifier. 3 blank boards of version 2.3 were ordered.